RCRA REVISION CHECKLIST 213

Burden Reduction Initiative
71 FR 16862-16915
	April 4, 2006
	(RCRA Cluster XVI, HSWA/Non-HSWA)

Name of State:  

State Statutory Authority: 

Title of Regulations:  							Effective Date:   

Date Checklist Completed:  

	
FEDERAL REQUIREMENTS	
FEDERAL RCRA CITATION	
ANALOGOUS STATE CITATION	
STATE ANALOG IS:	
				
EQUIV-ALENT	
LESS
STRIN-
GENT	
MORE STRIN-GENT	
BROADER IN SCOPE	
	PART 260 HAZARDOUS WASTE MANAGEMENT SYSTEM:  GENERAL	
	SUBPART B DEFINITIONS	
	DEFINITIONS	
†	add “Performance Track member facility”	260.10 “Performance Track member facility”						
	SUBPART C RULEMAKING PETITIONS	
†	STANDARDS AND CRITERIA FOR VARIANCES FROM CLASSIFICATION AS A SOLID WASTE	
	remove paragraph (b)(2)	260.31(b)(2)						
	redesignate paragraphs (b)(3) through (b)(8) as (b)(2) through (b)(7)	260.31(b)(2) - (b)(7)						
	PART 261 IDENTIFICATION AND LISTING OF HAZARDOUS WASTE	
	SUBPART A GENERAL	
†	EXCLUSIONS	
	replace “submits to the Regional Administrator or State Director” with “prepares” in the first sentence;  replace “for a period of no less than 3 years from the date specified in the notice” with “until closure of the facility” in the second sentence	261.4(a)(9)(iii)(E)						
	insert a comma after “March 15 of each year”;  remove “estimates the number of studies … during the current year, and”	261.4(f)(9)						
	PART 264 STANDARDS FOR OWNERS AND OPERATORS OF HAZARDOUS WASTE TREATMENT, STORAGE, AND DISPOSAL FACILITIES	
	SUBPART B GENERAL FACILITY STANDARDS	
†	GENERAL INSPECTION REQUIREMENTS	
	remove “any” before “operator error” in the second sentence;  add “, except for Performance Track member facilities … as described in paragraph (b)(5) of this section” to the end of the third sentence	264.15(b)(4)						
	add new paragraph (b)(5):  Performance Track member facilities that choose to reduce their inspection frequency must: 	264.15(b)(5) introductory paragraph						
	submit a Class I permit modification request 	264.15(b)(5)(i)						
	director will notify of decision within 60 days; notice and copy of application in operating record 	264.15(b)(5)(ii)						
	discontinuation of Performance Track membership must immediately notify Director of change in status; dated notice in operating record	264.15(b)(5)(iii)						
	PERSONNEL TRAINING	
†	add new subparagraph (a)(4):  For facility employees receiving emergency response training pursuant to OSHA regulations facility not required to provide separate emergency response training	264.16(a)(4)						
	SUBPART D CONTINGENCY PLAN AND EMERGENCY PROCEDURES	
	CONTENT OF CONTINGENCY PLAN	
†	add the following to the end of the paragraph:
“The owner or operator may develop one contingency plan which meets all regulatory requirements.  EPA recommends that the plan be based on the National Response Team’s Integrated Contingency Plan Guidance (“One Plan”).  When modifications are made to non-RCRA provisions in an integrated contingency plan, the changes do not trigger the need for a RCRA permit modification.”	264.52(b)						
†	EMERGENCY PROCEDURES	
	remove old paragraph (i) and redesignate old paragraph (j) as (i)	264.56(i)						
	SUBPART E MANIFEST SYSTEM, RECORDKEEPING, AND REPORTING	
†	OPERATING RECORD	
	replace “until closure of the facility” with “for three years unless noted as follows”	264.73(b)						
	add “of this part.  This information … until closure of the facility” after “appendix I”	264.73(b)(1)						
	replace “of” with “that shows” after “diagram” in the second sentence;  remove “specific” after “cross-references to” in the second sentence; remove the comma after “document numbers” and replace the semicolon after “a manifest” with a period; add to end of paragraph:  
“This information … until closure of the facility.”	264.73(b)(2)						
	remove “264.347” from the list of citations; add to end of paragraph:  “Maintain in the operating record …  until closure of the facility.”  	264.73(b)(6)						
	replace “§ 264.144.” with
“§ 264.144 of this part.  This information must be maintained… until closure of the facility;”	264.73(b)(8)						
	remove parentheses around phrase “and date of placement”;  insert “of this chapter” after each of the following citations: “§ 268.5”, “§ 268.6”, “§ 268.8”, and “§ 268.7”; add to end of paragraph:  “This information must be maintained … until closure of the facility;”	264.73(b)(10)						
	add new paragraph (b)(18):  monitoring, testing or analytical data where required by § 264.347 must be maintained in the operating record for five years.	264.73(b)(18)						
	add new paragraph (b)(19):  certifications as required by § 264.196(f) must be maintained in the operating record until closure of the facility.  	264.73(b)(19)						
	SUBPART F RELEASES FROM SOLID WASTE MANAGEMENT UNITS	
	DETECTION MONITORING PROGRAM	
†	remove the second sentence beginning with “A sequence of at least four samples . . .”	264.98(d)						
†	replace “part 264” with “this part” in the first sentence;  add to end of paragraph:  “However, the Regional Administrator, … waste constituents.”	264.98(g)(2)						
†	insert “or at an alternative site-specific schedule approved by the Administrator” after “within one month” in the first sentence; replace “found pursuant to” with “in” before  the second occurrence of “paragraph (g)(2)”	264.98(g)(3)						
†	COMPLIANCE MONITORING PROGRAM	
	remove the second sentence beginning with “A sequence of at least four samples . . .”	264.99(f)						
	completely revise; Annually determine whether additional hazardous constituents from Appendix IX are present in the uppermost aquifer; consult with the Regional Administrator to determine enhanced sampling event; report concentration of additional constituents within seven days and add them to the monitoring list 	264.99(g)						
	CORRECTIVE ACTION PROGRAM	
†	replace “semi-annually” with “annually” in the second sentence	264.100(g)						
	SUBPART G CLOSURE AND POST-CLOSURE	
	CLOSURE; TIME ALLOWED FOR CLOSURE	
†	replace “semi-annually” with “annually” and “that describe” with “describing”	264.113(e)(5)						
	CERTIFICATION OF CLOSURE	
†	replace “an independent registered professional engineer” with “a qualified Professional Engineer” in the second sentence; and “independent registered professional engineer’s” with “Professional Engineer’s” in the third sentence  	264.115						
	CERTIFICATION OF COMPLETION OF POST-CLOSURE CARE	
†	replace “an independent registered professional engineer” with “a qualified Professional Engineer” in the second sentence; and “independent registered professional engineer’s” with “Professional Engineer’s” in the third sentence  	264.120						
	SUBPART H FINANCIAL REQUIREMENTS	
	FINANCIAL ASSURANCE FOR CLOSURE	
†	replace “an independent registered professional engineer” with “a qualified Professional Engineer” in the first sentence  	264.143(i)						
	FINANCIAL ASSURANCE FOR POST-CLOSURE CARE	
†	replace “an independent registered professional engineer” with “a qualified Professional Engineer” in the first sentence  	264.145(i)						
	LIABILITY REQUIREMENTS	
†	replace “an independent registered professional engineer” with “a qualified Professional Engineer” in the first sentence	264.147(e)						
	SUBPART I USE AND MANAGEMENT OF CONTAINERS	
	INSPECTIONS	
†	insert “except for Performance Track member facilities, …of this part” after “where containers are stored,”; replace “looking for” with “The owner or operator must look for” 	264.174						
	SUBPART J TANKS SYSTEMS	
†	ASSESSMENT OF EXISTING TANK STSTEM’S INTEGRITY	
	replace “an independent registered professional engineer” with “a qualified Professional Engineer” 	264.191(a)						
	replace “an independent registered professional engineer” with “a qualified Professional Engineer”  	264.191(b)(5)(ii)						
†	DESIGN AND INSTALLATION OF NEW TANK SYSTEMS OR COMPONENTS	
	replace “an independent registered professional engineer” with “a qualified Professional Engineer” in the first sentence	264.192(a) introductory paragraph						
	replace “an independent registered professional engineer” with “a qualified Professional Engineer” in the second sentence.  	264.192(b) introductory paragraph						
†	CONTAINMENT AND DETECTION OF RELEASES	
	insert “and existing” after “For all new”	264.193(a)(1)						
	remove paragraphs (a)(2) through (a)(4); redesignate paragraph (a)(5) as (a)(2) and completely revise; 
For tank systems that store or treat materials that become hazardous wastes, within two years of the hazardous waste listing, or when the tank system has reached 15 years of age, whichever comes later 	264.193(a)(2)						
	replace “an independent registered professional engineer” with “a qualified Professional Engineer” in the first sentence  	264.193(i)(2)						
†	INSPECTIONS	
	remove subparagraphs (b)(1) through (b)(3); completely revise; 
inspect data gathered from monitoring and leak detection equipment	264.195(b)						
	redesignate existing paragraphs (c) and (d) as (g) and (h) without revision; add new paragraphs (c) through (f); 
Owner or operator must inspect at least once each operating day: 	264.195(c) introductory paragraph						
	above ground portions of tank system; construction materials and externally accessible portion of the tank system	264.195(c)(1)						
	construction materials and the area surrounding externally accessible portion of the tank system	264.195(c)(2)						
	at least weekly inspections when using leak detection systems or established workplace practices; alternate inspection schedule documentation	264.195(d)						
	performance Track member facilities may inspect less frequently upon approval of Director; application procedures	264.195(e)						
	ancillary equipment inspected at least once each operating day	264.195(f)						
	redesignate existing paragraphs (c) and (d) as (g) and (h) without revision	264.195(g) and (h)						
	RESPONSE TO LEAKS OR SPILLS AND DISPOSITION OF LEAKING OR UNFIT-FOR-USE TANK SYSTEMS	
†	replace “an independent, qualified, registered, professional engineer” with “a qualified Professional Engineer” in the first sentence;  replace the second sentence with “This certification must be … until closure of the facility.”	264.196(f)						
	SUBPART L WASTE PILES	
	DESIGN AND OPERATING REQUIREMENTS	
†	remove the following three phrases: “on which construction … January 29, 1992”, “on which construction …July 29, 1992” and “that is to commence … July 29, 1992”; remove definition of “Construction commences”	264.251(c) introductory paragraph						
	SUBPART M LAND TREATMENT	
	CLOSURE AND POST-CLOSURE CARE	
†	replace “an independent registered professional engineer” with “a qualified Professional Engineer”.  	264.280(b)						
	SUBPART N LANDFILLS	
†	SPECIAL REQUIREMENTS FOR BULK AND CONTAINERIZED LIQUIDS	
	remove paragraph (a); redesignate paragraph (b) as (a);  remove “Effective May 8, 1985,” and capitalize “The” at the beginning of the paragraph	264.314(a)						
	redesignate paragraphs (c) through (e) as (b) through (d).	264.314(b) - (d)						
	redesignate 264.314(f) as 264.314(e); in the introductory paragraph replace “Effective November 8, 1985, the” with “The”; remove the comma after “determines” 	264.314(e) introductory paragraph						
	old 264.314(f)(1) and (f)(2) redesignated as (e)(1) and (e)(2)	264.314(e)(1) and (e)(2)						
	SUBPART O INCINERATORS	
	PERFORMANCE STANDARDS	
†	remove italics from “-p-dioxins” in the second sentence and remove last sentence	264.343(a)(2)						
	MONITORING AND INSPECTIONS	
†	replace “log” with “record”;  add “of this part and maintained in the operating record for five years.” after “§ 264.73”	264.347(d)						
	SUBPART S SPECIAL PROVISIONS FOR CLEANUP	
	STAGING PILES	
†	replace “an independent, qualified, registered professional engineer” with “a qualified Professional Engineer”	264.554(c)(2)						
	SUBPART W DRIP PADS	
†	ASSESSMENT OF EXISTING DRIP PAD INTEGRITY	
	replace “an independent, qualified registered professional engineer” with “a qualified Professional Engineer”; remove “of this subpart” after both instances of “§ 264.573” and after “§ 264.573(b)” in the last sentence    	264.571(a)						
	remove “of this subpart” after “§ 264.573(b)” and “§ 264.573”;  replace “an independent qualified registered professional engineer” with “a qualified Professional Engineer”   	264.571(b)						
	replace “an independent qualified registered professional engineer” with “a qualified Professional Engineer” 	264.571(c)						
†	DESIGN AND OPERATING REQUIREMENTS	
	replace “an independent, qualified registered professional engineer” with “a qualified Professional Engineer”  	264.573(a)(4)(ii)						
	replace “an independent, qualified registered professional engineer” with “a qualified Professional Engineer”  	264.573(g)						
	INSPECTIONS	
	replace “an independent qualified registered professional engineer” with “a qualified Professional Engineer”  	264.574(a)						
	SUBPART BB AIR EMISSIONS STANDARDS FOR EQUIPMENT LEAKS	
†	ALTERNATIVE STANDARDS FOR VALVES IN GAS/VAPOR SERVICE OR IN LIGHT LIQUID SERVICE:  PERCENTAGE OF VALVES ALLOWED TO LEAK	
	remove paragraph (b)(1); redesignate paragraphs (b)(2) and (b)(3) as (b)(1) and (b)(2) without revision	264.1061(b)(1) and (b)(2)						
	remove paragraph (d).	264.1061(d)						
	ALTERNATIVE STANDARDS FOR VALVES IN GAS/VAPOR SERVICE OR IN LIGHT LIQUID SERVICE:  SKIP PERIOD LEAK DETECTION AND REPAIR	
†	redesignate paragraph (a)(1) as (a) without revision; remove paragraph (a)(2)	264.1062(a) 						
	SUBPART DD CONTAINMENT BUILDINGS	
	APPLICABILITY	
†	remove the second sentence.	264.1100 introductory paragraph						
†	DESIGN AND OPERATING STANDARDS	
	completely revise; certification by qualified PE that containment building design meets requirements of paragraphs (a), (b), and (c) 	264.1101(c)(2)						
†	insert “except for Performance Track member facilities that must inspect at least once each month, upon approval by the Director,” after “every seven days”;  add “To apply for reduced inspection frequency… follow the procedures described in § 264.15(b)(5).” to end of paragraph 	264.1101(c)(4)						
	PART 265 INTERIM STATUS STANDARDS FOR OWNERS AND OPERATORS OF HAZARDOUS WASTE TREATMENT, STORAGE, AND DISPOSAL FACILITIES	
	SUBPART B GENERAL FACILITY STANDARDS 	
†	GENERAL INSPECTION REQUIRMENTS	
	remove “any” before “operator error” in second sentence; add “, except for Performance Track member facilities … as described in paragraph (b)(5) of this section” to end of third sentence; remove “of this part” after “265.1090” in last sentence	265.15(b)(4)						
	add new paragraph (b)(5):  Performance Track member facilities choosing to reduce their inspection frequency must: 	265.15(b)(5) introductory paragraph						
	submit application; identify units and proposed inspection frequency; at least monthly inspections 	265.15(b)(5)(i)						
	director will notify of decision within 60 days; notice and copy of application in operating record	265.15(b)(5)(ii)						
	discontinuation of Performance Track membership must immediately notify Director of change in status; dated notice in operating record 	265.15(b)(5)(iii)						
	PERSONNEL TRAINING	
†	add new paragraph (a)(4):  For facility employees receiving emergency response training pursuant to OSHA regulations facility not required to provide separate emergency response training.	265.16(a)(4)						
	SUBPART D CONTINGENCY PLAN AND EMERGENCY PROCEDURES	
	CONTENT OF CONTINGENCY PLAN	
†	add to end of paragraph:
“The owner or operator may develop one contingency plan … for a RCRA permit modification.”	265.52(b)						
	EMERGENCY PROCEDURES	
†	Remove old  paragraph (i); redesignate old paragraph (j) as (i) 	265.56(i)						
	SUBPART E MANIFEST SYSTEM, RECORDKEEPING, AND REPORTING	
†	OPERATING RECORD	
	replace “until closure of the facility” with “for three years unless noted below”.	265.73(b) introductory paragraph						
	replace “appendix I;” with “Appendix I to part 265.”; add to end of paragraph:  “This information must be … closure of the facility;”	265.73(b)(1)						
	remove “specific” after “cross-references to”;  remove the comma after “document numbers” and replace semicolon after “a manifest” with a period; add to end of paragraph:  “This information must be… until closure of the facility;”	265.73(b)(2)						
	in first sentence remove the references 265.90, 265.222, 265.223, and 265.259, insert a comma after “265.302”, remove “through” prior to “265.304”, add reference to 265.224 in numerical order;  and remove “of this part” after “265.1090”;  add to end of paragraph: “Maintain in the operating record for three years … until closure of the facility.”  	265.73(b)(6)						
	add to end of paragraph:  
“must be maintained …until closure of the facility;”	265.73(b)(7)						
	insert “of this chapter” after “§ 268.5”, “§ 268.6”, “§ 268.8”, and “§ 268.7(a)”; add to end of paragraph: “All of this information … until closure of the facility.”	265.73(b)(8)						
	add new paragraph (b)(15):  maintain in operating record until closure; monitoring, testing or analytical data, and corrective action where required by §§ 265.90, 265.93(d)(2), and 265.93(d)(5), and §265.196(f) certification 	265.73(b)(15)						
	SUBPART F GROUND-WATER MONITORING	
†	APPLICABILITY	
	replace “submit to the Regional Administrator” with “develop”; add “This plan …until closure of the facility.” to end of paragraph.	265.90(d)(1)						
	replace “and submit a written report” with “ a report”; add “and place…until closure of the facility.” to end of paragraph	265.90(d)(3)						
†	PREPARATION, EVALUATION, AND RESPONSE	
	remove “and submit” and “program”;  add to end of paragraph: “This plan must …until closure of the facility.”	265.93(d)(2)						
	replace “, within 15 days after that determination, submit to the Regional Administrator a written” with “prepare a”; add to end of paragraph: “This report must… until closure of the facility.”	265.93(d)(5)						
	SUBPART G CLOSURE AND POST-CLOSURE CARE	
	CLOSURE; TIME ALLOWED FOR CLOSURE	
†	replace “semi-annual” with annual”; replace “that describe” with “describing”	265.113(e)(5)						
	CERTIFICATION OF CLOSURE	
†	replace “an independent registered professional engineer” with “a qualified Professional Engineer” in second sentence; replace “independent registered professional engineer’s” with “a qualified Professional Engineer’s” in third sentence 	265.115						
	CERTIFICATION OF COMPLETION OF POST-CLOSURE CARE	
†	replace “an independent registered professional engineer” with “a qualified Professional Engineer” in second sentence; replace “independent registered professional engineer’s” with “a qualified Professional Engineer’s” in third sentence.  	265.120						
	SUBPART H FINANCIAL REQUIREMENTS	
	FINANCIAL ASSURANCE FOR CLOSURE	
†	replace “an independent registered professional engineer” with “a qualified Professional Engineer” 	265.143(h)						
	FINANCIAL ASSURANCE FOR POST-CLOSURE CARE	
†	replace “an independent registered professional engineer” with “a qualified Professional Engineer” 	265.145(h)						
	LIABILITY REQUIREMENTS	
†	replace “an independent registered professional engineer” with “a qualified Professional Engineer”  	265.147(e)						
	SUBPART I USE AND MANAGEMENT OF CONTAINERS	
	INSPECTIONS	
†	completely revise; 
weekly inspections of container storage areas; Performance Track facilities inspect once a month; application for reduced inspection frequency; Comment regarding remedial action	265.174						
	SUBPART J TANK SYSTEMS	
†	ASSESSMENT OF EXISTING TANK SYSTEM’S INTEGRITY	
	replace “an independent, qualified, registered, professional engineer” with “a qualified Professional Engineer” in the second sentence 	265.191(a)						
	replace “an independent, qualified, registered, professional engineer” with “a qualified Professional Engineer”	265.191(b)(5)(ii)						
†	DESIGN AND INSTALLATION OF NEW TANK SYSTEMS OR COMPONENTS	
	replace “an independent, qualified, registered, professional engineer” with “a qualified Professional Engineer” in the second sentence 	265.192(a) introductory paragraph						
	replace “an independent, qualified, registered, professional engineer” with “a qualified Professional Engineer” in the second sentence.  	265.192(b) introductory paragraph						
†	CONTAINMENT AND DETECTION OF RELEASES	
	insert “and existing” after “all new” 	265.193(a)(1)						
	remove paragraphs (a)(2) through (a)(4); redesignate paragraph (a)(5) as (a)(2) and completely revise; 
For tank systems that store or treat materials that become hazardous wastes, within two years of the hazardous waste listing, or when the tank system has reached 15 years of age, whichever comes later 	265.193(a)(2) 						
	replace “an independent, qualified, registered, professional engineer” with “a qualified Professional Engineer” in the second sentence.  	265.193(i)(2)						
†	INSPECTIONS	
	remove subparagraphs (a)(1) through (a)(5); completely revise; 
inspect data gathered from monitoring and leak detection equipment	265.195(a)						
	redesignate existing paragraphs (b) and (c) as (f) and (g) without revision; add new paragraphs (b) through (e);  owner or operator must inspect at least once each operating day:	265.195(b) introductory paragraph						
	overfill/spill control equipment; 	265.195(b)(1)						
	above ground portions of tank system; 	265.195(b)(2)						
	construction materials and the area surrounding externally accessible portion of the tank system	265.195(b)(3)						
	at least weekly inspections when using leak detection systems or established workplace practices; alternate inspection schedule documentation	265.195(c)						
	Performance Track member facilities may inspect less frequently upon approval of Director; application procedures.	265.195(d)						
	Ancillary equipment inspected at least once each operating day	265.195(e)						
	redesignate paragraphs (b) and (c) as (f) and (g) without revision	265.195(f) and (g)						
	RESPONSE TO LEAKS OR SPILLS AND THE DISPOSITION OF LEAKING OR UNFIT-FOR-USE TANK SYSTEMS	
†	replace “an independent, qualified, registered, professional engineer” with “a qualified Professional Engineer”;  replace the last sentence with: “This certification is …until closure of the facility.”	265.196(f)						
†	SPECIAL REQUIREMENTS FOR GENERATORS OF BETWEEN 100 ANS 1,000 KG/MO THAT ACCUMULATE HAZARDOUS WASTE IN TANKS	
	replace “Generators” with “Except as noted in paragraph (d) of this section, generators” 	265.201(c) introductory paragraph						
	redesignate paragraphs (d) - (f) as (f) - (h) without revision; add new paragraphs (d) and (e):  weekly inspections by generators accumulating 100 to 1,000 kg/mo in tanks or tank systems with secondary containment; documentation of alternate inspection schedule	265.201(d)						
	Performance Track facilities inspect less frequently upon approval of Director; application procedures	265.201(e)						
	redesignate paragraphs (d) - (f) as (f) - (h) without revision	265.201(f) - (h)						
	SUBPART K SURFACE IMPOUNDMENTS	
	DESIGN AND OPERATING REQUIREMENTS	
†	remove the following three phrases: “on which construction … January 29, 1992”, “on which construction …July 29, 1992” and “that is to commence … July 29, 1992”; remove definition of “Construction commences”	265.221(a)						
†	RESPONSE ACTIONS	
	redesignate old section 265.223 titled “Response Actions” as 265.224.	265.224						
6	in the first sentence, replace the text after “§265.221(a) must” with “develop and keep on-site until closure of the facility a response action plan”	265.224(a)						
	SUBPART L WASTE PILES	
	RESPONSE ACTIONS							
†	in the first sentence, replace the text after “§265.254 must” with “develop and keep on-site until closure of the facility a response action plan”	265.259(a)						
	SUBPART M LAND TREATMENT	
	CLOSURE AND POST-CLOSURE	
†	replace “an independent registered professional engineer” with “a qualified Professional Engineer” 	265.280(e)						
	SUBPART N LANDFILLS	
	DESIGN AND OPERATING REQUIREMENTS	
†	remove the following three phrases: “on which construction … January 29, 1992”, “on which construction …July 29, 1992” and “that is to commence … July 29, 1992”; remove definition of “Construction commences”	265.301(a)						
	RESPONSE ACTIONS	
†	in the first sentence, replace the text after “§265.301(a) must” with “develop and keep on-site until closure of the facility a response action plan”	265.303(a)						
†	SPECIAL REQUIREMENTS FOR BULK AND CONTAINERIZED LIQUIDS	
	remove paragraph (a); redesignate paragraph (b) as (a);  remove “Effective May 8, 1985,” and capitalize “The” at the beginning of the paragraph	265.314(a)						
	redesignate paragraphs (c) through (g) as (b) through (f).	265.314(b) through (f)						
	redesignate 265.314(g) as 265.314(f); in the introductory paragraph replace “Effective November 8, 1985, the” with “The”; remove the comma after “determines” 	265.314(f) introductory paragraph						
	Old 265.314(g)(1) and (g)(2) redesignated as (f)(1) and (f)(2)	265.314(f)(1) and (f)(2)						
	SUBPART W DRIP PADS	
†	ASSESSMENT OF EXISTING DRIP PAD INTEGRITY	
	replace “an independent, qualified registered professional engineer” with “a qualified Professional Engineer”; remove “of this subpart” after each instance of “§ 265.440” and “§ 265.443”, and after § 265.443(b) in last sentence   	265.441(a)						
	remove “of this subpart” after each instance of “§ 265.443(b)” and “§ 265.443”; replace “an independent qualified registered professional engineer” with “a qualified Professional Engineer”   	265.441(b)						
	replace “an independent, qualified registered professional engineer” with “a qualified Professional Engineer”  	265.441(c)						
†	DESIGN AND OPERATING REQUIREMENTS	
	replace “an independent, qualified registered professional engineer” with “a qualified Professional Engineer”; replace “subsection (b)” with “paragraph (b) of this section” 	265.443(a)(4)(ii)						
	replace “an independent, qualified registered professional engineer” with “a qualified Professional Engineer” 	265.443(g)						
	INSPECTIONS	
†	remove “of this subpart” after “§ 265.443”; replace “an independent qualified, registered professional engineer” with “a qualified Professional Engineer”	265.444(a)						
	SUBPART BB AIR EMISSION STANDARDS FOR EQUIPMENT LEAKS	
†	ALTERNATIVE STANDARDS FOR VALVES IN GAS/VAPOR SERVICE OR IN LIGHT LIQUID SERVICE:  PERCENTAGE OF VALVES ALLOWED TO LEAK	
	remove paragraph (b)(1); redesignate paragraphs (b)(2) and (b)(3) as (b)(1) and (b)(2) without revision	265.1061(b)(1) and (2)						
	remove paragraph (d).	265.1061(d)						
	ALTERNATIVE STANDARDS FOR VALVES IN GAS/VAPOR SERVICE OR IN LIGHT LIQUID SERVICE:  SKIP PERIOD LEAK DETECTION AND REPAIR 	
†	redesignate paragraph (a)(1) as (a) without revision and remove paragraph (a)(2)	265.1062(a)						
	SUBPART DD CONTAINMENT BUILDINGS	
	APPLICABILITY	
†	remove the second sentence 	265.1100 introductory paragraph						
†	DESIGN AND OPERATING STANDARDS	
	completely revise; certification by qualified PE that containment building design meets requirements of paragraphs (a), (b), and (c) 	265.1101(c)(2)						
	insert “except for Performance Track member facilities that must inspect at least once each month, upon approval by the Director,” after “every seven days”;  add “To apply for reduced inspection frequency… follow the procedures described in § 264.15(b)(5).” to end of paragraph 	265.1101(c)(4)						
	PART 266 STANDARDS FOR THE MANAGEMENT OF SPECIFIC HAZARDOUS WASTES AND SPECIFIC TYPES OF HAZARDOUS WASTE MANAGEMENT FACILITIES	
	SUBPART H HAZARDOUS WASTE BURNED IN BOILERS AND INDUSTRIAL FURNACES	
	PERMIT STANDARDS FOR BURNERS	
†	replace “until closure of the facility” with “for five years”	266.102(e)(10)						
†	INTERIM STATUS STANDARDS FOR BURNERS	
	replace “three years” with “five years”	266.103(d)						
	replace “until closure of the boiler or industrial furnace unit” with “for five years”	266.103(k)						
	PART 268 LAND DISPOSAL RESTRICTIONS	
	SUBPART A GENERAL	
†	TESTING, TRACKING, AND RECORDKEEPING REQUIREMENTS FOR GENERATORS, TREATERS, AND DISPOSAL FACILITIES	
	insert “concurrently with the hazardous waste determination required in § 262.11 of this chapter” after “can be made” in second sentence; replace “as referenced in § 260.11 of this chapter” with “(incorporated by reference, see § 260.11 of this chapter)” in third sentence; insert after third sentence: “(Alternatively, the generator must send the waste to a RCRA-permitted hazardous waste treatment facility…and paragraph (b) of this section.)”	268.7(a)(1)						
	insert “or if the generator chooses not to make the determination of whether his waste must be treated,” after “treatment standards” in the first sentence; insert “of this section” after “paragraph (a)(4)” in second sentence; insert after second sentence: “(Alternatively, if the generator chooses not to make the determination … treatment facility must make the determination.)”	268.7(a)(2)						
	completely revise: one time 268.7(b)(3) notice and (b)(4) certification for initial shipment of recyclable material used in a manner constituting disposal subject to 266.20(b); records of recipients of waste-derived products	268.7(b)(6)						
	SPECIAL RULES REGARDING WASTES THAT EXHIBIT A CHARACTERISTIC	
†	insert as the second sentence “This determination … required in § 262.11 of this chapter.”  insert “40 CFR” before “Part 261” in the parentheticals in the second and third sentences	268.9(a)						
†	replace “generators and treaters” with “generator’s and treater’s” in first sentence; remove “that is placed in the generators and treaters files” from second sentence;  remove third and fourth sentences  	268.9(d)						
	PART 270 EPA-ADMINISTERED PERMIT PROGRAMS:  THE HAZARDOUS WASTE PERMIT PROGRAM	
	SUBPART B PERMIT APPLICATION	
	CONTENTS OF PART B:  GENERAL REQUIREMENTS	
†	replace “a registered professional engineer” with “a qualified Professional Engineer”	270.14(a)						
	SPECIFIC PART B INFORMATION REQUIREMENTS FOR TANK SYSTEMS	
†	replace “an independent, qualified, registered professional engineer” with “a qualified Professional Engineer”	270.16(a)						
	SPECIAL PART B INFORMATION REQUIREMENTS FOR DRIP PADS	
†	replace “an independent qualified, registered professional engineer” with “a qualified Professional Engineer”	270.26(c)(15)						
	SUBPART D CHANGES TO PERMITS	
	PERMIT MODIFICATION AT THE REQUEST OF THE PERMITTEE	
†	add new paragraph (l):  Performance Track facilities; procedures; compliance with requirements under § 264.15(b)(5); application approved if Director does not deny or issue an extension to the deadline in writing within 60 days; adherence to revised inspection schedule.	270.42(l)						
†	add new entry O to the table in Appendix I to § 270.42; see provision as shown at 71 FR 16914.	270.42, Appendix I, Item O