RCRA REVISION CHECKLIST 20

Listing of Spent Solvents
50 FR 53315-53320
December 31, 1985
as amended on January 21, 1986, at 51 FR 2702
(HSWA Cluster I)
	STATE ANALOG IS:
		     ANALOGOUS	  EQUIV-	   MORE	BROADER
   FEDERAL REQUIREMENT     | 	FEDERAL RCRA CITATION    |	   STATE CITATION	| ALENT  |	STRINGENT |	IN SCOPE	

PART 261 - IDENTIFICATION AND LISTING OF HAZARDOUS WASTE

SUBPART D - LISTS OF HAZARDOUS WASTES

HAZARDOUS WASTE FROM NON-SPECIFIC SOURCES	 

    1	list of "F" wastes	261.31	

§261.31 - Hazardous waste from nonspecific sources	 
  Industry &
EPA Hazardous							Hazard
  Waste No.			Hazardous Waste				 Code	 

Generic:

F001..................	The following spent halogenated solvents used in degreasing:		  (T)
	Tetrachloroethylene, trichloroethylene, methylene chloride,
	1,1,1-trichloroethane, carbon tetrachloride, and chlorinated 
	fluorocarbons; all spent solvent mixtures/blends used in degreasing
	containing, before use, a total of ten percent or more (by volume)
	of one or more of the above halogenated solvents or those solvents
	listed in F002, F004, and F005; and still bottoms from the recovery
	of these spent solvents and spent solvent mixtures.
F002..................	The following spent halogenated solvents:  Tetrachloroethylene,		  (T)
	methylene chloride, trichloroethylene, 1,1,1-trichloroethane,
	chlorobenzene, 1,1,2-trichloro-1,2,2-trifluoroethane, ortho-dichlorobenzene, 
	and trichlorofluoromethane; all spent solvent mixtures/blends containing, 
	before use, a total of ten percent or more (by volume) of one or more 
	of the above halogenated solvents or those solvents listed in F001, 
	F004, and F005; and still bottoms from the recovery of these spent 
	solvents and spent solvent mixtures.
F003..................	The following spent non-halogenated solvents:  Xylene, acetone,	  (I)*
	ethyl acetate, ethyl benzene, ethyl ether, methyl isobutyl ketone,
	n-butyl alcohol, cyclohexanone, and methanol; all spent solvent
	mixtures/blends containing, before use, only the above spent 
	non-halogenated solvents; and all spent solvent mixtures/blends 
	containing, before use, one or more of the above non-halogenated 
F003 cont’d......	solvents, and a total of ten percent or more (by volume) of one or
	more of those solvents listed in F001, F002, F004, and F005; and
	still bottoms from the recovery of these spent solvents and spent
	solvent mixtures.
F004..................	The following spent non-halogenated solvents:  Cresols and cresylic	  (T)
	acid, and nitrobenzene; all spent solvent mixtures/blends containing, 
	before use, a total of ten percent or more (by volume) of one or more 
	of the above non-halogenated solvents or those solvents listed in 
	F001, F002, and F005; and still bottoms from the recovery of these 
	spent solvents and spent solvents mixtures.
F005..................	The following spent non-halogenated solvents:  Toluene, methyl ethyl	  (I,T)
	ketone, carbon disulfide, isobutanol, and pyridine; all spent solvent 
	mixtures/blends containing, before use, a total of ten percent or more 
	(by volume) of one or more of the above non-halogenated solvents or 
	those solvents listed in F001, F002, and F004; and still bottoms from 
	the recovery of these spent solvents and spent solvent mixtures.

*	(I,T) should be used to specify mixtures containing ignitable and toxic constituents.