RCRA REVISION CHECKLIST 23

Generators of 100 to 1000 kg Hazardous Waste
51 FR 10146-10176
March 24, 1986
(HSWA Cluster I)

Note:  On July 19, 1988 (53 FR 27162, Revision Checklist 47), technical corrections were made to provisions addressed by this checklist.  Consequently, States seeking authorization for this checklist are advised to incorporate the technical corrections addressed in Revision Checklist 47 when revising their code in order to avoid separate revisions.  Revision Checklist 42 also addresses requirements for small quantity generators.
	STATE ANALOG IS:
		     ANALOGOUS	  EQUIV-	   MORE	BROADER
   FEDERAL REQUIREMENT     | 	FEDERAL RCRA CITATION    |	   STATE CITATION	| ALENT  |	STRINGENT |	IN SCOPE	

PART 260 - HAZARDOUS WASTE MANAGEMENT SYSTEM:  GENERAL

SUBPART B - DEFINITIONS

DEFINITIONS	 
small quantity
generator	260.10	

PART 261 - IDENTIFICATION AND LISTING OF HAZARDOUS WASTE

SUBPART A - GENERAL

PURPOSE AND SCOPE	 

subpart A scope	261.1(a)(1)	

SPECIAL REQUIREMENTS FOR HAZARDOUS WASTE GENERATED BY CONDITIONALLY
EXEMPT SMALL QUANTITY GENERATORS	 
conditionally
exempt generators	261.5(a)	

exceptions	261.5(b)	

quantity determination	261.5(c)	

quantity exclusions	261.5(d)	

acutely hazardous	261.5(e)	

accumulation	261.5(f)	
requirements to be
conditionally exempt	261.5(g)	
mixing with non-
hazardous waste	261.5(h)	
mixtures that exceed
exclusion level	261.5(i)	

mixtures with used oil	261.5(j)	

remove paragraph	261.5(k)	

SUBPART D - LISTS OF HAZARDOUS WASTE

DISCARDED COMMERCIAL CHEMICAL PRODUCTS, ETC.	 

introductory text	261.33(f)	

PART 262 - STANDARDS APPLICABLE TO GENERATORS OF HAZARDOUS WASTE

SUBPART B - THE MANIFEST

GENERAL REQUIREMENTS	 
100 to 1000 kg
exemption	262.20(e)	

SUBPART C - PRE-TRANSPORT REQUIREMENTS

ACCUMULATION TIME	 

introductory text	262.34(a)	
100 to 1000 kg and
accumulation of
180 days	262.34(d)	
200 miles transport
and 270 day
accumulation	262.34(e)	

6000 kg or 180 days	262.34(f)	

SUBPART D - RECORDKEEPING AND REPORTING

SPECIAL REQUIREMENTS FOR GENERATORS OF BETWEEN 100 AND 1000 kg/mo.	 

special requirements	262.44	

PART 263 - STANDARDS APPLICABLE TO TRANSPORTERS OF HAZARDOUS WASTE

SUBPART B - COMPLIANCE WITH THE MANIFEST SYSTEM AND RECORDKEEPING

MANIFEST SYSTEM	 
applicability of
100 to 1000 kg	263.20(h)	

PART 270 - EPA ADMINISTERED PERMIT PROGRAMS:  THE HAZARDOUS
WASTE PROGRAM

SUBPART A - GENERAL INFORMATION

PURPOSE AND SCOPE OF THESE REGULATIONS	 

specific exclusions	270.1(c)(2)(i)	

SUBPART B - PERMIT APPLICATION

GENERAL APPLICATION REQUIREMENTS	 

existing facilities	270.10(e)(1)(iii)