RCRA REVISION CHECKLIST 189

Chlorinated Aliphatics Listing and LDRs for Newly Identified Wastes
65 FR 67068-67133
November 8, 2000
(RCRA Cluster XI, HSWA)

	FEDERAL REQUIREMENTS		FEDERAL RCRA CITATION	ANALOGOUS STATE CITATION	STATE ANALOG IS:				
					EQUIV-ALENT	LESS
STRIN-
GENT	MORE STRIN-GENT	BROADER IN SCOPE	
	PART 261 – IDENTIFICATION AND LISTING OF HAZARDOUS WASTE								
	SUBPART D – LISTS OF HAZARDOUS WASTES								
	HAZARDOUS WASTES FROM SPECIFIC SOURCES								
	add following waste streams to subgroup “Organic chemicals” in alphanumeric order		261.32						
	Industry and EPA hazardous waste No.		Hazardous Waste					Hazard code	
	*	*	*	*	*	*	*	*	*	*	*	*								
	Organic chemicals:								
	*	*	*	*	*	*	*	*	*	*	*	*								
	K174		Wastewater treatment sludges from the production of ethylene dichloride or vinyl chloride monomer (including sludges that result from commingled ethylene dichloride or vinyl chloride monomer wastewater and other wastewater), unless the sludges meet the following conditions: (i) they are disposed of in a subtitle C or non-hazardous landfill licensed or permitted by the state or federal government; (ii) they are not otherwise placed on the land prior to final disposal; and (iii) the generator maintains documentation demonstrating that the waste was either disposed of in an on-site landfill or consigned to a transporter or disposal facility that provided a written commitment to dispose of the waste in an off-site landfill.  Respondents in any action brought to enforce the requirements of subtitle C must, upon a showing by the government that the respondent managed wastewater treatment sludges from the production of vinyl chloride monomer or ethylene dichloride, demonstrate that they meet the terms of the exclusion set forth above.  In doing so, they must provide appropriate documentation (e.g., contracts between the generator and the landfill owner/operator, invoices documenting delivery of waste to landfill, etc.) that the terms of the exclusion were met.						(T)	
	K175 		Wastewater treatment sludges from the production of vinyl chloride monomer using mercuric chloride catalyst in an acetylene-based process.						(T)	
	*	*	*	*	*	*	*	*	*	*	*	*								

	APPENDIX VII TO PART 261								
	BASIS FOR LISTING HAZARDOUS WASTE								

	add to appendix in alphanumeric order, the following waste streams		261 Appendix VII						
	EPA hazardous waste No.		Hazardous constituents for which listed						
	*	*	*	*	*	*	*	*	*	*	*	*								
	K174			1,2,3,4,6,7,8-Heptachlorodibenzo-p-dioxin (1,2,3,4,6,7,8-HpCDD), 1,2,3,4,6,7,8-Heptachlorodibenzofuran (1,2,3,4,6,7,8-HpCDF), 1,2,3,4,7,8,9-Heptachlorodibenzofuran (1,2,3,6,7,8,9-HpCDF), HxCDDs (All Hexachlorodibenzo-p-dioxins), HxCDFs (All Hexachlorodibenzofurans), PeCDDs (All Pentachlorodibenzo-p-dioxins), OCDD (1,2,3,4,6,7,8,9-Octachlorodibenzo-p-dioxin), OCDF (1,2,3,4,6,7,8,9-Octachlorodibenzofuran), PeCDFs (All Pentachlorodibenzofurans), TCDDs (All Tetrachlorodibenzo-p-dioxins), TCDFs (All Tetrachlorodibenzofurans).						
	K175			Mercury						
	*	*	*	*	*	*	*	*	*	*	*	*								
	APPENDIX VIII TO PART 261								
	HAZARDOUS CONSTITUENTS								
	add to appendix in alphabetical order, the following entries		261 Appendix VIII						
	Common name			Chemical abstracts name		Chemical abstracts No.		Hazardous waste No.	
	*	*	*	*	*	*	*	*	*	*	*	*								
	Octachlorodibenzo-p-dioxin (OCDD).				1,2,3,4,6,7,8,9-Octachlorodibenzo-p-dioxin			
3268-87-9		
	
	Octachlorodibenzofuran (OCDF).				1,2,3,4,6,7,8,9-Octachlorodibenzofuran			39001-02-0			
	*	*	*	*	*	*	*	*	*	*	*	*								

	PART 268 – LAND DISPOSAL RESTRICTIONS								
	SUBPART C – PROHIBITIONS ON LAND DISPOSAL								
	WASTE SPECIFIC PROHIBITIONS -- CHLORINATED ALIPHATIC WASTES								
	add new paragraph; effective May 8, 2001, wastes K174 and K175, soil and debris contaminated with these wastes, radioactive wastes mixed with these wastes, and soil and debris contaminated with radioactive wastes mixed with these wastes are prohibited from land disposal		268.33(a)						
	add new paragraph; requirements of 268.33(a) do not apply if:		268.33(b) intro						
	wastes meet treatment standards specified in 268 subpart D;		268.33(b)(1)						
	exemption from a prohibition pursuant to petition granted under 268.6, with respect to wastes and units covered by the petition;		268.33(b)(2) 						
	wastes meet treatment standards established pursuant to petition granted under 268.44;		268.33(b)(3) 						
	hazardous debris has met treatment standards in 268.40 or alternative treatment standards in 268.45; or		268.33(b)(4)						
	extension to effective date of prohibition granted pursuant to 268.5, with respect to wastes covered by extension		268.33(b)(5)						
	add new paragraph; to determine if identified hazardous waste exceeds 268.40 treatment standards, initial generator must test waste, or use knowledge of waste; if waste contains regulated constituents in excess of 268 subpart D levels, waste is prohibited from land disposal, and all requirements of part 268 are applicable, except as otherwise specified		268.33(c)						
	add new paragraph; disposal of K175 wastes  complying with 268.40 treatment standards must also be macroencapsulated in accordance with 268.45 Table 1 unless waste is placed in:		268.33(d) intro						
	Subtitle C monofill containing only applicable K175 wastes that meet 268.40 treatment standards; or		268.33(d)(1)						
	dedicated Subtitle C landfill cell in which other co-disposed wastes are at pH#6.0		268.33(d)(2)						
	SUBPART D – TREATMENT STANDARDS								
	APPLICABILITY OF TREATMENT STANDARDS								
	add entries to F039 in alphabetic order, add in alphanumeric order new entries for K174 and K175, and add new footnote 12 as shown at 65 FR 67128-67131		268.40/Table						
	UNIVERSAL TREATMENT STANDARDS								
	add following to the subgroup “Organic Constituents” in alphabetical order		268.48(a)/Table						
	UNIVERSAL TREATMENT STANDARDS   NOTE:  NA means not applicable								
	REGULATED CONSTITUENT
Common Name			CAS1 Number	Wastewater Standard		Nonwastewater Standard		
					Concentration in mg/l2		Concentration in mg/kg3 unless noted as “mg/l TCLP”		
	*	*	*	*	*	*	*	*	*	*	*	*								
	1,2,3,4,6,7,8-Heptachlorodibenzo-p-dioxin (1,2,3,4,6,7,8-HpCDD)				35822-46-9	0.000035		0.0025		
	1,2,3,4,6,7,8-Heptachlorodibenzofuran (1,2,3,4,6,7,8-HpCDF)				67562-39-4	0.000035		0.0025		
	1,2,3,4,7,8,9-Heptachlorodibenzofuran (1,2,3,4,7,8,9-HpCDF)				55673-89-7	0.000035		0.0025		
	*	*	*	*	*	*	*	*	*	*	*	*								
	1,2,3,4,6,7,8,9-Octachlorodibenzo-p-dioxin (OCDD)				3268-87-9	0.000063		0.005		
	1,2,3,4,6,7,8,9-Octachlorodibenzofuran (OCDF)				39001-02-0	0.000063		0.005		
	*	*	*	*	*	*	*	*	*	*	*	*