RCRA REVISION CHECKLIST 235

Disposal of Coal Combustion Residuals from Electric Utilities
80 FR 21302-21501
	April 17, 2015
	(RCRA Cluster XXIV, Non-HSWA)

Name of State:  

State Statutory Authority: 

Title of Regulations:  							Effective Date:   

Date Checklist Completed:  

	
FEDERAL REQUIREMENTS	
FEDERAL RCRA CITATION	
ANALOGOUS STATE CITATION	
STATE ANALOG IS:	
				
EQUIV-ALENT	
LESS
STRIN-
GENT	
MORE STRIN-GENT	
BROADER IN SCOPE	
	PART 261 IDENTIFICATION AND LISTING OF HAZARDOUS WASTE	
	SUBPART A - GENERAL	
	Fly ash waste, bottom ash waste, slag waste, and flue gas emission control waste generated primarily from the combustion of coal or other fossil fuels, except as provided by § 266.112 of this chapter for facilities that burn or process hazardous waste.	261.4(b)(4)(i)						
	The following wastes generated primarily from processes that support the combustion of coal or other fossil fuels that are co-disposed with the wastes in paragraph (b)(4)(i) of this section, except as provided by § 266.112 of this chapter for facilities that burn or process hazardous waste:	261.4(b)(4)(ii)						
	Coal pile run-off. For purposes of paragraph (b)(4) of this section, coal pile run-off means any precipitation that drains off coal piles.	261.4(b)(4)(ii)(A)						
	Boiler cleaning solutions. For purposes of paragraph (b)(4) of this section, boiler cleaning solutions means water solutions and chemical solutions used to clean the fire-side and waterside of the boiler.	261.4(b)(4)(ii)(B)						
	Boiler blowdown. For purposes of paragraph (b)(4) of this section, boiler blowdown means water purged from boilers used to generate steam.	261.4(b)(4)(ii)(C)						
	Process water treatment and demineralizer regeneration wastes. For purposes of paragraph (b)(4) of this section, process water treatment and demineralizer regeneration wastes means sludges, rinses, and spent resins generated from processes to remove dissolved gases, suspended solids, and dissolved chemical salts from combustion system process water.	261.4(b)(4)(ii)(D)						
	Cooling tower blowdown. For purposes of paragraph (b)(4) of this section, cooling tower blowdown means water purged from a closed cycle cooling system. Closed cycle cooling systems include cooling towers, cooling ponds, or spray canals.	261.4(b)(4)(ii)(E)						
	Air heater and precipitator washes. For purposes of paragraph (b)(4) of this section, air heater and precipitator washes means wastes from cleaning air preheaters and electrostatic precipitators.	261.4(b)(4)(ii)(F)						
	Effluents from floor and yard drains and sumps. For purposes of paragraph (b)(4) of this section, effluents from floor and yard drains and sumps means wastewaters, such as wash water, collected by or from floor drains, equipment drains, and sumps located inside the power plant building; and wastewaters, such as rain runoff, collected by yard drains and sumps located outside the power plant building.	261.4(b)(4)(ii)(G)						
	Wastewater treatment sludges. For purposes of paragraph (b)(4) of this section, wastewater treatment sludges refers to sludges generated from the treatment of wastewaters specified in paragraphs (b)(4)(ii)(A) through (F) of this section.	261.4(b)(4)(ii)(H)