{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Test Info","ESRI_MAPINFO_SHEET"],"not_rendered":{"images":1,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Test Info","index":0,"n_rows":228418,"n_cols":55,"rows_kept":1125,"cut":true,"bounds":{"rows_first":500,"rows_last":125,"rows_between":500,"halvings":2}}
[]
["Model Year","Certificate Manufacturer Name","Certified Test Group","Certified Evaporative Family","Represented Test Vehicle Make","Represented Test Vehicle Model","Vehicle ID","Vehicle Configuration Number","Displacement (L)","Curb Weight (lbs.)","Gross Vehicle Weight Rating (lbs.)","Equivalent Test Weight (lbs.)","Test Drive","Test Drive Description","Transmission Type","Transmission Type Description","Transmission type, if other","Number of Gears","Transmission Lockup Yes/No?","Creeper Gear Yes/No?","Vehicle Fuel Category","Vehicle Fuel Category Description","Hybrid Yes/No?","Set Coefficient A (lbf)","Set Coefficient B (lbf/mph)","Set Coefficient C (lbf/mph**2)","Target Coefficient A (lbf)","Target Coefficient B (lbf/mph)","Target Coefficient C (lbf/mph**2)","Test Number","Test Originator","Test Procedure","Test Procedure Description","Test Fuel","Test Fuel Description","Certification/In-Use Code","Vehicle Class","Vehicle Class Description","Certification Region","Certification Region Description","Emission Standard Level Code","Emission Standard Level Description","Useful Life Miles (k)","Emission Name","Rounded Emission Result (g/mi)","Certification Level (g/mi)","Emission Standard (g/mi)","Additive Deterioration Factor","Multiplicative Deterioration Factor","Using NMOG/NMHC Ratio?","Ratio of NMOG to NMHC","Upward Diesel Adjustment Factor","Downward Diesel Adjustment Factor","Reactivity Factor (RAF)","Carline Models Covered"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059216","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","CO",0.14,0.1,"1.7",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059216","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","HCHO",0.0004,1E-3,"0.004",0.0002,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059216","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.0077,0.012,"999.999",4.3E-3,null,"Y",1.1,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059216","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.0188,0.031,"0.070",null,1,"Y",1.1,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059216","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.0111,0.019,"999.999",0.0082,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059216","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","PM",3.0000000000000003E-4,0,"0.003",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059216","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","CO",0.14,0.1,"1.7",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059216","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","HCHO",0.0004,1E-3,"0.004",0.0002,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059216","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.0077,0.012,"999.999",4.3E-3,null,"Y",1.09907,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059216","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.0188,0.031,"0.070",null,1,"Y",1.09907,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059216","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.0111,0.019,"999.999",0.0082,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059216","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","PM",3.0000000000000003E-4,0,"0.003",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059218","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","120","CREE",999,999,"999.999",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059218","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.0002,0.004,"999.999",4.3E-3,null,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059218","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.0025,0.015000000000000001,"0.070",null,1,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059218","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",2.3E-3,0.01,"999.999",0.0082,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059218","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","CREE",999,999,"999.999",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059218","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.0002,0.004,"999.999",4.3E-3,null,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059218","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.0025,0.015000000000000001,"0.070",null,1,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059218","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",2.3E-3,0.01,"999.999",0.0082,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059219","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","CO",2.4530000000000003,2.4530000000000003,"999.999",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059219","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.006500000000000001,0.011000000000000001,"999.999",4.3E-3,null,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059219","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.0097,0.018000000000000002,"999.999",0.0082,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059219","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","PM",0.0004,0,"0.006",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059219","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","CO",2.4530000000000003,2.4530000000000003,"999.999",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059219","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.006500000000000001,0.011000000000000001,"999.999",4.3E-3,null,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059219","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.0097,0.018000000000000002,"999.999",0.0082,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059219","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","PM",0.0004,0,"0.006",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059221","MFR","95","SC03","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","CO",0.24100000000000002,0.24100000000000002,"999.999",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059221","MFR","95","SC03","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",6.0000000000000006E-4,0.005,"999.999",4.3E-3,null,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059221","MFR","95","SC03","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.0204,0.029,"999.999",0.0082,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059221","MFR","95","SC03","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","CO",0.24100000000000002,0.24100000000000002,"999.999",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059221","MFR","95","SC03","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",6.0000000000000006E-4,0.005,"999.999",4.3E-3,null,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.530000000000001,-0.11460000000000001,0.02633,35.87,-0.0473,0.027600000000000003,"LHNX10059221","MFR","95","SC03","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.0204,0.029,"999.999",0.0082,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.200000000000001,-0.538,0.03258,39.46,-0.052000000000000005,0.030359999999999998,"LHNX10059222","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","50","CO",0.9,0.9,"12.5",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.200000000000001,-0.538,0.03258,39.46,-0.052000000000000005,0.030359999999999998,"LHNX10059222","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","HC-NM",0.16,0.2,"0.3",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","Honda","ODYSSEY","ELMR1A",0,3.5,4592,6019,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.200000000000001,-0.538,0.03258,39.46,-0.052000000000000005,0.030359999999999998,"LHNX10059222","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","50","CO",0.9,0.9,"12.5",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046178","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","CO",0.397,0.397,"999.999",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046178","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.0109,0.015000000000000001,"999.999",4.3E-3,null,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046178","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.0158,0.024,"999.999",0.0082,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046178","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","CO",0.397,0.397,"999.999",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046178","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.0109,0.015000000000000001,"999.999",4.3E-3,null,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046178","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.0158,0.024,"999.999",0.0082,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046367","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","CO",0.139,0.139,"999.999",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046367","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.008700000000000001,0.013000000000000001,"999.999",4.3E-3,null,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046367","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.0118,0.02,"999.999",0.0082,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046367","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","CO",0.139,0.139,"999.999",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046367","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.008700000000000001,0.013000000000000001,"999.999",4.3E-3,null,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046367","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.0118,0.02,"999.999",0.0082,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",1.53,0.0956,0.02717,39.46,-0.052000000000000005,0.0304,"JHNX10046368","MFR","11","Cold CO","26","Cold CO Regular (Tier 2)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","50","CO",0.66,0.7000000000000001,"12.5",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",1.53,0.0956,0.02717,39.46,-0.052000000000000005,0.0304,"JHNX10046368","MFR","11","Cold CO","26","Cold CO Regular (Tier 2)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","HC-NM",0.1,0.1,"0.3",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",1.53,0.0956,0.02717,39.46,-0.052000000000000005,0.0304,"JHNX10046368","MFR","11","Cold CO","26","Cold CO Regular (Tier 2)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","50","CO",0.66,0.7000000000000001,"12.5",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046399","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","120","CREE",365,365,"999.999",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046399","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","CREE",365,365,"999.999",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046399","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","METHANE",2.9000000000000002E-3,0.004,"0.030",1.3000000000000002E-3,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046399","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","N2O",1.7000000000000001E-3,2E-3,"0.010",0.0002,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046400","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","120","CREE",225,225,"999.999",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046400","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.0011,0.005,"999.999",4.3E-3,null,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046400","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.0044,0.017,"0.070",null,1,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046400","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",3.3E-3,0.012,"999.999",0.0082,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046400","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","CREE",225,225,"999.999",0,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046400","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.0011,0.005,"999.999",4.3E-3,null,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046400","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.0044,0.017,"0.070",null,1,"Y",1.03,{"$nulls":3},"Honda: ODYSSEY FWD"]
[2022,"Honda","NHNXT03.5J4C","NHNXR01502SA","HONDA","ODYSSEY FWD","EHMR4A",1,3.5,4588,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.3,-0.2429,0.02863,35.87,-0.0473,0.027600000000000003,"JHNX10046400","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",3.3E-3,0.012,"999.999",0.0082,null,"N",{"$nulls":4},"Honda: ODYSSEY FWD"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066852","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","CO",0.46,0.8,"1.7",0.31,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066852","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.010700000000000001,0.021,"99.999",0.010100000000000001,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066852","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.019200000000000002,0.031,"0.070",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066852","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.0085,0.01,"99.999",1.9E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066852","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","PM",6.0000000000000006E-4,1E-3,"0.003",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066852","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","CREE",999,999,"999",0.267518,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066852","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","METHANE",2.9000000000000002E-3,0.006,"0.030",3.1000000000000003E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066852","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","CO",0.46,0.8,"1.7",0.31,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066852","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.010700000000000001,0.021,"99.999",0.010100000000000001,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066852","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.019200000000000002,0.031,"0.070",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066852","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.0085,0.01,"99.999",1.9E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066852","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","PM",6.0000000000000006E-4,1E-3,"0.003",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066853","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.0002,0.01,"99.999",0.010100000000000001,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066853","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.0037,0.016,"0.070",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066853","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.0035,0.005,"99.999",1.9E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066853","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","CREE",999,999,"999",0.267518,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066853","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.0002,0.01,"99.999",0.010100000000000001,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066853","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.0037,0.016,"0.070",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066853","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.0035,0.005,"99.999",1.9E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066854","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","CO",0.48510000000000003,0.795,"99.999",0.31,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066854","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.014700000000000001,0.025,"99.999",0.010100000000000001,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066854","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.0279,0.04,"99.999",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066854","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.0132,0.015000000000000001,"99.999",1.9E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066854","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","PM",1.8000000000000002E-3,2E-3,"0.006",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066854","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","CO",0.48510000000000003,0.795,"99.999",0.31,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066854","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.014700000000000001,0.025,"99.999",0.010100000000000001,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066854","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.0279,0.04,"99.999",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066854","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.0132,0.015000000000000001,"99.999",1.9E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066854","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","PM",1.8000000000000002E-3,2E-3,"0.006",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066855","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","CO",0.8182,1.1280000000000001,"99.999",0.31,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066855","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",3.9000000000000003E-3,0.014,"99.999",0.010100000000000001,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066855","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.0143,0.026000000000000002,"99.999",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066855","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.010400000000000001,0.012,"99.999",1.9E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066855","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","CO",0.8182,1.1280000000000001,"99.999",0.31,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066855","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",3.9000000000000003E-3,0.014,"99.999",0.010100000000000001,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066855","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.0143,0.026000000000000002,"99.999",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066855","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.010400000000000001,0.012,"99.999",1.9E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.904,-0.12879,0.03388,31.094,0.41046,0.0302,"NKMX10066856","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","50","CO",0.5700000000000001,0.7000000000000001,"12.5",0.1,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.904,-0.12879,0.03388,31.094,0.41046,0.0302,"NKMX10066856","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","HC-NM",0.05,0.1,"0.3",0.0073,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.904,-0.12879,0.03388,31.094,0.41046,0.0302,"NKMX10066856","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","50","CO",0.5700000000000001,0.7000000000000001,"12.5",0.1,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066857","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","4","CO",0.52,0.5,"1.7",null,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066857","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","4","NMOG",0.029,0.029,"99.999",null,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066857","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","4","NMOG+NOX",0.0397,0.04,"0.140",null,1,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10066857","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","4","NOX",0.010700000000000001,0.011000000000000001,"99.999",null,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067671","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","CO",0.53,0.8,"1.7",0.31,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067671","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.013600000000000001,0.024,"99.999",0.010100000000000001,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067671","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.023700000000000002,0.036000000000000004,"0.070",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067671","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.010100000000000001,0.012,"99.999",1.9E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067671","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","CREE",370,370,"999",0.267518,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067671","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","METHANE",0.004,0.007,"0.030",3.1000000000000003E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067671","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","N2O",0.0016,2E-3,"0.010",0.0002,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067671","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","CO",0.53,0.8,"1.7",0.31,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067671","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.013600000000000001,0.024,"99.999",0.010100000000000001,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067671","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.023700000000000002,0.036000000000000004,"0.070",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067671","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.010100000000000001,0.012,"99.999",1.9E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067672","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.0007,0.011000000000000001,"99.999",0.010100000000000001,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067672","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.0046,0.017,"0.070",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067672","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",3.9000000000000003E-3,0.006,"99.999",1.9E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067672","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","CREE",245,245,"999",0.267518,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067672","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.0007,0.011000000000000001,"99.999",0.010100000000000001,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067672","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.0046,0.017,"0.070",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXT03.5KU5","NKMXR0155KUG","KIA","CARNIVAL","KA4U2L5GA067F",0,3.5,4727,6041,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.447000000000001,0.23520000000000002,0.027583999999999997,28.268,0.37315,0.027455,"NKMX10067672","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",3.9000000000000003E-3,0.006,"99.999",1.9E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Carnival"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066983","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","CO",0.12,0.7000000000000001,"2.1",0.54,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066983","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",7.6E-3,0.029,"99.999",0.0217,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066983","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.0233,0.051000000000000004,"0.125",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066983","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.015700000000000002,0.022000000000000002,"99.999",0.006,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066983","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","PM",0.0002,0,"0.003",0.0002,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066983","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CREE",999,1000,"999",0.6730149999999999,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066983","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","METHANE",3.9000000000000003E-3,0.01,"0.030",0.0061,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066983","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.12,0.7000000000000001,"2.1",0.54,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066983","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",7.6E-3,0.029,"99.999",0.0217,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066983","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.0233,0.051000000000000004,"0.125",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066983","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.015700000000000002,0.022000000000000002,"99.999",0.006,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066983","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","PM",0.0002,0,"0.003",0.0002,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066984","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","CO",0.15910000000000002,0.6990000000000001,"99.999",0.54,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066984","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",3.9000000000000003E-3,0.026000000000000002,"99.999",0.0217,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066984","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.056,0.084,"99.999",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066984","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.0521,0.058,"99.999",0.006,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066984","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","PM",1E-3,1E-3,"0.006",0.0002,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066984","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.15910000000000002,0.6990000000000001,"99.999",0.54,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066984","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",3.9000000000000003E-3,0.026000000000000002,"99.999",0.0217,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066984","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.056,0.084,"99.999",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066984","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.0521,0.058,"99.999",0.006,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066984","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","PM",1E-3,1E-3,"0.006",0.0002,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066985","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","CO",0.1796,0.72,"99.999",0.54,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066985","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",1.9E-3,0.024,"99.999",0.0217,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066985","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.0111,0.039,"99.999",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066985","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.0092,0.015000000000000001,"99.999",0.006,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066985","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.1796,0.72,"99.999",0.54,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066985","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",1.9E-3,0.024,"99.999",0.0217,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066985","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.0111,0.039,"99.999",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066985","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.0092,0.015000000000000001,"99.999",0.006,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",9.040000000000001,-0.11403999999999999,0.023250999999999997,41.194,0.45619,0.020842,"NKMX10066986","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","50","CO",0.21,0.4,"10.0",0.17,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",9.040000000000001,-0.11403999999999999,0.023250999999999997,41.194,0.45619,0.020842,"NKMX10066986","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","HC-NM",0.01,0,"0.3",0.02,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",9.040000000000001,-0.11403999999999999,0.023250999999999997,41.194,0.45619,0.020842,"NKMX10066986","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","50","CO",0.21,0.4,"10.0",0.17,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066987","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",0.0011,0.023,"99.999",0.0217,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066987","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.0067,0.034,"0.125",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066987","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.0056,0.012,"99.999",0.006,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066987","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CREE",999,1000,"999",0.6730149999999999,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066987","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.0011,0.023,"99.999",0.0217,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066987","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.0067,0.034,"0.125",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066987","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.0056,0.012,"99.999",0.006,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066988","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","4","CO",0.22,0.2,"2.1",null,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066988","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","4","NMOG",0.0167,0.017,"99.999",null,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066988","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","4","NMOG+NOX",0.030600000000000002,0.031,"0.250",null,1,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10066988","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","4","NOX",0.013900000000000001,0.014,"99.999",null,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067435","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","CO",0.17,0.7000000000000001,"2.1",0.54,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067435","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",0.0082,0.03,"99.999",0.0217,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067435","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.0228,0.05,"0.125",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067435","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.0146,0.021,"99.999",0.006,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067435","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CREE",306,307,"999",0.6730149999999999,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067435","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","METHANE",4.3E-3,0.01,"0.030",0.0061,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067435","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","N2O",0.0022,0.006,"0.010",0.004,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067435","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.17,0.7000000000000001,"2.1",0.54,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067435","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.0082,0.03,"99.999",0.0217,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067435","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.0228,0.05,"0.125",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067435","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.0146,0.021,"99.999",0.006,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",3.8E-3,0.026000000000000002,"99.999",0.0217,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.0135,0.041,"0.125",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.0097,0.016,"99.999",0.006,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CREE",207,208,"999",0.6730149999999999,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",3.8E-3,0.026000000000000002,"99.999",0.0217,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.0135,0.041,"0.125",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV02.5EP6","NKMXR0132EPG","Kia","STINGER","CK-U2H5TA120A",0,2.5,3973,5027,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.099,0.23961,0.018883,37.449000000000005,0.41472,0.018947,"NKMX10067442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.0097,0.016,"99.999",0.006,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065923","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","CO",0.25,0.3,"2.1",0.02,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065923","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",0.017,0.026000000000000002,"99.999",8.6E-3,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065923","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.0201,0.03,"0.125",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065923","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",3.1000000000000003E-3,0.005,"99.999",0.0016,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065923","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","PM",0.0011,1E-3,"0.003",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065923","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CREE",999,999,"999",0.471638,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065923","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","METHANE",0.0059,0.009000000000000001,"0.030",2.8E-3,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065923","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.25,0.3,"2.1",0.02,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065923","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.017,0.026000000000000002,"99.999",8.6E-3,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065923","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.0201,0.03,"0.125",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065923","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",3.1000000000000003E-3,0.005,"99.999",0.0016,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065923","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","PM",0.0011,1E-3,"0.003",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065924","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","CO",0.09,0.11,"99.999",0.02,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065924","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",0.0132,0.022000000000000002,"99.999",8.6E-3,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065924","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.0239,0.034,"99.999",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065924","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.010700000000000001,0.012,"99.999",0.0016,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065924","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","PM",9.0000000000000008E-4,1E-3,"0.006",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065924","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.09,0.11,"99.999",0.02,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065924","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.0132,0.022000000000000002,"99.999",8.6E-3,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065924","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.0239,0.034,"99.999",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065924","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.010700000000000001,0.012,"99.999",0.0016,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065924","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","PM",9.0000000000000008E-4,1E-3,"0.006",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065925","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",0.0008,0.009000000000000001,"99.999",8.6E-3,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065925","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.006200000000000001,0.016,"0.125",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065925","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.0054,0.007,"99.999",0.0016,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065925","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CREE",999,999,"999",0.471638,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065925","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.0008,0.009000000000000001,"99.999",8.6E-3,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065925","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.006200000000000001,0.016,"0.125",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065925","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.0054,0.007,"99.999",0.0016,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065926","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","CO",0.01,0.03,"99.999",0.02,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065926","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",0.0027,0.011000000000000001,"99.999",8.6E-3,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065926","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.0073,0.018000000000000002,"99.999",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065926","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.0046,0.006,"99.999",0.0016,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065926","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.01,0.03,"99.999",0.02,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065926","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.0027,0.011000000000000001,"99.999",8.6E-3,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065926","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.0073,0.018000000000000002,"99.999",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065926","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.0046,0.006,"99.999",0.0016,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",8.997,0.48313,0.016294,49.918,0.71805,0.016933,"NKMX10065927","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","50","CO",0.73,0.7000000000000001,"10.0",0.01,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",8.997,0.48313,0.016294,49.918,0.71805,0.016933,"NKMX10065927","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","HC-NM",0.14,0.1,"0.3",0.006200000000000001,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",8.997,0.48313,0.016294,49.918,0.71805,0.016933,"NKMX10065927","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","50","CO",0.73,0.7000000000000001,"10.0",0.01,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065928","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","4","CO",0.32,0.3,"2.1",{"$nulls":7},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065928","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","4","NMOG",0.030100000000000002,0.03,"99.999",null,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065928","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","4","NMOG+NOX",0.032,0.032,"0.250",null,1,{"$nulls":5},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065928","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","4","NOX",1.9E-3,2E-3,"99.999",{"$nulls":7},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065952","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",0.0004,0.009000000000000001,"99.999",8.6E-3,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065952","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.0046,0.015000000000000001,"0.125",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065952","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.004200000000000001,0.006,"99.999",0.0016,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065952","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CREE",264,264,"999",0.471638,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065952","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.0004,0.009000000000000001,"99.999",8.6E-3,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065952","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.0046,0.015000000000000001,"0.125",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10065952","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.004200000000000001,0.006,"99.999",0.0016,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10066850","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","CO",0.56,0.6,"2.1",0.02,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10066850","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",0.0195,0.028,"99.999",8.6E-3,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10066850","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.0235,0.034,"0.125",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10066850","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.004,0.006,"99.999",0.0016,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10066850","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CREE",390,390,"999",0.471638,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10066850","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","METHANE",0.0077,0.01,"0.030",2.8E-3,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10066850","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","N2O",0.0022,0.003,"0.010",1.2000000000000001E-3,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10066850","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.56,0.6,"2.1",0.02,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10066850","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.0195,0.028,"99.999",8.6E-3,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10066850","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.0235,0.034,"0.125",0,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2022,"Kia","NKMXV03.3EK6","NKMXR0132EKG","Kia","STINGER","CK_U1L3TA144A",0,3.3000000000000003,4176,5137,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.331000000000001,0.34598999999999996,0.015739,45.38,0.65277,0.015392999999999999,"NKMX10066850","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.004,0.006,"99.999",0.0016,{"$nulls":6},"KIA MOTORS CORPORATION: Stinger AWD, Stinger RWD"]
[2021,"Altech","MAECD06.26BA","MAECF0000GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.26BA","MAECF0000GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.26BA","MAECF0000GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.022000000000000002,0.11,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.26BA","MAECF0000GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.26BA","MAECF0000GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.26BA","MAECF0000GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.01,0.098,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.26BA","MAECF0000GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.26BA","MAECF0000NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BA","MAECF0000NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BA","MAECF0000NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.022000000000000002,0.11,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BA","MAECF0000NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BA","MAECF0000NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BA","MAECF0000NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.01,0.098,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BA","MAECF0000NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BA","MAECF0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BA","MAECF0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BA","MAECF0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.022000000000000002,0.11,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BA","MAECF0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BA","MAECF0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BA","MAECF0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.01,0.098,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BA","MAECF0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BA","MAECR0000NH1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BA","MAECR0000NH1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BA","MAECR0000NH1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.022000000000000002,0.11,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BA","MAECR0000NH1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BA","MAECR0000NH1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BA","MAECR0000NH1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.01,0.098,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BA","MAECR0000NH1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BA","MAECR0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BA","MAECR0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BA","MAECR0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.022000000000000002,0.11,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BA","MAECR0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BA","MAECR0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BA","MAECR0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.01,0.098,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BA","MAECR0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BC","MAECF0210GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.26BC","MAECF0210GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.26BC","MAECF0210GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.022000000000000002,0.11,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.26BC","MAECF0210GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.26BC","MAECF0210GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.26BC","MAECF0210GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.01,0.098,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.26BC","MAECF0210GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.26BC","MAECF0250NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BC","MAECF0250NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BC","MAECF0250NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.022000000000000002,0.11,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BC","MAECF0250NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BC","MAECF0250NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BC","MAECF0250NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.01,0.098,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BC","MAECF0250NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BC","MAECF0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BC","MAECF0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BC","MAECF0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.022000000000000002,0.11,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BC","MAECF0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BC","MAECF0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BC","MAECF0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.01,0.098,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BC","MAECF0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250  2WD Bed Delete, F250  4WD Bed Delete, F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.26BC","MAECR0250NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BC","MAECR0250NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BC","MAECR0250NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.022000000000000002,0.11,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BC","MAECR0250NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BC","MAECR0250NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BC","MAECR0250NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.01,0.098,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BC","MAECR0250NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BC","MAECR0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BC","MAECR0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BC","MAECR0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.022000000000000002,0.11,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BC","MAECR0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BC","MAECR0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BC","MAECR0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.01,0.098,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.26BC","MAECR0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BA","MAECF0000GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.27BA","MAECF0000GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.27BA","MAECF0000GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.022000000000000002,0.11,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.27BA","MAECF0000GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.27BA","MAECF0000GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.27BA","MAECF0000GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.01,0.098,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.27BA","MAECF0000GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.27BA","MAECF0000NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BA","MAECF0000NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BA","MAECF0000NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.022000000000000002,0.11,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BA","MAECF0000NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BA","MAECF0000NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BA","MAECF0000NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.01,0.098,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BA","MAECF0000NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BA","MAECF0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BA","MAECF0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BA","MAECF0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.022000000000000002,0.11,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BA","MAECF0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BA","MAECF0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BA","MAECF0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.01,0.098,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BA","MAECF0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BA","MAECR0000NH1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BA","MAECR0000NH1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BA","MAECR0000NH1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.022000000000000002,0.11,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BA","MAECR0000NH1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BA","MAECR0000NH1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BA","MAECR0000NH1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.01,0.098,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BA","MAECR0000NH1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BA","MAECR0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BA","MAECR0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BA","MAECR0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.022000000000000002,0.11,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BA","MAECR0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BA","MAECR0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BA","MAECR0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.01,0.098,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BA","MAECR0000NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BC","MAECF0210GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.27BC","MAECF0210GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.27BC","MAECF0210GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.022000000000000002,0.11,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.27BC","MAECF0210GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.27BC","MAECF0210GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.27BC","MAECF0210GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.01,0.098,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.27BC","MAECF0210GDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2021,"Altech","MAECD06.27BC","MAECF0250NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BC","MAECF0250NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BC","MAECF0250NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.022000000000000002,0.11,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BC","MAECF0250NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BC","MAECF0250NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BC","MAECF0250NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.01,0.098,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BC","MAECF0250NDJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BC","MAECF0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BC","MAECF0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BC","MAECF0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.022000000000000002,0.11,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BC","MAECF0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BC","MAECF0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BC","MAECF0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.01,0.098,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BC","MAECF0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350  4WD Bed Delete, F350 2WD Bed Delete"]
[2021,"Altech","MAECD06.27BC","MAECR0250NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BC","MAECR0250NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BC","MAECR0250NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.022000000000000002,0.11,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BC","MAECR0250NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BC","MAECR0250NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BC","MAECR0250NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.01,0.098,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BC","MAECR0250NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BC","MAECR0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","CO",0.7000000000000001,1.5,"4.2",0.768,{"$nulls":6},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BC","MAECR0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",6.3E-3,0.044000000000000004,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BC","MAECR0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.022000000000000002,0.11,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BC","MAECR0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.015700000000000002,0.066,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BC","MAECR0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG",3.1000000000000003E-3,0.041,"999.999",0.0376,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BC","MAECR0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.01,0.098,"0.270",null,1,{"$nulls":5},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"Altech","MAECD06.27BC","MAECR0360NHJ","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065442","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","CO",0.08,0.6,"2.1",0.47000000000000003,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065442","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","CREE",999,999,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065442","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","METHANE",0.003,0,"0.03",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065442","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","N2O",2E-3,0,"0.01",0.003,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065442","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NMOG",0.021,0.021,"999.999",0,null,null,1.1,null,null,1,"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065442","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NMOG+NOX",0.031,0.034,"0.125",0.003,null,null,1.1,{"$nulls":3},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065442","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NOX",0.01,0.013000000000000001,"999.999",0.003,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065442","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.08,0.6,"2.1",0.47000000000000003,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065442","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CREE",999,999,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065442","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","METHANE",0.003,0,"0.03",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065442","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","N2O",2E-3,0,"0.01",0.003,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065442","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.021,0.021,"999.999",0,null,"Y",1.1,null,null,1,"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065442","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.031,0.034,"0.125",3.3E-3,null,null,1.04,{"$nulls":3},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065442","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.01,0.013000000000000001,"999.999",0.003,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065444","MFR","3","HWFE","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","CREE",999,999,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065444","MFR","3","HWFE","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NMOG",1.2000000000000001E-3,1E-3,"999.999",0,null,null,1.1,{"$nulls":3},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065444","MFR","3","HWFE","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NMOG+NOX",0.004200000000000001,0.007,"0.125",3.3E-3,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065444","MFR","3","HWFE","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NOX",0.003,0.006,"999.999",0.003,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065444","MFR","3","HWFE","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CREE",999,999,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065444","MFR","3","HWFE","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",1.2000000000000001E-3,1E-3,"999.999",0,null,null,1.1,{"$nulls":3},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065444","MFR","3","HWFE","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.004200000000000001,0.007,"0.125",3.3E-3,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065444","MFR","3","HWFE","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.003,0.006,"999.999",0.003,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.800000000000004,-0.45480000000000004,0.039900000000000005,85.06,-0.22360000000000002,0.038200000000000005,"MASX10065446","MFR","11","Cold CO","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","HC-NM",0.11,0.1,"0.3",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.800000000000004,-0.45480000000000004,0.039900000000000005,85.06,-0.22360000000000002,0.038200000000000005,"MASX10065446","MFR","11","Cold CO","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","50","CO",1.3,1,"10",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.800000000000004,-0.45480000000000004,0.039900000000000005,85.06,-0.22360000000000002,0.038200000000000005,"MASX10065446","MFR","11","Cold CO","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","HC-NM",0.11,0.1,"0.3",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.800000000000004,-0.45480000000000004,0.039900000000000005,85.06,-0.22360000000000002,0.038200000000000005,"MASX10065446","MFR","11","Cold CO","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","50","CO",1.3,1,"10",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065447","MFR","95","SC03","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","4","CO",0.01,0,"2.7",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065447","MFR","95","SC03","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","4","HC-NM+NOX",0.03,0,"0.2",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065448","MFR","90","US06","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","4","CO",0.4,0,"8",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065448","MFR","90","US06","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","4","HC-NM+NOX",0.011000000000000001,0.01,"0.14",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXJ04.0AEX","MASXR0160P1Y","Aston Martin","DBX","8001PT8342",0,4,5082,null,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",51.64,-0.6349,0.038400000000000004,77.33,-0.2033,0.0347,"MASX10065449","MFR","51","CA fuel 50 Deg(F) exhaust test","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","50","CO",0.24,0.2,"2.1",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DBX V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050824","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","CO",0.07,0.4,"2.1",0.36,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050824","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","CREE",387,387,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050824","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","METHANE",0.005,0.02,"0.03",0.011300000000000001,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050824","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","N2O",0.006,0.01,"0.01",2E-3,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050824","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NMOG",0.0219,0.033,"999.999",0.011300000000000001,null,null,1.04,null,null,1,"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050824","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NMOG+NOX",0.0509,0.064,"0.125",0.013000000000000001,null,null,1.04,{"$nulls":3},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050824","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NOX",0.029,0.031,"999.999",2E-3,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050824","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.07,0.4,"2.1",0.36,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050824","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CREE",387,387,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050824","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","METHANE",0.005,0.02,"0.03",0.011300000000000001,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050824","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","N2O",0.006,0.01,"0.01",2E-3,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050824","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.0219,0.033,"999.999",0.011300000000000001,null,"Y",1.04,null,null,1,"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050824","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.0509,0.064,"0.125",0.013300000000000001,null,null,1.04,{"$nulls":3},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050824","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.029,0.031,"999.999",2E-3,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050825","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","CREE",260,260,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050825","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NMOG",0,0.011000000000000001,"999.999",0.011300000000000001,null,null,1.04,{"$nulls":3},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050825","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NMOG+NOX",2E-3,0.015000000000000001,"0.125",0.013300000000000001,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050825","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NOX",2E-3,0.004,"999.999",2E-3,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050825","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CREE",260,260,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050825","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0,0.011000000000000001,"999.999",0.011300000000000001,null,null,1.04,{"$nulls":3},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050825","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",2E-3,0.015000000000000001,"0.125",0.013300000000000001,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050825","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",2E-3,0.004,"999.999",2E-3,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050826","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","4","CO",0.2,0,"8",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050826","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","4","HC-NM+NOX",0.037000000000000005,0.04,"0.14",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050850","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","4","CO",0.7000000000000001,0.7000000000000001,"2.7",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050850","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","4","HC-NM+NOX",0.03,0,"0.2",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",15.8,0.0937,0.0281,45.51,0.0188,0.030100000000000002,"JASX10050851","MFR","11","Cold CO","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","HC-NM",0.07,0.1,"0.3",0.011300000000000001,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",15.8,0.0937,0.0281,45.51,0.0188,0.030100000000000002,"JASX10050851","MFR","11","Cold CO","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","50","CO",0.3,0,"10",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",15.8,0.0937,0.0281,45.51,0.0188,0.030100000000000002,"JASX10050851","MFR","11","Cold CO","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","HC-NM",0.07,0.1,"0.3",0.011300000000000001,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",15.8,0.0937,0.0281,45.51,0.0188,0.030100000000000002,"JASX10050851","MFR","11","Cold CO","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","50","CO",0.3,0,"10",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV04.0AES","MASXR0160P1Y","Aston Martin","DB11 V8","562TT5348",0,4,3891,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.26,0.09190000000000001,0.0251,40.94,0.016900000000000002,0.027100000000000003,"JASX10050852","MFR","51","CA fuel 50 Deg(F) exhaust test","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","50","CO",0.12,0.1,"2.1",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V8, Vantage Manual, Vantage V8"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055440","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","CO",0.98,1.1,"2.1",0.1,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055440","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","CREE",502,502,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055440","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","METHANE",0.011000000000000001,0.01,"0.03",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055440","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","N2O",0,0,"0.01",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055440","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NMOG",0.033800000000000004,0.034,"999.999",0,null,null,1.04,null,null,1,"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055440","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NMOG+NOX",0.06,0.06,"0.125",0,null,null,1.04,{"$nulls":3},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055440","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NOX",0.0262,0.026000000000000002,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055440","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.98,1.1,"2.1",0.1,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055440","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CREE",502,502,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055440","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","METHANE",0.011000000000000001,0.01,"0.03",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055440","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","N2O",0,0,"0.01",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055440","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.033800000000000004,0.034,"999.999",0,null,"Y",1.04,null,null,1,"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055440","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.06,0.06,"0.125",0,null,null,1.04,{"$nulls":3},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055440","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.0262,0.026000000000000002,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","CREE",290,290,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NMOG",0,0,"999.999",0,null,null,1.04,{"$nulls":3},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NMOG+NOX",0.007,0.007,"0.125",0,null,null,1.04,{"$nulls":3},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NOX",0.007,0.007,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CREE",290,290,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0,0,"999.999",0,null,null,1.04,{"$nulls":3},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.007,0.007,"0.125",0,null,null,1.04,{"$nulls":3},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055442","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.007,0.007,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",8.25,0.0604,0.0268,45.51,0.0188,0.030100000000000002,"KASX10055447","MFR","11","Cold CO","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","HC-NM",0.27,0.3,"0.3",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",8.25,0.0604,0.0268,45.51,0.0188,0.030100000000000002,"KASX10055447","MFR","11","Cold CO","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","50","CO",1.6,2,"10",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",8.25,0.0604,0.0268,45.51,0.0188,0.030100000000000002,"KASX10055447","MFR","11","Cold CO","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","HC-NM",0.27,0.3,"0.3",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",8.25,0.0604,0.0268,45.51,0.0188,0.030100000000000002,"KASX10055447","MFR","11","Cold CO","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","50","CO",1.6,2,"10",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055462","MFR","51","CA fuel 50 Deg(F) exhaust test","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","50","CO",0.84,0.8,"2.1",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055462","MFR","51","CA fuel 50 Deg(F) exhaust test","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","50","NMOG",0.047400000000000005,0.047,"999.999",0,null,null,1.04,{"$nulls":3},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055462","MFR","51","CA fuel 50 Deg(F) exhaust test","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","50","NMOG+NOX",0.0794,0.08,"0.25",0,null,"Y",1.04,null,null,1,"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055462","MFR","51","CA fuel 50 Deg(F) exhaust test","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","50","NOX",0.032,0.032,"999.999",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055848","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","4","CO",0.7000000000000001,1,"8",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055848","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","4","HC-NM+NOX",0.046,0.05,"0.14",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055849","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","4","CO",0.59,0.6,"2.7",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"aston martin","MASXV05.2AM5","MASXR0160P1Y","Aston Martin","DBS","7002PT7056",0,5.2,4134,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.8100000000000005,0.08070000000000001,0.0245,40.94,0.016900000000000002,0.027100000000000003,"KASX10055849","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","4","HC-NM+NOX",0.03,0,"0.2",0,{"$nulls":6},"Aston Martin Lagonda Ltd: DB11 V12, DBS"]
[2021,"BMW","MBMXJ02.0B4X","MBMXR0130F60","BMW","X4 xDrive30i","LE67191",0,2,4116,5291,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.8,0.17200000000000001,0.02247,61.5,-0.09,0.027049999999999998,"LBMX10058491","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","CO",0.15,0.3,"1.0",0.18,{"$nulls":6},"BMW: 228i Gran Coupe, 228i xDrive Gran Coupe, 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, X1 sDrive28i, X1 xDrive28i, X2 sDrive28i, X2 xDrive28i  Mini: COOPER S CLUBMAN, COOPER S CLUBMAN ALL4, COOPER S COUNTRYMAN, COOPER S COUNTRYMAN ALL4"]
[2021,"BMW","MBMXJ02.0B4X","MBMXR0130F60","BMW","X4 xDrive30i","LE67191",0,2,4116,5291,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.8,0.17200000000000001,0.02247,61.5,-0.09,0.027049999999999998,"LBMX10058491","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG",0.0047,0.009000000000000001,"999.999",4.5000000000000005E-3,null,"Y",1.1,{"$nulls":3},"BMW: 228i Gran Coupe, 228i xDrive Gran Coupe, 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, X1 sDrive28i, X1 xDrive28i, X2 sDrive28i, X2 xDrive28i  Mini: COOPER S CLUBMAN, COOPER S CLUBMAN ALL4, COOPER S COUNTRYMAN, COOPER S COUNTRYMAN ALL4"]
[2021,"BMW","MBMXJ02.0B4X","MBMXR0130F60","BMW","X4 xDrive30i","LE67191",0,2,4116,5291,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.8,0.17200000000000001,0.02247,61.5,-0.09,0.027049999999999998,"LBMX10058491","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG+NOX",0.015700000000000002,0.02,"0.030",null,1,{"$nulls":5},"BMW: 228i Gran Coupe, 228i xDrive Gran Coupe, 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, X1 sDrive28i, X1 xDrive28i, X2 sDrive28i, X2 xDrive28i  Mini: COOPER S CLUBMAN, COOPER S CLUBMAN ALL4, COOPER S COUNTRYMAN, COOPER S COUNTRYMAN ALL4"]
[2021,"BMW","MBMXJ02.0B4X","MBMXR0130F60","BMW","X4 xDrive30i","LE67191",0,2,4116,5291,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.8,0.17200000000000001,0.02247,61.5,-0.09,0.027049999999999998,"LBMX10058491","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NOX",0.011000000000000001,0.011000000000000001,"999.999",0,{"$nulls":6},"BMW: 228i Gran Coupe, 228i xDrive Gran Coupe, 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, X1 sDrive28i, X1 xDrive28i, X2 sDrive28i, X2 xDrive28i  Mini: COOPER S CLUBMAN, COOPER S CLUBMAN ALL4, COOPER S COUNTRYMAN, COOPER S COUNTRYMAN ALL4"]
[2021,"BMW","MBMXJ02.0B4X","MBMXR0130F60","BMW","X4 xDrive30i","LE67191",0,2,4116,5291,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.8,0.17200000000000001,0.02247,61.5,-0.09,0.027049999999999998,"LBMX10058491","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","PM",0.0002,0,"0.003",0,{"$nulls":6},"BMW: 228i Gran Coupe, 228i xDrive Gran Coupe, 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, X1 sDrive28i, X1 xDrive28i, X2 sDrive28i, X2 xDrive28i  Mini: COOPER S CLUBMAN, COOPER S CLUBMAN ALL4, COOPER S COUNTRYMAN, COOPER S COUNTRYMAN ALL4"]
[2021,"BMW","MBMXJ02.0B4X","MBMXR0130F60","BMW","X4 xDrive30i","LE67191",0,2,4116,5291,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.8,0.17200000000000001,0.02247,61.5,-0.09,0.027049999999999998,"LBMX10058491","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","120","CREE",999,999,"999",0.2,{"$nulls":6},"BMW: 228i Gran Coupe, 228i xDrive Gran Coupe, 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, X1 sDrive28i, X1 xDrive28i, X2 sDrive28i, X2 xDrive28i  Mini: COOPER S CLUBMAN, COOPER S CLUBMAN ALL4, COOPER S COUNTRYMAN, COOPER S COUNTRYMAN ALL4"]
[2021,"BMW","MBMXJ02.0B4X","MBMXR0130F60","BMW","X4 xDrive30i","LE67191",0,2,4116,5291,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.8,0.17200000000000001,0.02247,61.5,-0.09,0.027049999999999998,"LBMX10058491","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","120","METHANE",0.0008,1E-3,"0.030",0.0002,{"$nulls":6},"BMW: 228i Gran Coupe, 228i xDrive Gran Coupe, 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, X1 sDrive28i, X1 xDrive28i, X2 sDrive28i, X2 xDrive28i  Mini: COOPER S CLUBMAN, COOPER S CLUBMAN ALL4, COOPER S COUNTRYMAN, COOPER S COUNTRYMAN ALL4"]
[2021,"BMW","MBMXJ02.0B4X","MBMXR0130F60","BMW","X4 xDrive30i","LE67191",0,2,4116,5291,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.8,0.17200000000000001,0.02247,61.5,-0.09,0.027049999999999998,"LBMX10058491","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","120","N2O",0.0004,0,"0.010",0,{"$nulls":6},"BMW: 228i Gran Coupe, 228i xDrive Gran Coupe, 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, X1 sDrive28i, X1 xDrive28i, X2 sDrive28i, X2 xDrive28i  Mini: COOPER S CLUBMAN, COOPER S CLUBMAN ALL4, COOPER S COUNTRYMAN, COOPER S COUNTRYMAN ALL4"]
[2021,"BMW","MBMXJ02.0B4X","MBMXR0130F60","BMW","X4 xDrive30i","LE67191",0,2,4116,5291,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.8,0.17200000000000001,0.02247,61.5,-0.09,0.027049999999999998,"LBMX10058491","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","CO",0.15,0.3,"1.0",0.18,{"$nulls":6},"BMW: 228i Gran Coupe, 228i xDrive Gran Coupe, 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, X1 sDrive28i, X1 xDrive28i, X2 sDrive28i, X2 xDrive28i  Mini: COOPER S CLUBMAN, COOPER S CLUBMAN ALL4, COOPER S COUNTRYMAN, COOPER S COUNTRYMAN ALL4"]
[2021,"BMW","MBMXJ02.0B4X","MBMXR0130F60","BMW","X4 xDrive30i","LE67191",0,2,4116,5291,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.8,0.17200000000000001,0.02247,61.5,-0.09,0.027049999999999998,"LBMX10058491","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","NMOG",0.0047,0.009000000000000001,"999.999",4.5000000000000005E-3,null,"Y",1.1,{"$nulls":3},"BMW: 228i Gran Coupe, 228i xDrive Gran Coupe, 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, X1 sDrive28i, X1 xDrive28i, X2 sDrive28i, X2 xDrive28i  Mini: COOPER S CLUBMAN, COOPER S CLUBMAN ALL4, COOPER S COUNTRYMAN, COOPER S COUNTRYMAN ALL4"]
[2021,"BMW","MBMXJ02.0B4X","MBMXR0130F60","BMW","X4 xDrive30i","LE67191",0,2,4116,5291,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.8,0.17200000000000001,0.02247,61.5,-0.09,0.027049999999999998,"LBMX10058491","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","NMOG+NOX",0.015700000000000002,0.02,"0.030",null,1,{"$nulls":5},"BMW: 228i Gran Coupe, 228i xDrive Gran Coupe, 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, X1 sDrive28i, X1 xDrive28i, X2 sDrive28i, X2 xDrive28i  Mini: COOPER S CLUBMAN, COOPER S CLUBMAN ALL4, COOPER S COUNTRYMAN, COOPER S COUNTRYMAN ALL4"]
[2021,"BMW","MBMXJ02.0B4X","MBMXR0130F60","BMW","X4 xDrive30i","LE67191",0,2,4116,5291,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.8,0.17200000000000001,0.02247,61.5,-0.09,0.027049999999999998,"LBMX10058491","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","NOX",0.011000000000000001,0.011000000000000001,"999.999",0,{"$nulls":6},"BMW: 228i Gran Coupe, 228i xDrive Gran Coupe, 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, X1 sDrive28i, X1 xDrive28i, X2 sDrive28i, X2 xDrive28i  Mini: COOPER S CLUBMAN, COOPER S CLUBMAN ALL4, COOPER S COUNTRYMAN, COOPER S COUNTRYMAN ALL4"]
[2021,"BMW","MBMXJ02.0B4X","MBMXR0150G30","BMW","X4 xDrive30i","LE67191",0,2,4116,5291,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.8,0.17200000000000001,0.02247,61.5,-0.09,0.027049999999999998,"LBMX10058492","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","NMOG+NOX",3.8E-3,0.008,"0.030",null,1,{"$nulls":5},"BMW: 330i, 330i xDrive, 430i Convertible, 430i Coupe, 430i xDrive Coupe, 530i, 530i xDrive, X3 sDrive30i, X3 xDrive30i, X4 xDrive30i, Z4 sDrive30i  TOYOTA: Supra 2.0"]
[2021,"BMW","MBMXJ04.4SM5","MBMXR0150G1X","BMX","X5 M Competition","LB16155",3,4.4,5455,6615,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",7.4,-0.187,0.03247,79.2,-0.369,0.03646,"MBMX10064418","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","N2O",1.2000000000000001E-3,1E-3,"0.010",0.0002,{"$nulls":6},"BMW: M5, M5 Competition, M8 Competition Convertible, M8 Competition Coupe, M8 Competition Gran Coupe, M8 Convertible, M8 Coupe, M8 Gran Coupe"]
[2021,"BMW","MBMXV01.5H60","MBMXR0140G3H","MINI","Mini Cooper SE Countryman ALL4","3F94106",2,1.5,3984,5016,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y",-1.2,0.232,0.019379999999999998,43.300000000000004,0.11900000000000001,0.021349999999999997,"LBMX10059165","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.0123,0.012,"99.999",0,{"$nulls":6},"Mini: MINI COOPER SE COUNTRYMAN ALL4"]
[2021,"FCA US LLC","MCRXD03.65V1","MCRXR0180TP0","RAM","Promaster 3500 Cab Chassis","L1VF16049",0,3.6,8500,9350,8500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",26.51,0.6166,0.06573,63.14,1.0976000000000001,0.06317,"MCRX10064998","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","CA","California + CAA Section 177 states","L3ULEV340","California LEV-III ULEV340","150","NOX",0.0216,0.022000000000000002,"0.200",0,1,"N",{"$nulls":4},"RAM: Promaster 3500 Cab Chassis"]
[2021,"FCA US LLC","MCRXD06.45W3","MCRXF0273TP0","RAM","3500 4X4","L1D280342",0,6.4,10774,14000,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",28.05,0.7385,0.03694,111.53,0.34690000000000004,0.04582,"MCRX10066461","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B400","Federal Tier 3 HD Class 3 Bin 400","150","NMOG",0.0056,0.006,"999.999",0,1,"N",{"$nulls":4},"RAM: 3500 Cab Chassis 4X2, 3500 Cab Chassis 4X4"]
[2021,"FCA US LLC","MCRXT02.05P4","MCRXR0136PP0","Jeep","Wrangler 4dr 4X4","V0JLJ1158",0,2,4311,5400,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",23.86,-0.11470000000000001,0.04053,60.07,-0.1565,0.044039999999999996,"MCRX10065356","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",2.9000000000000002E-3,0.014,"999.999",0.0112,1,"N",{"$nulls":4},"Jeep: Wrangler 2dr 4X4"]
[2021,"FCA US LLC","MCRXT03.25P0","MCRXR0118PP0","Jeep","Cherokee Trailhawk 4X4","L9KLJ3153",0,3.2,4128,5500,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",18.34,0.1922,0.02464,38.47,0.6612,0.022879999999999998,"KCRX10051356","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.0285,0.028,"0.070",0,1,"N",{"$nulls":4},"Jeep: Cherokee 4X4, Cherokee 4x4 Active Drive II, Cherokee FWD, Cherokee Trailhawk 4X4"]
[2021,"FCA US LLC","MCRXT03.65P5","MCRXR0140RP0","Dodge","Durango AWD","L0WDE8891",1,3.6,5035,6500,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",32.03,-0.3447,0.034159999999999996,59.300000000000004,-0.2675,0.03514,"MCRX10063764","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","CREE",999,999,"999",0,1,"N",{"$nulls":4},"Chrysler: Grand Caravan, Pacifica, Pacifica AWD, Voyager"]
[2021,"FCA US LLC","MCRXT05.75P1","MCRXR0183RP1","RAM","1500 4X4","V9DT64709",1,5.7,5607,7100,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y",17.91,0.5954,0.02776,62.45,0.07050000000000001,0.03704,"MCRX10064804","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","N2O",0,0,"0.010",0.0005,1,"N",{"$nulls":4},"RAM: 1500 4X2, 1500 4X4"]
[2021,"FCA US LLC","MCRXT05.75P2","MCRXR0204RP0","RAM","1500 Classic 4X4","V9DS69205",1,5.7,5433,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",38.42,0.2164,0.03479,83,-0.1404,0.04131,"MCRX10065982","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.44,1.2,"999.9",0.81,1,"N",{"$nulls":4},"Jeep: Grand Cherokee 4X4"]
[2021,"FCA US LLC","MCRXV05.75P3","MCRXR0141PK0","Chrysler","300","L0LXC5440",1,5.7,4375,5350,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",14.530000000000001,0.2492,0.01962,47.660000000000004,0.19190000000000002,0.020989999999999998,"MCRX10066158","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","METHANE",0.018600000000000002,0.019,"0.030",0.0007,1,"N",{"$nulls":4},"Dodge: Challenger, Charger"]
[2021,"Ferrari","MFEXV03.9HYB","MFEXR111508H","Ferrari","SF90 Stradale Coupe","236237",2,3.9,3979,4597,4250,"A","All Wheel Drive","AM","Automated Manual",null,8,"N","N",null,null,"N",-14.23,-1.2650000000000001,0.047,55.348000000000006,0.463,0.024,"MFEX10063877","MFR","90","US06","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.9390000000000001,1.08,"999.99",0.13870000000000002,{"$nulls":6},"Ferrari North America, Inc.: SF90 Stradale Coupe"]
[2021,"FOMOCO","MFMXD03.57BG","MFMXR0185NDJ","Ford","T350 Transit","LTH1-3.5-J-430",0,3.5,6981,10360,8500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",13.68,0.046200000000000005,0.048479999999999995,49.53,0.3642,0.048229999999999995,"LFMX10061341","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","M7","MDV7 (Cal. LEV 2/3 MDV GVW 10001-14000)","CA","California + CAA Section 177 states","L3ULEV400","California LEV-III ULEV400","150","NOX",0.0148,0.021,"999.999",0.006500000000000001,{"$nulls":6},"Ford: TRANSIT T350 VAN 2WD FFV, TRANSIT T350 WAGON 2WD FFV"]
[2021,"FOMOCO","MFMXD06.27BC","MFMXR0250NHJ","Ford","F350 4x4","LFE1-6.2-J-578",2,6.2,10442,14000,12000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",39.300000000000004,-0.4217,0.08932999999999999,81.18,0.2046,0.08335,"LFMX10063976","MFR","21","Federal fuel 2-day exhaust (w/can load)","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","M7","MDV7 (Cal. LEV 2/3 MDV GVW 10001-14000)","CA","California + CAA Section 177 states","L3ULEV270","California LEV-III ULEV270","150","NOX",0.0284,0.14400000000000002,"999.999",0.1153,{"$nulls":6},"Ford: F350 PICKUP 2WD FFV, F350 PICKUP 4WD FFV"]
[2021,"FOMOCO","MFMXD07.373K","MFMXR0360NHJ","Ford","F350 4x4","LFE1-7.3-J-591",0,7.3,7449,14000,10500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",20.62,0.7983399999999999,0.05071,71.54,1.0966,0.04824,"LFMX10060379","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.013300000000000001,0.10400000000000001,"0.270",0,{"$nulls":6},"Ford: F350 2WD, F350 4WD"]
[2021,"FOMOCO","MFMXT02.33MC","MFMXR0135NDV","Ford","Ranger - Chassis Cab","KFG1-2.3-H-366",0,2.3000000000000003,5025,6050,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",15.23,0.03904,0.053869999999999994,30.46,0.1952,0.053869999999999994,"KFMX10055155","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.014,0.034,"9.999",0.02,{"$nulls":6},"Ford: RANGER 2WD INCOMPLETE"]
[2021,"FOMOCO","MFMXT02.53CE","MFMXR0135LLN","Lincoln","Corsair PHEV","LTF1-2.5-H-558",0,2.5,4517,5480,4750,"A","All Wheel Drive","CVT","Continuously Variable",null,1,"N","N",null,null,"Y",-13.88,0.2577,0.022000000000000002,36.86,0.4329,0.02367,"MFMX10066376","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","NMOG",0.0098,0.016,"9.999",0.006,null,"Y",1.03,{"$nulls":3},"Lincoln: CORSAIR AWD PHEV"]
[2021,"FOMOCO","MFMXT03.33U3","MFMXR0170NDG","Ford","Explorer","LTW1-3.3-L-477",1,3.3000000000000003,4595,5830,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",39.660000000000004,0.3038,0.028300000000000002,56.02,0.34940000000000004,0.029759999999999998,"LFMX10059014","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.012700000000000001,0.02,"9.999",0.0074,null,"Y",1.1,{"$nulls":3},"Ford: INTERCEPTOR UTILITY AWD FFV"]
[2021,"FOMOCO","MFMXT03.55HM","MFMXR0215GDH","Ford","T150 Transit Van MDPV","LTH1-3.5-J-448",0,3.5,6276,8550,6500,"P","Part-time 4-Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",39.410000000000004,0.10300000000000001,0.046759999999999996,64.27,0.46950000000000003,0.045649999999999996,"LFMX10060235","MFR","3","HWFE","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","T3B160","Federal Tier 3 Bin 160","150","OPT-CREE",369,371,"999",2,{"$nulls":6},"Ford: TRANSIT T150 WAGON 2WD FFV, TRANSIT T150 WAGON 4WD FFV"]
[2021,"FOMOCO","MFMXT05.03DP","MFMXR0260NDV","Ford","F150 Super Cab 4X4","MFD1-5.0-J-941",0,5,5119,7150,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",33.07,0.1236,0.04031,50.93,0.1598,0.04263,"MFMX10065941","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","METHANE",0.007200000000000001,0.014,"0.040",6.8000000000000005E-3,{"$nulls":6},"Ford: F150 PICKUP 2WD FFV, F150 PICKUP 4WD FFV"]
[2021,"GM","MGMXD06.6377","MGMXR021260A","CHEVROLET","SILVERADO 2500 HD 4WD","66CRMNT182",0,6.6000000000000005,6572,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",27.14,0.39790000000000003,0.04111,66.01,1.2610000000000001,0.037700000000000004,"MGMX10063910","MFR","52","Fed. fuel 50 F exh.","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","CA","California + CAA Section 177 states","L3ULEV200","California LEV-III ULEV200","4","NMOG",0.1173,0.117,"99.999",null,null,"N",{"$nulls":3},1,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD"]
[2021,"GM","MGMXD06.6398","MGMXF016360D","CHEVROLET","SILVERADO 4WD CAB CHAS","66CRLNT042",1,6.6000000000000005,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",52.07,0.3572,0.12171,85.15,0.9866,0.11964999999999999,"LGMX10057437","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NMOG+NOX",0.1439,0.14400000000000002,"0.270",null,1,"N",{"$nulls":3},1,"Chevrolet: SILVERADO 3500 HD 2WD CAB CHAS, SILVERADO 3500 HD 4WD CAB CHAS  GMC: SIERRA 3500 HD 2WD CAB CHAS, SIERRA 3500 HD 4WD CAB CHAS"]
[2021,"GM","MGMXT02.0550","MGMXR015740B","CADILLAC","XT5 AWD","206LNS5224",4,2,5350,6001,5500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,9,"Y","N",null,null,"N",22.64,0.1396,0.031229999999999997,40.35,0.4394,0.030129999999999997,"MGMX10065695","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV50","California LEV-III ULEV50","150","NMOG+NOX",0.004200000000000001,0.004,"99.999",null,1,"N",{"$nulls":3},1,"Cadillac: XT5 HEARSE AWD, XT5 HEARSE FWD, XT5 LIMO AWD, XT5 LIMO FWD"]
[2021,"GM","MGMXT03.0353",null,"CADILLAC","ESCALADE 4WD","30KLMN1832",0,3,6310,7700,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N",-18.01,0.8604,0.024249999999999997,41,0.8659,0.030729999999999997,"MGMX10064975","MFR","90","US06","19","Federal Cert Diesel 7-15 PPM Sulfur","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",1.01,1,"99.9",null,null,"N",null,0,0,1,"Cadillac: ESCALADE 2WD, ESCALADE 4WD  Chevrolet: SUBURBAN 2WD, SUBURBAN 4WD, TAHOE 2WD, TAHOE 4WD  GMC: YUKON 2WD, YUKON 4WD, YUKON XL 2WD, YUKON XL 4WD"]
[2021,"GM","MGMXT05.3388","MGMXR017350D","GMC","YUKON XL 4WD","53KSMN1691",0,5.3,6097,7700,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N",-17.87,0.755,0.028159999999999998,42.6,0.7544000000000001,0.03388,"MGMX10062244","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","4","NMOG",0.0879,0.08800000000000001,"99.999",null,null,"N",{"$nulls":3},1,"Chevrolet: TAHOE 2WD, TAHOE 4WD  GMC: YUKON 2WD, YUKON 4WD"]
[2021,"GM","MGMXV01.4001","MGMXR011230A","BUICK","ENCORE AWD","145SV508DA",1,1.4000000000000001,3314,4409,3625,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",11.67,0.29150000000000004,0.022359999999999998,32.69,0.3044,0.024249999999999997,"MGMX10066212","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NOX",2.3E-3,2E-3,"99.999",null,null,"N",{"$nulls":3},1,"Buick: ENCORE AWD, ENCORE FWD  Chevrolet: TRAX AWD, TRAX FWD"]
[2021,"GM","MGMXV02.7105","MGMXR01103AA","CADILLAC","CT4 V AWD","276LDN4836",3,2.7,3793,null,4000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",7.25,0.8185,0.01373,46.95,0.20070000000000002,0.023,"MGMX10064775","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B50","Federal Tier 3 Bin 50","120","N2O",0.0002,0,"0.010",null,null,"N",{"$nulls":3},1,"Cadillac: CT4, CT4 AWD, CT4 V, CT4 V AWD"]
[2021,"Honda","MHNXT01.5YLC","MHNXR01221SA","HONDA","CR-V 1.5L TC","ELSJ1C",0,1.5,3644,null,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",14.8,-0.1096,0.025929999999999998,47.77,-0.3769,0.03039,"LHNX91004387","EPA","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV50","California LEV-III ULEV50","150","NMOG+NOX",1.8000000000000002E-3,0.008,"0.050",null,1,"Y",1.03,{"$nulls":3},"Honda: CR-V AWD, CR-V FWD"]
[2021,"Honda","MHNXV01.5DFB","MHNXR0116VSA","HONDA","Clarity Plug-in Hybrid","DJWJ1C",0,1.5,4065,null,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y",8.63,0.3165,0.015519999999999999,26.78,0.3123,0.01713,"JHNX10048911","MFR","81","Charge Depleting UDDS","62","Electricity","C","LDV","LDV/Passenger Car","FA","Federal","T3B20","Federal Tier 3 Bin 20","120","CREE",136,146,"999",9.5,null,"N",{"$nulls":4},"Honda: Clarity"]
[2021,"Honda","MHNXV03.5NBC","MHNXR0150VSA","HONDA","PILOT 4WD 9AT","EGLV1A",4,3.5,4361,5842,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,9,"Y","N",null,null,"N",6.33,0.2076,0.02651,25.93,0.4932,0.025519999999999998,"GHNX10035977","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","120","CREE",251,251,"999",0.11,null,"N",{"$nulls":4},"Honda: PASSPORT AWD, PASSPORT FWD, PILOT AWD, PILOT FWD"]
[2021,"Hyundai","MHYXV01.6BC5","MHYXR0110BCE","HYUNDAI","VELOSTER","JS-U0G6TD717F",0,1.6,2976,3858,3250,"F","2-Wheel Drive, Front","AM","Automated Manual",null,7,"N","N",null,null,"N",10.104000000000001,0.11020999999999999,0.019711,27.858,0.23795,0.019461,"LHYX10055930","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.0204,0.046,"0.070",0,null,"N",{"$nulls":4},"HYUNDAI MOTOR COMPANY: Veloster"]
[2021,"Hyundai","MHYXV01.6KC5","MHYXR0127KCE","HYUNDAI","Kona","OS8R6HU07AC",0,1.6,3256,4255,3500,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N",7.691000000000001,0.21142999999999998,0.02328,38.256,0.47281999999999996,0.023186,"JHYX10049639","MFR","11","Cold CO","26","Cold CO Regular (Tier 2)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","50","CO",0.35000000000000003,0.4,"10.0",0.06,{"$nulls":6},"HYUNDAI MOTOR COMPANY: Kona AWD, Kona FWD"]
[2021,"Hyundai","MHYXV01.6SB5","MHYXR0120SBG","HYUNDAI","Venue","QX-U0G6MC114F",0,1.6,2737,3770,3000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N",2.165,0.34354,0.020572999999999998,27.946,-0.035019999999999996,0.025287999999999998,"LHYX91004330","EPA","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",8.6E-3,0.016,"99.999",0.007500000000000001,null,"Y",1.03,{"$nulls":3},"HYUNDAI MOTOR COMPANY: Venue"]
[2021,"Hyundai","MHYXV02.4LH3","MHYXR0133LHG","Hyundai","Tucson","TL9F4AU05AC",0,2.4,3492,4718,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",8.735000000000001,0.16016999999999998,0.025900000000000003,28.845000000000002,0.40079,0.024343,"KHYX10053752","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","NMOG",0,2E-3,"99.999",1.9E-3,null,"Y",1.03,{"$nulls":3},"HYUNDAI MOTOR COMPANY: Tucson FWD"]
[2021,"Hyundai","MHYXV03.3GK6","MHYXR0140GKE","Genesis","G70","IK8L3HU07AC",0,3.3000000000000003,3913,4993,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",24.012,0.38855999999999996,0.014718,45.499,0.9397099999999999,0.010969,"KHYX10050222","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","4","CO",0.18,0.2,"2.1",0,{"$nulls":6},"GENESIS: G70 AWD, G70 RWD"]
[2021,"Jaguar Land Rover L","MJLXJ05.0FSM","MJLXR0140P1Z","Jaguar","F-PACE SVR","4AKTT210",0,5,4645,5620,5000,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-19.064,0.22033,0.02515,52.550000000000004,0.09655999999999999,0.02822,"KJLX10055077","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.0281,0.045000000000000005,"999.999",0.016900000000000002,null,"N",{"$nulls":4},"Jaguar: F-PACE SVR  Land Rover: Range Rover Velar"]
[2021,"Jaguar Land Rover L","MJLXT05.0FSN","MJLXR0175001","Land Rover","Range Rover LWB","LG366679",0,5,6028,7055,6500,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",51.186,0.10990000000000001,0.031400000000000004,61.42,0.11570000000000001,0.03279,"JJLX10052063","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","HCHO",3.0000000000000003E-4,1E-3,"0.004",3.0000000000000003E-4,null,"N",{"$nulls":4},"Land Rover: Range Rover, Range Rover LWB, Range Rover LWB SVA, Range Rover SVA, Range Rover Sport, Range Rover Sport SVR"]
[2021,"Kia","MKMXT02.0NE5","MKMXR0122NEG","Kia","Seltos","SP2U0N0MC016A",0,2,3185,4167,3500,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,8,"Y","N",null,null,"N",7.4270000000000005,0.22229,0.023851999999999998,34.717,-0.02225,0.027496,"MKMX10059981","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","PM",2E-3,2E-3,"0.006",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Seltos AWD, Seltos FWD"]
[2021,"Kia","MKMXV01.6AB6","MKMXR0110ABG","KIA","Rio","SC9R6GU07AC",2,1.6,2731,3616,3000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N",4.541,0.3058,0.016834,33.802,-0.05662,0.021662999999999998,"LKMX10055945","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.0064,0.032,"0.125",0,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Rio"]
[2021,"Kia","MKMXV02.0BE3","MKMXR0114BEG","Kia","Soul","SK0N0GU05AC",0,2,2912,4023,3250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",7.643000000000001,0.050100000000000006,0.024884,37.001000000000005,-0.09508,0.027755,"LKMX10056588","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NOX",0.0049,0.008,"99.999",3.4000000000000002E-3,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Soul, Soul Eco dynamics"]
[2021,"Landi Renzo","MLDRD06.2C10","MLDRF0000C10","FORD","F250 PICKUP 4x4","1FT7X2A6XHEB69563",1,6.2,8921,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",50.9,0.6301,0.1245,87.81,0.8608,0.12465999999999999,"HLDR10053267","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV3B200","Federal Tier 3 HD Class 3 Bin 200","150","NOX",0.152,0.152,"999.999",null,null,"N",{"$nulls":4},"Landi Renzo USA: F250 2WD BED DELETE, F250 4WD BED DELETE, F250 PICKUP 2WD, F250 PICKUP 4WD, F350 2WD BED DELETE, F350 4WD BED DELETE, F350 INCOMPLETE 2WD, F350 INCOMPLETE 4WD, F350 PICKUP 2WD, F350 PICKUP 4WD"]
[2021,"MAZDA","MTKXV01.5FNM","MTKXR0107GBK","MAZDA","Mazda2","0EBP5VS1-002",0,1.5,2414,3360,2750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",7.673,0.09566,0.01705,20.25,0.20970999999999998,0.017287999999999998,"LTKX10057454","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.0057,0.063,"0.125",0,null,"Y",1.03,{"$nulls":3},"MAZDA: MAZDA2"]
[2021,"MAZDA","MTKXV02.5CDA","MTKXR0098GDP","MAZDA","CX-5","8EBPYUDG1-002",2,2.5,3693,4669,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",12.773000000000001,0.09493,0.024295,36.338,0.11446999999999999,0.025809,"JTKX91003671","EPA","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG",0,0.003,"99.999",2.6000000000000003E-3,null,"Y",{"$nulls":4},"MAZDA: CX-30 2WD, CX-30 4WD, MAZDA3 4-Door 2WD, MAZDA3 4-Door 4WD, MAZDA3 5-Door 2WD, MAZDA3 5-Door 4WD"]
[2021,"Mercedes-Benz","MMBXT02.0U3A","MMBXR0170LNF","Mercedes-Benz","GLE 350 4MATIC","V167E20DETC-Z2138-1",0,1.991,4874,6210,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",36.711,0.36067,0.024430999999999998,61.59,0.3617,0.02613,"MMBX10065008","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","HCHO",3.0000000000000003E-4,1E-3,"0.004",0.0004,{"$nulls":6},"Mercedes-Benz: GLE 350, GLE 350 4MATIC"]
[2021,"Mercedes-Benz","MMBXT04.0HY1","MMBXR0170LNC","Mercedes-Benz","GLS 580 4MATIC","X167E40DETC-Z2030",2,3.982,5828,7480,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"Y",34.913000000000004,0.27576,0.029736,63.84,0.3617,0.03061,"MMBX10065120","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","METHANE",0.004200000000000001,0.008,"0.030",0.004,{"$nulls":6},"Mercedes-Benz: GLE 580 4MATIC, GLS 580 4MATIC"]
[2021,"Mercedes-Benz","MMBXV02.0U3C","MMBXR0095LNA","Mercedes-Benz","CLA 250 4MATIC","C118E20DETC-Z2036-1",2,1.991,3549,4597,3875,"F","2-Wheel Drive, Front","AM","Automated Manual",null,7,"Y","N",null,null,"N",20.253,0.20770999999999998,0.015564,34.84,0.4449,0.015359999999999999,"MMBX10064461","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","CREE",279,280,"999",0.505,{"$nulls":6},"Mercedes-Benz: A 220, A 220 4MATIC, A 250 4MATIC, CLA 250, CLA 250 4MATIC"]
[2021,"Mitsubishi Motors Co","MMTXT02.4H3M","MMTXR0148A2L","MITSUBISHI","Outlander PHEV","EB21-RH61",0,2.36,4365,5269,4750,"A","All Wheel Drive","A","Automatic",null,1,"Y","N",null,null,"Y",-7.12,0.19090000000000001,0.021429999999999998,37.795,0.38466999999999996,0.022321999999999998,"MMTX10061486","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","HCHO",0.00014,0.0002,"0.0040",1E-4,null,"N",{"$nulls":4},"Mitsubishi Motors Corporation: Outlander PHEV"]
[2021,"Nissan","MNSXT05.6N9B","MNSXR0201PGA","INFINITI","QX80 4WD SENSORY","TWE530",0,5.6000000000000005,6081,7412,6500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N",14.200000000000001,0.2822,0.03076,39.410000000000004,0.9573,0.02614,"MNSX10062718","MFR","35","California fuel 3-day exhaust","46","CARB LEV3 E10 Regular Gasoline","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.0229,0.027,"0.125",0,{"$nulls":6},"INFINITI: QX80 4WD  NISSAN: ARMADA 4WD"]
[2021,"Nissan","MNSXV03.5P7C","MNSXR0149PCA","NISSAN","MURANO AWD SL","JJC526",0,3.5,4127,5280,4500,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N",9.78,0.1693,0.02335,33.28,0.1383,0.025089999999999998,"MNSX10064520","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.0409,0.042,"999.999",0.0008,{"$nulls":6},"NISSAN: MURANO AWD, MURANO FWD"]
[2021,"Porsche","MPRXV02.5B82","MPRXR0130R82","Porsche","Cayman S","ECFE-982S-PDK-20",0,2.5,3210,3737,3500,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N",24.212,0.32922999999999997,0.013973999999999999,40.241,0.62591,0.011878,"LPRX10064237","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3LEV160","California LEV-III LEV160","150","PM",1E-3,1E-3,".003",0,{"$nulls":6},"Porsche: 718 Boxster, 718 Boxster S, 718 Boxster T, 718 Cayman, 718 Cayman S, 718 Cayman T"]
[2021,"SC Auto Sports, LLC","MSCAV0.00MDP",null,"Kandi","K23","LA003004",0,99.99000000000001,2954,3781,3375,"F","2-Wheel Drive, Front","A","Automatic",null,1,"N","N",null,null,"N",12.58,0.4157,0.016139999999999998,31.970000000000002,0.48160000000000003,0.016714,"MSCA10067716","MFR","84","Charge Depleting Highway","62","Electricity","C","LDV","LDV/Passenger Car","FA","Federal","T3B0","Federal Tier 3 Bin 0","150","PM",0,0,"0",0,{"$nulls":6},"Transportation Research Center: Kandi K23"]
[2021,"Subaru","MFJXJ02.5BUY","MFJXR01155AD","SUBARU","OUTBACK AWD","LBE-YB16",0,2.5,3757,4850,4000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,8,"Y","N",null,null,"N",11.200000000000001,0.1345,0.02257,33.49,0.11910000000000001,0.023739999999999997,"LFJX10056998","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","PM",1E-4,0,"0.006",1E-4,{"$nulls":6},"Subaru: IMPREZA 4-Door, IMPREZA 4-Door SPORT, IMPREZA 5-Door, IMPREZA 5-Door SPORT"]
[2021,"Toyota","MTYXT02.5P3M","MTYXR0130A82","LEXUS","NX 300h AWD","15-AZ1H",0,2.494,4180,5335,4500,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y",24.423000000000002,-0.19402,0.028308,39.19,0.18162,0.025845999999999997,"FTYX10029503","MFR","35","California fuel 3-day exhaust","46","CARB LEV3 E10 Regular Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","N2O",0.0004,2E-3,"0.010",1.9E-3,null,"N",{"$nulls":4},"LEXUS: NX 300h AWD"]
[2021,"Volkswagen Group of","MVGAJ02.0A3P","MVGAR0145ACW","AUDI","Q5 55 TFSIe","MA3P-Q5-526",1,1.984,4773,5941,5250,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"Y",-0.135,0.21925,0.021369,59.012,-0.0651,0.026143,"MVGA10067122","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","CO",0.1,0.2,"1.0",0.05,{"$nulls":6},"Audi: Q5"]
[2021,"Volkswagen Group of","MVGAJ02.0A7G","MVGAR0140ACN","AUDI","Q5","MA7G-Q5",0,1.984,4200,null,4500,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"Y",-1.641,0.52352,0.017554999999999998,43.995000000000005,0.5390699999999999,0.019854999999999998,"MVGA10065411","MFR","95","SC03","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.0118,0.015000000000000001,"99.999",3.4000000000000002E-3,{"$nulls":6},"Audi: Q5, Q5 Sportback"]
[2021,"Volkswagen Group of","MVGAT02.0VAA","MVGAR0135VCS","VOLKSWAGEN","Atlas Cross Sport AWD","LC200114",0,2,4348,5666,5000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-6.412,0.67652,0.024100999999999997,43.231,0.62215,0.027004999999999998,"LVGA10061255","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.056900000000000006,0.07200000000000001,"99.999",0.01504,{"$nulls":6},"Volkswagen: Atlas, Atlas 4Motion 2.0L, Atlas Cross Sport, Atlas Cross Sport 4Motion"]
[2021,"Volkswagen Group of","MVGAT06.0EAR","MVGAR0155ECR","BENTLEY","Bentayga W12","BY636/2 28877",0,5.95,5549,null,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",6.931,0.36306,0.025463,62.272000000000006,0.21739,0.029566,"MVGA10067467","MFR","3","HWFE","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CREE",999,999,"999",0.49,{"$nulls":6},"Bentley: Bentayga"]
[2021,"Volkswagen Group of","MVGAV02.0AAB","MVGAR0110ACA","VOLKSWAGEN","Audi S3","AU371090047",0,1.984,3549,null,3875,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N",14.927000000000001,-0.0032,0.019438999999999998,52.403000000000006,0.17723999999999998,0.019846,"KVGA10056282","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.006500000000000001,0.014,"0.125",null,1,{"$nulls":5},"Audi: S3, TTS Coupe"]
[2021,"Volkswagen Group of","MVGAV06.5LDR","MVGAR0130NAJ","LAMBORGHINI","Aventador SVJ","LB73X_SVJ_8509",0,6.498,4123,null,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,7,"N","N",null,null,"N",1.476,0.42651999999999995,0.01869,57.326,0.7608499999999999,0.019330999999999997,"MVGA10066394","MFR","95","SC03","47","CARB LEV3 E10 Premium Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3LEV160","California LEV-III LEV160","150","PM",0.003,0.003,"99.999",0.00013,{"$nulls":6},"Lamborghini: Aventador Coupe, Aventador Roadster, Aventador S Coupe, Aventador S Roadster"]
[2021,"Volvo","MVVXJ02.0U70","MVVXR0142E61","Volvo","XC90 T5 AWD","201807",0,1.969,4682,6060,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.5,0.42700000000000005,0.0247,40.756,0.36990999999999996,0.026049,"JVVX10046755","MFR","90","US06","47","CARB LEV3 E10 Premium Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.004,0.004,"999.999",0,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: XC40 FWD"]
[2021,"Westport ","MBAFD06.2CNG","MBAFR0360NHJ","Ford","F250","HEB21979",0,6.2,10000,null,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",48.65,0.9143,0.07443,88.41,1.1380000000000001,0.0758,"HBAF10046373","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.016,0.07,"999.99",0.05,1,{"$nulls":5},"BAF_Bifuel: Ford F250/350, Ford F350"]
[2020,"Blossman Services, ","LBLMD06.0395","LBLMF0176860","Chevrolet","G3500 Express 2WD Cutaway CH","1GC1KVEG3HF108414",0,6,6851,9500,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",75.7,-0.164,0.09437,98.9,0.8639,0.08803,"JBLM10052437","MFR","21","Federal fuel 2-day exhaust (w/can load)","42","LPG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B250","Federal Tier 3 HD Class 2b Bin 250","150","NOX",0.053000000000000005,0.1,"999.99",0.05,{"$nulls":6},"Blossman: G3500 EXPRESS 2WD CUTAWAY CH, G3500 SAVANA 2WD CUTAWAY CH"]
[2020,"BMW","LBMXJ02.0H30","LBMXR0140G3H","BMW","X3 xDrive30e","LG69397",0,2,4586,5776,5000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y",26.3,-0.217,0.025419999999999998,70.8,-0.255,0.02775,"LBMX10061779","MFR","84","Charge Depleting Highway","62","Electricity","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NOX",2E-3,0.008,"99.999",0.0057,{"$nulls":6},"BMW: 530e, 530e xDrive, X3 xDrive30e"]
[2020,"BMW","LBMXJ04.4SM5","LBMXR0180G05","BMX","X5 M Competition","LB16155",0,4.4,5425,6615,5500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-4.2,-0.153,0.03361,70.8,-0.276,0.036359999999999996,"LBMX10060886","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",6.0000000000000006E-4,0.008,"99.999",0.0074,null,"Y",1.03,{"$nulls":3},"BMW: X5 M, X5 M Competition, X6 M, X6 M Competition"]
[2020,"BMW","LBMXV02.0B46","LBMXR0100F5X","Mini","JOHN COOPER WORKS CONVERTIBLE","3G57569",0,2,3143,3946,3500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",19.1,-0.12300000000000001,0.02394,45.800000000000004,-0.066,0.0238,"LBMX10058372","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","50","CO",0.47000000000000003,0.5,"10.0",0,{"$nulls":6},"Mini: COOPER S CONVERTIBLE, COOPER S HARDTOP 2 DOOR, COOPER S HARDTOP 4 DOOR, JOHN COOPER WORKS CONVERTIBLE, JOHN COOPER WORKS HARDTOP"]
[2020,"FCA US LLC","LCRXD03.65V1","LCRXR0180TP0","RAM","Promaster 3500 Cab Chassis","L0VF19538",0,3.6,8500,9350,8500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",20.95,0.6805,0.06568,63.04,1.0973,0.06317,"LCRX10060611","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B340","Federal Tier 3 HD Class 2b Transitional Bin 340","150","NOX",0.011300000000000001,0.011000000000000001,"999.999",0,1,"N",{"$nulls":4},"RAM: Promaster 3500 Cab Chassis"]
[2020,"FCA US LLC","LCRXD06.45W3","LCRXF0353TC0","RAM","3500 4X4","L9D289765",0,6.4,10750,14000,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",48.84,0.0766,0.04519,125.8,-0.15560000000000002,0.052309999999999995,"KCRX10056913","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B570","Federal Tier 3 HD Class 3 Transitional Bin 570","150","NMOG+NOX",0.061500000000000006,0.062,"0.570",0,1,"N",{"$nulls":4},"RAM: 3500 Cab Chassis 4X2, 3500 Cab Chassis 4X4"]
[2020,"FCA US LLC","LCRXJ02.95P0","LCRXR0108PP0","Alfa Romeo","Stelvio AWD","L0GUG6106",0,2.9,4386,5423,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",33.13,-0.2827,0.02889,56.620000000000005,-0.1293,0.02932,"LCRX10060672","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",6.8000000000000005E-3,0.007,"999.999",0,1,"N",null,0,0,null,"ALFA ROMEO: Giulia"]
[2020,"FCA US LLC","LCRXT02.45P1","LCRXR0106PP0","Jeep","Cherokee 4X4","V9KLJ1721",0,2.4,3908,5500,4250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",2.75,0.1461,0.025529999999999997,26.77,0.403,0.02486,"KCRX10054211","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV50","California LEV-III ULEV50","150","PM",0.0007,1E-3,"0.003",0.0005,1,"N",{"$nulls":4},"Jeep: Compass 4X2"]
[2020,"FCA US LLC","LCRXT03.65P0","LCRXR0166PP0","Dodge","Durango AWD","L8WKJ3259",0,3.6,5072,6500,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",31,-0.2667,0.03252,61.14,-0.2675,0.03514,"JCRX10048594","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","PM",9.0000000000000008E-4,1E-3,"0.006",0,1,"N",{"$nulls":4},"Jeep: Gladiator Pickup 4x4"]
[2020,"FCA US LLC","LCRXT03.65P5","LCRXR0140RP0","Dodge","Durango AWD","L0WDE8891",0,3.6,5041,6500,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",32.03,-0.3447,0.034159999999999996,59.300000000000004,-0.2675,0.03514,"LCRX10059710","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","PM",0,0,"0.01",0,1,"N",{"$nulls":4},"Chrysler: Pacifica AWD"]
[2020,"FCA US LLC","LCRXT05.75P1","LCRXR0183RP1","RAM","1500 4X4","L9DT66806",0,5.7,5509,7100,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y",23.17,0.37720000000000004,0.031059999999999997,62.45,0.07050000000000001,0.03704,"KCRX91003843","EPA","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","METHANE",0.0085,0.014,"0.030",5.3E-3,1,"N",null,0,0,null,"RAM: 1500 4X2, 1500 4X4"]
[2020,"FCA US LLC","LCRXT05.75P2","LCRXR0225RP1","RAM","1500 Classic 4X4","V9DS69205",0,5.7,5354,6900,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",39.050000000000004,0.215,0.034319999999999996,82.31,-0.1424,0.04142,"LCRX10062174","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.0245,0.026000000000000002,"999.999",0.0016,1,"N",null,0,0,null,"RAM: 1500 Classic 4X2, 1500 Classic 4X4"]
[2020,"FCA US LLC","LCRXT05.75P8","LCRXR0183RP1","RAM","1500 4X4","V9DT64709",0,5.7,5553,7100,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y",20.37,0.6702,0.02669,62.45,0.07050000000000001,0.03704,"LCRX10062002","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.036000000000000004,0.044000000000000004,"0.125",0,1,"N",{"$nulls":4},"RAM: 1500 4X2, 1500 4X4"]
[2020,"FCA US LLC","LCRXV05.75P4","LCRXR0141PK0","Dodge","Challenger","L0LAD1176",0,5.7,4194,5300,4500,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N",21.35,-0.20980000000000001,0.02601,45.82,0.15030000000000002,0.02436,"LCRX10062233","MFR","25","California fuel 2-day exhaust (w/can load)","47","CARB LEV3 E10 Premium Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B160","Federal Tier 3 Bin 160","150","NMOG",0.040600000000000004,0.043000000000000003,"999.999",2.1000000000000003E-3,1,"N",null,0,0,null,"Dodge: Challenger"]
[2020,"FOMOCO","LFMXD03.56BG","LFMXF0185NDJ","Ford","T350 Transit Regular Cab","LTH1-3.5-447",0,3.5,7550,9950,8500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",26.71,0.1965,0.07628,51.27,0.38420000000000004,0.07708999999999999,"LFMX10061374","MFR","21","Federal fuel 2-day exhaust (w/can load)","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","CA","California + CAA Section 177 states","L3ULEV200","California LEV-III ULEV200","150","NMOG",0.055600000000000004,0.096,"999.999",0.0409,{"$nulls":6},"Ford: TRANSIT T250 CHASSIS CAB 2WD FFV, TRANSIT T250 CHASSIS CAB 4WD FFV, TRANSIT T250 CUTAWAY 2WD FFV, TRANSIT T250 CUTAWAY 4WD FFV, TRANSIT T350 CHASSIS CAB 2WD FFV, TRANSIT T350 CHASSIS CAB 4WD FFV, TRANSIT T350 CUTAWAY 2WD FFV, TRANSIT T350 CUTAWAY 4WD FFV"]
[2020,"FOMOCO","LFMXD03.56BZ","LFMXR0215GDJ","Ford","T150 Transit Van <10K","LTH1-3.5-J-435",1,3.5,8124,9950,9000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",38.660000000000004,-0.02191,0.08008,66.02,0.34290000000000004,0.07930000000000001,"LFMX10061168","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","CA","California + CAA Section 177 states","L3ULEV200","California LEV-III ULEV200","4","NOX",0.045700000000000005,0.046,"999.999",{"$nulls":7},"Ford: TRANSIT T150 VAN 2WD, TRANSIT T150 VAN 4WD, TRANSIT T250 VAN 2WD, TRANSIT T250 VAN 4WD, TRANSIT T350 VAN 2WD, TRANSIT T350 VAN 4WD, TRANSIT T350 WAGON 2WD, TRANSIT T350 WAGON 4WD"]
[2020,"FOMOCO","LFMXD06.26BC","LFMXF0250NDJ","Ford","F350 4x4","HFE1-6.2-J-791",3,6.2,8921,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",32.910000000000004,0.5343,0.0921,70.18,1.081,0.09670000000000001,"HFMX10046742","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","CA","California + CAA Section 177 states","L3ULEV200","California LEV-III ULEV200","150","CO2",999,999,"999",0,{"$nulls":6},"Ford: F250 2WD BED DELETE FFV, F250 4WD BED DELETE FFV, F350 2WD BED DELETE FFV, F350 4WD BED DELETE FFV"]
[2020,"FOMOCO","LFMXD06.761B",null,"Ford","F350 4x4","LFE1-6.7-J-580",0,6.7,9326,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",5.9,-0.12204999999999999,0.06328,67.23,0.3272,0.06161,"LFMX91004404","EPA","2","CVS 75 and later (w/o can. load)","19","Federal Cert Diesel 7-15 PPM Sulfur","B","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","CA","California + CAA Section 177 states","L3ULEV200","California LEV-III ULEV200","150","METHANE",0.0152,0.017,"99.999",0,{"$nulls":3},0.0022,-0.0545,null,"Ford: F250 2WD BED DELETE DIESEL, F250 4WD BED DELETE DIESEL, F250 PICKUP 2WD DIESEL, F250 PICKUP 4WD DIESEL, F350 2WD BED DELETE DIESEL, F350 2WD DIESEL, F350 4WD BED DELETE DIESEL, F350 4WD DIESEL"]
[2020,"FOMOCO","LFMXT01.01B7","LFMXR0090GDE","Ford","1.0L EcoSport","JBW1-1.0-J-074",1,1,3094,3990,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",4.33,0.0577,0.02512,25.64,0.14300000000000002,0.026189999999999998,"JFMX10051251","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDT1","LDT1 (LVW-3750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","PM",3.4000000000000002E-3,0.003,"0.010",0,{"$nulls":6},"Ford: ECOSPORT FWD"]
[2020,"FOMOCO","LFMXT02.33U1","LFMXR0170NDF","Ford","Ford Explorer","LTW1-2.3-L-472",0,2.3000000000000003,4421,5860,4750,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",18.44,0.07680000000000001,0.02812,33.72,0.1768,0.02897,"LFMX10058102","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.021,0.02,"999.99",0.0008,{"$nulls":6},"Ford: EXPLORER AWD, EXPLORER RWD"]
[2020,"FOMOCO","LFMXT02.52F1","LFMXR0135LDF","Ford","Escape FHEV","LTC1-2.5-H-525",1,2.5,3706,4730,4000,"P","Part-time 4-Wheel Drive","CVT","Continuously Variable",null,1,"N","N",null,null,"Y",7.38,0.08594,0.02549,30.43,0.264,0.024739999999999998,"LFMX10060707","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","PM",0.0002,0,"0.006",0,{"$nulls":6},"Ford: ESCAPE AWD HEV, ESCAPE FWD HEV, ESCAPE FWD HEV SE SPORT"]
[2020,"FOMOCO","LFMXT03.33DU","LFMXR0260NDG","Ford","F150 Super Cab 4x4","JFC1-3.3-J-028",1,3.3000000000000003,4687,6500,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",23.82,0.01228,0.03686,49.78,0.23320000000000002,0.0369,"JFMX91003524","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","N2O",1E-4,1E-3,"0.010",6.0000000000000006E-4,{"$nulls":6},"Ford: F150 2WD FFV BASE PAYLOAD LT, F150 4WD FFV BASE PAYLOAD LT, F150 PICKUP 2WD FFV, F150 PICKUP 4WD FFV"]
[2020,"FOMOCO","LFMXT03.54HF","LFMXR0260NDV","Ford","Expedition","JB81-3.5-F-077",0,3.5,6044,7650,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N",21.04,0.14389,0.03343,44.34,0.2849,0.035969999999999995,"JFMX10049737","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","HCHO",0.0007,1E-3,"0.004",3.0000000000000003E-4,{"$nulls":6},"Ford: Expedition 2WD, Expedition 4WD, Expedition MAX 2WD, Expedition MAX 4WD  Lincoln: NAVIGATOR 2WD, NAVIGATOR 4WD, NAVIGATOR L 2WD, NAVIGATOR L 4WD"]
[2020,"FOMOCO","LFMXT05.03DP","LFMXR0260NDV","Ford","F150 SuperCrew Cab 4X4","JFA00111",0,5,5181,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",23.34,0.1106,0.03839,44.94,0.11230000000000001,0.04126,"LFMX10061921","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",3.4000000000000002E-3,0.006,"9.999",0.003,{"$nulls":6},"Ford: F150 2WD FFV BASE PAYLOAD LT, F150 4WD FFV BASE PAYLOAD LT, F150 5.0L 2WD FFV GVWR>7599 LBS, F150 5.0L 4WD FFV GVWR>7599 LBS, F150 PICKUP 2WD FFV, F150 PICKUP 4WD FFV"]
[2020,"FOMOCO","LFMXV03.0VLG","LFMXR0135NDE","Lincoln","Continental","HPL1-3.0-J-837",0,3,4689,5700,5000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",27.275000000000002,0.10160000000000001,0.01982,54.550000000000004,0.5082,0.01982,"HFMX10040932","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","B","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","50","CO",0.55,0.6,"10.0",0.02,{"$nulls":6},"Lincoln: CONTINENTAL AWD, CONTINENTAL COACH"]
[2020,"GM","LGMXD06.0395","LGMXR0223841","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","60GCGNT397",0,6,7950,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",29.37,0.3628,0.07293999999999999,56.2,0.7994,0.07175,"GGMX10037951","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B250","Federal Tier 3 HD Class 2b Bin 250","150","CO",1.05,1.5,"6.4",0.49,null,"N",{"$nulls":3},1,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD CARGO INCOM, G2500 EXPRESS 2WD PASS, G2500 EXPRESS 2WD PASS INCOM, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD CARGO INCOM, G3500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD PASS INCOM  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD CARGO INCOM, G2500 SAVANA 2WD PASS, G2500 SAVANA 2WD PASS INCOM, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD CARGO INCOM, G3500 SAVANA 2WD PASS, G3500 SAVANA 2WD PASS INCOM"]
[2020,"GM","LGMXD06.6394","LGMXR021260A","CHEVROLET","SILVERADO 4WD CAB CHAS","66CRLN1018",1,6.6000000000000005,8000,10000,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",26.27,0.4409,0.05149,52.83,1.0395,0.0492,"LGMX91004181","EPA","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","CA","California + CAA Section 177 states","L3ULEV200","California LEV-III ULEV200","150","NOX",0.021400000000000002,0.021,"99.999",null,null,"N",{"$nulls":3},1,"Chevrolet: SILVERADO 2500 HD 2WD, SILVERADO 2500 HD 4WD  GMC: SIERRA 2500 HD 2WD, SIERRA 2500 HD 4WD"]
[2020,"GM","LGMXT02.0100","LGMXR009537C","BUICK","ENVISION AWD","204JXN5313",0,2,4116,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",21.3,0.0592,0.02217,43.49,0.3289,0.02155,"JGMX10046978","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.0064,0.006,"99.999",null,null,"Y",1.03,null,null,1,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2020,"GM","LGMXT02.5201","LGMXR014640A","GMC","ACADIA FWD","25TLNN5939",1,2.5,4200,6001,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",14.74,0.09380000000000001,0.02521,30.26,0.375,0.024200000000000003,"LGMX10059046","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.0171,0.017,"99.999",null,null,"Y",1.03,null,null,1,"Chevrolet: BLAZER FWD  GMC: ACADIA FWD"]
[2020,"GM","LGMXT03.6161","LGMXR013835A","GMC","CANYON 4WD","36TPHVT711",0,3.6,4566,6000,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",28.48,0.28,0.028919999999999998,50.77,0.5893,0.02887,"HGMX10044802","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.0008,1E-3,"99.999",null,null,"Y",1.03,null,null,1,"Chevrolet: COLORADO 2WD, COLORADO 4WD  GMC: CANYON 2WD, CANYON 4WD"]
[2020,"GM","LGMXT05.3382","LGMXR021250B","CHEVROLET","K1500 SUBURBAN 4WD","53KPHN1323",0,5.3,5992,7500,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",26.35,0.1885,0.03174,57.17,0.7254,0.02903,"HGMX10041495","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.31,0.3,"99.9",null,null,"N",{"$nulls":3},1,"Chevrolet: C1500 SUBURBAN 2WD, K1500 SUBURBAN 4WD  GMC: C1500 YUKON XL 2WD, K1500 YUKON XL 4WD"]
[2020,"GM","LGMXT05.3384","LGMXR016150A","CHEVROLET","K1500 SUBURBAN 4WD","53KPHN1323",0,5.3,5992,7500,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",26.35,0.1885,0.03174,57.17,0.7254,0.02903,"HGMX10041494","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.004,0.004,"0.125",null,1,"N",{"$nulls":3},1,"Chevrolet: C1500 TAHOE 2WD, K1500 TAHOE 4WD  GMC: C1500 YUKON 2WD, K1500 YUKON 4WD"]
[2020,"GM","LGMXT06.2375","LGMXR017350D","GMC","SIERRA 4WD AT4","62KPKNT378",3,6.2,5480,7000,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N",30.67,0.1116,0.03687,49.58,0.9144,0.034,"LGMX10057401","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",2.9000000000000002E-3,0.003,"0.125",null,1,"N",{"$nulls":3},1,"Chevrolet: SILVERADO 4WD, SILVERADO 4WD TRAILBOSS  GMC: SIERRA 4WD, SIERRA 4WD AT4"]
[2020,"GM","LGMXV02.0031","LGMXR013030B","CADILLAC","CTS AWD","206GAE4665",0,2,3947,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",22.45,0.1278,0.01737,54.89,0.4611,0.01609,"JGMX10046586","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.011000000000000001,0.011000000000000001,"0.070",null,1,"N",{"$nulls":3},1,"Chevrolet: CAMARO"]
[2020,"GM","LGMXV03.6048","LGMXR0133810","CADILLAC","XTS","366JGN4763",0,3.6,4088,null,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",16.04,0.1335,0.017849999999999998,38.36,0.3168,0.0182,"JGMX10047201","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NOX",3.8E-3,0.004,"99.999",null,null,"N",{"$nulls":3},1,"Chevrolet: IMPALA"]
[2020,"GM","LGMXV04.2088","LGMXR0112835","CADILLAC","CT6 AWD","426KKV4251",0,4.2,4626,null,5000,"A","All Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",0.89,-0.1452,0.021400000000000002,50.1,0.4169,0.02002,"KGMX91004285","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","N2O",0.0032,0.003,"0.010",null,null,"N",{"$nulls":3},1,"Cadillac: CT6 AWD"]
[2020,"GM","LGMXV06.2091","LGMXR01383CC","CHEVROLET","CORVETTE","621LYV2893",1,6.2,3715,null,4000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.83,0.10070000000000001,0.02299,34.44,0.7623000000000001,0.01903,"LGMX91004526","EPA","3","HWFE","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG+NOX",0.0548,0.055,"0.125",null,1,"N",{"$nulls":3},1,"Chevrolet: CORVETTE"]
[2020,"Honda","LHNXV01.53EB","LHNXR0127VSA","HONDA","ACCORD","EJA01C",2,1.5,3316,null,3625,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,7,"Y","N",null,null,"N",2.85,0.384,0.01637,49.550000000000004,-0.596,0.02744,"JHNX10050346","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","NMOG+NOX",1.5E-3,0.009000000000000001,"0.030",null,1,"Y",1.03,{"$nulls":3},"Honda: ACCORD"]
[2020,"Honda","LHNXV01.5FBB","LHNXR0086VFA","HONDA","FIT","EJR71M",0,1.5,2591,null,2875,"F","2-Wheel Drive, Front","M","Manual",null,6,"N","N",null,null,"N",5.42,0.1316,0.01817,21.740000000000002,0.2786,0.01783,"JHNX10046559","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",0.0071,0.02,"999.999",0.012400000000000001,null,"Y",1.100561,{"$nulls":3},"Honda: FIT"]
[2020,"Honda","LHNXV03.5FEM","LHNXR0129VFB","ACURA","RLX HYBRID","EJ9S1D",0,3.5,4394,null,4750,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"Y",-8.94,0.029300000000000003,0.02053,35.7,0.3205,0.01926,"JHNX91003585","EPA","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NOX",0.010100000000000001,0.012,"999.999",1.4E-3,null,"N",{"$nulls":4},"Acura: RLX"]
[2020,"Hyundai","LHYXV01.6AB6","LHYXR0120ABG","HYUNDAI","Accent","HC5U0G6MC012F",0,1.6,2712,3638,3000,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N",6.849,0.15866,0.017601,37.791000000000004,-0.23049,0.022439,"LHYX10056463","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.020800000000000003,0.029,"99.999",0.0081,{"$nulls":6},"HYUNDAI MOTOR COMPANY: Accent"]
[2020,"Hyundai","LHYXV01.6BC5","LHYXR0110BCE","HYUNDAI","VELOSTER","JS-U0G6TD717F",0,1.6,2976,3858,3250,"F","2-Wheel Drive, Front","AM","Automated Manual",null,7,"N","N",null,null,"N",10.104000000000001,0.11020999999999999,0.019711,27.858,0.23795,0.019461,"LHYX10055930","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","METHANE",6.6E-3,0.011000000000000001,"0.030",0.004,null,"N",{"$nulls":4},"HYUNDAI MOTOR COMPANY: Veloster"]
[2020,"Hyundai","LHYXV02.0CE5","LHYXR0130CEG","HYUNDAI","Elantra","AD-U0N0MC041F",0,2,2932,3924,3250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",2.529,0.31085999999999997,0.015118,32.753,-0.13613999999999998,0.020458999999999998,"LHYX10056323","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",1.8000000000000002E-3,0.005,"99.999",0.0032,null,"Y",1.03,{"$nulls":3},"HYUNDAI MOTOR COMPANY: Elantra, Elantra SE"]
[2020,"Hyundai","LHYXV02.0GG6","LHYXR0140GGE","Genesis","G70","IK8F0HU07AC",0,2,3827,4828,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",19.1,0.35850000000000004,0.017679999999999998,45.234,0.63154,0.017051999999999998,"KHYX10050164","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CREE",999,1000,"999",0.556345,{"$nulls":6},"GENESIS: G70 AWD, G70 RWD"]
[2020,"Hyundai","LHYXV02.4MH3","LHYXR0135MHG","Hyundai","Santa Fe","TM9F4AU05AC",1,2.4,3781,4729,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.28,0.2278,0.02512,32.042,0.26722,0.025202,"KHYX10051796","MFR","52","Fed. fuel 50 F exh.","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","4","CO",0.26,0.3,"1.0",null,null,"N",{"$nulls":4},"HYUNDAI MOTOR COMPANY: Santa Fe FWD"]
[2020,"Hyundai","LHYXV03.3HK6","LHYXR0140HME","Hyundai","G80","DH7L3HU07AC",0,3.3000000000000003,4674,5644,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",22.783,-0.07886,0.021903,54.636,0.33407,0.019313,"JHYX10044120","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","CO",0.7118,0.912,"99.999",0.2,null,"N",{"$nulls":4},"GENESIS: G80 AWD, G80 RWD"]
[2020,"Jaguar Land Rover L","LJLXJ03.0FSP","LJLXR0160P1Z","Jaguar","XF AWD","U25307",0,3,4314,5240,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-28.1,0.6151,0.012751,36.99,0.6192000000000001,0.015791,"FJLX10053437","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","120","PM",1.7000000000000001E-3,2E-3,"0.003",0,null,"N",{"$nulls":4},"Jaguar: F-TYPE Convertible, F-TYPE Coupe, F-TYPE S AWD Convertible, F-TYPE S AWD Coupe, F-TYPE S Convertible, F-TYPE S Coupe, XE, XE AWD, XF, XF AWD, XF Sportbrake AWD, XJ, XJ AWD, XJL, XJL AWD"]
[2020,"Jaguar Land Rover L","LJLXT03.0HTR","LJLXR0175P1Z","Land Rover","Defender","3ELTT039",1,3,5320,6975,5500,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y",0.5640000000000001,0.09530000000000001,0.034166999999999996,47.83,0.40945,0.034871,"LJLX10063196","MFR","51","CA fuel 50 Deg(F) exhaust test","46","CARB LEV3 E10 Regular Gasoline","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","4","NMOG+NOX",0.0182,0.018000000000000002,"0.060",0,null,"N",{"$nulls":4},"Land Rover: Defender 110 MHEV, Defender 90 MHEV, Range Rover MHEV, Range Rover Sport MHEV"]
[2020,"Kia","LKMXT03.3KJ5","LKMXR0139KJG","KIA","SEDONA","YP9L3AU05AC",0,3.3000000000000003,4740,6085,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",13.567,0.12983,0.029598,36.606,0.35780999999999996,0.028627,"KKMX10050495","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","CREE",266,267,"999",0.506315,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Sedona"]
[2020,"Kia","LKMXV01.6L13","LKMXR0120L1E","KIA","NIRO","DE7G6VU01AC",0,1.6,3274,4255,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"N","N",null,null,"Y",6.273000000000001,0.20675,0.01948,25.264000000000003,0.32832,0.019509,"HKMX10042778","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","4","CO",0.1,0.1,"1.0",{"$nulls":7},"HYUNDAI MOTOR COMPANY: Ioniq, Ioniq Blue  KIA MOTORS CORPORATION: Niro, Niro FE, Niro Touring"]
[2020,"Kia","LKMXV01.6L2T","LKMXR0110L2G","KIA","Niro Plug-in","DE8G6WU11AC",0,1.6,3419,4409,3750,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,6,"N","N",null,null,"Y",2.527,0.03523,0.021547,24.281000000000002,0.30811,0.021120999999999997,"JKMX10048362","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","50","CO",1.49,1.5,"10.0",0.04,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Niro Plug-in Hybrid"]
[2020,"Kia","LKMXV02.0D2T","LKMXR0125D2G","KIA","OPTIMA PLUG-IN HYBRID","JF0N0WU03AC",0,2,3794,4850,4000,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"N","N",null,null,"Y",4.327,0.17052,0.015743,32.622,-0.00098,0.018866,"LKMX10055407","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NOX",2.1000000000000003E-3,0.006,"99.999",0.004,{"$nulls":6},"KIA MOTORS CORPORATION: Optima plug-in hybrid"]
[2020,"Landi Renzo","LLDRD06.2C10","LLDRF0000C10","FORD","F250 PICKUP 4x4","1FT7X2A6XHEB69563",1,6.2,8921,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",50.9,0.6301,0.1245,87.81,0.8608,0.12465999999999999,"HLDR10054464","MFR","90","US06","41","CNG","C","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","CA","California + CAA Section 177 states","L3SULEV200","California LEV-III SULEV200","150","HC-NM+NOX",0.41590000000000005,0.41600000000000004,"999.999",null,null,"N",{"$nulls":4},"Landi Renzo USA: F250 2WD BED DELETE, F250 4WD BED DELETE, F250 PICKUP 2WD, F250 PICKUP 4WD, F350 2WD BED DELETE, F350 4WD BED DELETE, F350 INCOMPLETE 2WD, F350 INCOMPLETE 4WD, F350 PICKUP 2WD, F350 PICKUP 4WD"]
[2020,"Maserati","LMAXJ03.0DFI","LMAXR0110161","Maserati","Levante S","332493",0,3,4994,null,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",24.729000000000003,0.43632,0.020437,66.99300000000001,0.19022999999999998,0.024047,"LMAX10059464","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3LEV160","California LEV-III LEV160","150","NOX",0.043300000000000005,0.046,"999.999",0.003,{"$nulls":6},"MASERATI: GHIBLI, GHIBLI S, GHIBLI S Q4, LEVANTE, LEVANTE S, QUATTROPORTE S, QUATTROPORTE S Q4"]
[2020,"MAZDA","LTKXV02.5CDA","LTKXR0117GCP","MAZDA","CX-5","8EBPYUDG1-002",1,2.5,3693,4669,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",12.773000000000001,0.09493,0.024295,36.338,0.11446999999999999,0.025809,"JTKX10049689","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","120","CREE",249,249,"999.9999",0,{"$nulls":6},"MAZDA: MAZDA6"]
[2020,"Mercedes-Benz","LMBXD03.0HD1",null,"Mercedes-Benz","Sprinter 3500 /Freightliner Sprinter 3500","L907DE30TC-Z2054-3",0,2.987,7400,9990,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N",41.297000000000004,-0.45838999999999996,0.056345,82.87,0.321,0.05001,"LMBX91004578","EPA","2","CVS 75 and later (w/o can. load)","19","Federal Cert Diesel 7-15 PPM Sulfur","B","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",2.9000000000000002E-3,0.003,"99.999",3.0000000000000003E-4,null,"Y",1,1E-4,0,null,"Mercedes-Benz: Freightliner Sprinter 2500, Freightliner Sprinter 3500, Sprinter 2500, Sprinter 3500"]
[2020,"Mercedes-Benz","LMBXJ03.0U2A","LMBXR0155LNS","Mercedes-Benz","E 450 4MATIC (station wagon)","S213E30DETC-Z9015-1",0,2.996,4429,5909,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",35.9,0.2622,0.01569,56.86,0.3435,0.016579999999999998,"KMBX10053530","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.0146,0.02,"99.999",0.0051,null,"Y",1.1,{"$nulls":3},"Mercedes-Benz: AMG SLC 43"]
[2020,"Mercedes-Benz","LMBXT02.0HY1","LMBXR0155LNP","Mercedes-Benz","GLC 350e 4MATIC","X253E20DETC-Z2029",0,1.991,4578,5699,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"Y",22.53,0.3267,0.021509999999999998,51.03,0.2713,0.02276,"LMBX10063224","MFR","90","US06","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","PM",1.5E-3,2E-3,"0.006",0.0002,{"$nulls":6},"Mercedes-Benz: GLC 350 e 4MATIC"]
[2020,"Mercedes-Benz","LMBXV02.0U2A","LMBXR0155LNS","Mercedes-Benz","SLC 300","R172E20DETC-Z2034",1,1.991,3449,4012,3750,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",13.88,0.3728,0.01249,36.19,0.39790000000000003,0.01426,"LMBX10061121","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","METHANE",3.1000000000000003E-3,0.008,"0.030",0.0049,{"$nulls":6},"Mercedes-Benz: SLC 300"]
[2020,"Mercedes-Benz","LMBXV02.0U3C","LMBXR0095LNA","Mercedes-Benz","CLA 250 4MATIC","C118E20DETC-Z2036-1",0,1.991,3545,4597,3875,"F","2-Wheel Drive, Front","AM","Automated Manual",null,7,"Y","N",null,null,"N",20.428,0.18202,0.016309,34.84,0.4449,0.015359999999999999,"LMBX10060525","MFR","95","SC03","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","CO",0.2876,0.638,"99.999",0.35000000000000003,{"$nulls":6},"Mercedes-Benz: CLA 250, CLA 250 4MATIC"]
[2020,"Mercedes-Benz","LMBXV04.0U2A","LMBXR0170LNS","Mercedes-Benz","AMG GT R (coupe)","R190E40DETC-Z8018-1",1,3.982,3673,4167,4000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N",22.14,-0.16371,0.025318,40.45,0.6906,0.019200000000000002,"KMBX10055833","MFR","95","SC03","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.027200000000000002,0.034,"99.999",0.007,{"$nulls":6},"Mercedes-Benz: AMG GT (coupe), AMG GT (roadster), AMG GT C (coupe), AMG GT C (roadster), AMG GT R (coupe), AMG GT R (roadster)"]
[2020,"Mercedes-Benz","LMBXV04.0U2B","LMBXR0155LNA","Mercedes-Benz","AMG GT 63 S 4MATIC+","X290E40DETC-Z9018",0,3.982,4874,5820,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",32.372,0.24935,0.020728,65.17,0.5062,0.02054,"KMBX10056490","MFR","3","HWFE","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","METHANE",0.0016,2E-3,"0.030",0,{"$nulls":6},"Mercedes-Benz: AMG GT 63 4MATIC+, AMG GT 63 S 4MATIC+"]
[2020,"Nissan","LNSXT02.5R5A","LNSXR0114PEA","NISSAN","ROGUE AWD","BTEN43",0,2.5,3656,4720,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",13.34,-0.13290000000000002,0.025869999999999997,38.43,-0.161,0.02803,"JNSX10051203","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","CO",4.03,4.14,"999.999",0.11,{"$nulls":6},"NISSAN: ROGUE AWD, ROGUE FWD"]
[2020,"Nissan","LNSXT05.6N9C","LNSXR0174PBA","NISSAN","ARMADA 4WD","TXE425",0,5.6000000000000005,5973,7500,6500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N",17.650000000000002,0.3168,0.02997,41.79,0.9689000000000001,0.02615,"LNSX10057723","MFR","35","California fuel 3-day exhaust","46","CARB LEV3 E10 Regular Gasoline","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.0165,0.02,"0.125",0,{"$nulls":6},"INFINITI: QX80 2WD  NISSAN: ARMADA 2WD, ARMADA 4WD"]
[2020,"Nissan","LNSXV03.5P7C","LNSXR0149PCA","NISSAN","MURANO AWD SL","JJE437",0,3.5,4151,5280,4500,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"N",6.82,0.17020000000000002,0.0234,33.28,0.1383,0.025089999999999998,"LNSX10061811","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.0035,0.005,"999.999",1.3000000000000002E-3,{"$nulls":6},"NISSAN: MURANO AWD, MURANO FWD"]
[2020,"Porsche","LPRXT03.0CV6","LPRXR0150RED","Porsche","Cayenne","EC-9YA-19",0,3,4696,6239,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",49.458000000000006,0.71636,0.01991,49.458000000000006,0.71636,0.01991,"KPRX10054420","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.017,0.033,"999.999",0.016,{"$nulls":6},"Porsche: Cayenne, Cayenne S"]
[2020,"Porsche","LPRXV03.0PV6","LPRXR0190RP7","Porsche","Panamera 4","ECFE-971-19",0,3,4464,5622,4750,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"N","N",null,null,"N",49.458000000000006,0.39797,0.018632,49.458000000000006,0.39797,0.018632,"KPRX10055809","MFR","95","SC03","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","CO",0.3,0.6,"999.9",0.28,{"$nulls":6},"Porsche: Panamera, Panamera 4, Panamera 4 Executive, Panamera 4 ST, Panamera 4S, Panamera 4S Executive, Panamera 4S ST"]
[2020,"RUF","LRAXV03.8T12","LRAXR0150T12","RUF","TURBO 12/CTR 3/CTR 2017","TURBO 12/CTR 3",9,3.8000000000000003,3570,null,4000,"R","2-Wheel Drive, Rear","M","Manual",null,7,"N","N",null,null,"N",7.232,-0.06231,0.01966,40.644000000000005,0.32561999999999997,0.0151,"JRAX10053567","MFR","11","Cold CO","29","Cold CO E10 Premium Gasoline (Tier 3)","B","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","HC-NM",0.21,0.2,"0.3",0,null,"N",{"$nulls":4},"RUF Automobile GmbH: RUFTURBO12/CTR3/CTR ANNIVERSARY"]
[2020,"Subaru","LFJXV02.5JHZ","LFJXR01303BC","SUBARU","WRX STI","JBE-ZC741",0,2.5,3395,4409,3875,"F","2-Wheel Drive, Front","M","Manual",null,6,"N","N",null,null,"N",19.3,0.3224,0.01974,41.31,0.6154000000000001,0.01908,"JFJX91003692","EPA","25","California fuel 2-day exhaust (w/can load)","47","CARB LEV3 E10 Premium Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B160","Federal Tier 3 Bin 160","150","NMOG+NOX",0.077,0.12300000000000001,"0.160",null,1,"Y",1.1,{"$nulls":3},"Subaru: WRX"]
[2020,"Toyota","LTYXT03.5M5M","LTYXR0165P82","TOYOTA","SIENNA AWD","17-GL2A",0,3.456,4750,5995,5000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N",26.09,-0.0648,0.028669999999999998,50.255,0.27049,0.026423,"HTYX10042003","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.0022,0.009000000000000001,"0.070",0.006900000000000001,null,"Y",1.03,null,null,1,"LEXUS: RX 350, RX 350 AWD, RX 350L, RX 350L AWD  TOYOTA: HIGHLANDER, HIGHLANDER AWD, SIENNA, SIENNA AWD"]
[2020,"Toyota","LTYXV03.5M5A","LTYXR0165P12","LEXUS","RC 350 AWD","18-GC1A",0,3.456,3965,null,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",28.1,0.19160000000000002,0.018793,56.28,0.42906,0.018438,"JTYX10049933","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","PM",0.0005,0,"0.003",0,null,"N",{"$nulls":4},"LEXUS: GS 350, GS 350 AWD, GS 350 F SPORT, IS 300 AWD, IS 350, IS 350 AWD, RC 300 AWD, RC 350, RC 350 AWD"]
[2020,"Volkswagen Group of","LVGAJ02.0A3T","LVGAR0135ACT","AUDI","Q3","U3-252",0,1.984,3957,5162,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",3.754,-0.10160000000000001,0.024152999999999997,42.939,0.03979,0.024676999999999998,"KVGA91004288","EPA","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","PM",0.0016,2E-3,"0.006",0,{"$nulls":6},"Audi: Q3 quattro"]
[2020,"Volkswagen Group of","LVGAJ03.0N7F","LVGAR0140NCP","AUDI","SQ5","LN7F-SQ5",0,2.995,4497,5732,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",12.432,0.10454,0.022087,60.249,0.30746,0.023105999999999998,"LVGA10059587","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.0188,0.022000000000000002,"99.999",3.6000000000000003E-3,null,null,1.1,null,null,1,"Audi: S4, S5, S5 Cabriolet, S5 Sportback"]
[2020,"Volkswagen Group of","LVGAT02.0VAA","LVGAR0135VCS","VOLKSWAGEN","Atlas Cross Sport AWD","LC200114",0,2,4348,5666,5000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-6.412,0.67652,0.024100999999999997,43.231,0.62215,0.027004999999999998,"LVGA10061259","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","4","CO",0.54,0.5,"2.1",{"$nulls":7},"Volkswagen: Atlas, Atlas Cross Sport, Atlas Cross Sport 4Motion"]
[2020,"Volkswagen Group of","LVGAV01.4V7P","LVGAR0110VBE","VOLKSWAGEN","Jetta","VW371-00-0015",0,1.395,3062,null,3375,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N",13.635,0.02821,0.016762,27.269000000000002,0.14107,0.016762,"LVGA10062182","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.0037,0.029,"0.070",null,1,{"$nulls":5},"Volkswagen: Jetta"]
[2020,"Volkswagen Group of","LVGAV02.0VAB","LVGAR0135ACU","VOLKSWAGEN","Arteon","VW483000092",0,1.984,3949,null,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",2.2030000000000003,0.29153999999999997,0.015364999999999998,41.994,0.59683,0.015189999999999999,"LVGA10061004","MFR","3","HWFE","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.0022,2E-3,"99.999",0,null,"Y",1.1,{"$nulls":3},"Volkswagen: Arteon, Arteon 4Motion"]
[2020,"Volkswagen Group of","LVGAV06.0EAR","LVGAR0190ECN","BENTLEY","Continental GT Convertible W12","BY635069238/20",0,5.95,5423,null,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"N","N",null,null,"N",0.9670000000000001,0.09354,0.020312,59.574000000000005,0.43804,0.020545,"LVGA10062301","MFR","95","SC03","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",3.6000000000000003E-3,0.01,"99.999",6.6E-3,null,"Y",1.1,{"$nulls":3},"Bentley: Continental GT, Continental GT Convertible, Flying Spur"]
[2020,"Volvo","LVVXJ02.0S30","LVVXR0142EV4","Volvo","XC90 T6 AWD","201915",0,1.969,4704,6060,5000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",24.2,0.12,0.0268,50.443000000000005,0.17962999999999998,0.027462,"KVVX10053412","MFR","3","HWFE","47","CARB LEV3 E10 Premium Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","PM",3.0000000000000003E-4,0,"0.003",0,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: XC90 AWD"]
[2020,"Westport ","LBAFD06.2CNG","LBAFR0250NHJ","Ford","F250","HEB21979",0,6.2,10000,null,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",48.65,0.9143,0.07443,88.41,1.1380000000000001,0.0758,"HBAF10046373","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NOX",0.016,0.07,"999.99",0.05,1,{"$nulls":5},"BAF_Bifuel: Ford F250/350, Ford F350"]
[2019,"Auto Gas America","KAGTD06.039P","KAGTF022385P","CHEVROLET","SILVERADO","1GC4KZCGOGF242304",0,6,6695,10800,9500,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N",74.391,-0.26880000000000004,0.09723599999999999,98.9,0.8639,0.08803,"HAGT10050216","MFR","95","SC03","42","LPG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B250","Federal Tier 3 HD Class 2b Bin 250","150","NMOG",0.032,0.07,"99.99",0.037000000000000005,null,"Y",{"$nulls":4},"Auto Gas America: Chevrolet C25 SILVERADO 2WD, Chevrolet C35 SILVERADO 2WD, Chevrolet K25 SILVERADO 4WD, Chevrolet K35 SILVERADO 4WD, GMC C25 SIERRA 2WD, GMC C35 SIERRA 2WD, GMC K25 SIERRA 4WD, GMC K35 SIERRA 4WD"]
[2019,"BMW","KBMXJ02.0B4X","KBMXR0130F3X","BMW","X4 xDrive30i","LA58295",2,2,4147,5225,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",0.7000000000000001,0.012,0.02247,59.800000000000004,-0.35900000000000004,0.027729999999999998,"KBMX10051713","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","120","N2O",0.0008,1E-3,"0.010",0,{"$nulls":6},"BMW: 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, 330i xDrive Gran Turismo, 330i xDrive Sports Wagon, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe"]
[2019,"BMW","KBMXJ04.4N63","KBMXR0180G05","BMW","X7 xDrive50i","LB39405",0,4.4,5617,7253,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",1.8,0.139,0.02838,70.2,-0.48300000000000004,0.03684,"KBMX10055347","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.06,0.06,"0.125",null,1,{"$nulls":5},"BMW: X5 xDrive50i, X7 xDrive50i"]
[2019,"BMW","KBMXV01.5H60","KBMXR0140G3H","MINI","Mini Cooper SE Countryman ALL4","3B86027",0,1.5,3948,5016,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y",1.3,-0.023,0.0204,44.2,0.027,0.02214,"JBMX10046022","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","120","PM",2E-3,0,"0.01",0,{"$nulls":6},"Mini: MINI COOPER SE COUNTRYMAN ALL4"]
[2019,"BMW","KBMXV02.0M48","KBMXR0100F56","Mini","JOHN COOPER WORKS COUNTRYMAN ALL4","3B91503",0,2,3653,4740,4000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",5.9,-0.033,0.021400000000000002,44,0.05,0.02234,"JBMX10046027","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","PM",2.4000000000000002E-3,2E-3,"0.006",0,{"$nulls":6},"Mini: JOHN COOPER WORKS CONVERTIBLE, JOHN COOPER WORKS HARDTOP"]
[2019,"BMW","KBMXV04.4SM5","KBMXR0150G1X","BMW","M5","G577414",3,4.4,4395,5380,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",4.9,0.322,0.01707,69.3,0.135,0.02102,"JBMX10050140","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","PM",0.0005,0,"0.003",0,{"$nulls":6},"BMW: M5, M5 Competition"]
[2019,"FCA US LLC","KCRXD06.45V4","KCRXF0205TC0","RAM","3500 Cab Chassis 4X4","L9DF89814",0,6.4,8751,10000,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",35.83,0.34740000000000004,0.09380000000000001,90.74,0.1348,0.09978,"KCRX10056656","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","CA","California + CAA Section 177 states","L3LEV395","California LEV-III LEV395","150","METHANE",0.027,0.03,"999.99",0,1,"N",{"$nulls":4},"RAM: 3500 Cab Chassis 4X2, 3500 Cab Chassis 4X4"]
[2019,"FCA US LLC","KCRXJ02.95P0","KCRXR0112PP1","Alfa Romeo","Stelvio AWD","L8AR90988",0,2.9,4367,5423,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",32.62,-0.19890000000000002,0.02844,56.620000000000005,-0.1293,0.02932,"JCRX10051757","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.050300000000000004,0.05,"999.999",0,1,"N",{"$nulls":4},"ALFA ROMEO: Stelvio AWD"]
[2019,"FCA US LLC","KCRXT02.45P1","KCRXR0118PP0","Jeep","Cherokee 4X4","L9KLJ0092",0,2.4,3908,5500,4250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",12.06,-0.016,0.02591,24.69,0.37120000000000003,0.02513,"KCRX91003762","EPA","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","T3B110","Federal Tier 3 Transitional Bin 110","120","NOX",1.2000000000000001E-3,1E-3,"999.999",0,1,"N",{"$nulls":4},"Jeep: Cherokee 4X4, Cherokee FWD"]
[2019,"FCA US LLC","KCRXT02.45P4","KCRXR0110PP0","Jeep","Cherokee 4X4","V9KLJ1721",0,2.4,3908,5500,4250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",2.75,0.1461,0.025529999999999997,26.77,0.403,0.02486,"KCRX10054215","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.0025,2E-3,"999.999",0,1,"N",null,0,0,null,"Jeep: Renegade 4x2, Renegade 4x4"]
[2019,"FCA US LLC","KCRXT03.65P7","KCRXR0136PP0","RAM","1500 4X4","L9DT68860",0,3.6,5123,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y",2.2,0.6784,0.030019999999999998,48.9,0.38530000000000003,0.03599,"KCRX10054867","MFR","95","SC03","46","CARB LEV3 E10 Regular Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",7.6E-3,0.008,"999.999",0,1,"N",null,0,0,null,"Jeep: Wrangler 4X4"]
[2019,"FCA US LLC","KCRXT03.65PC","KCRXR0153PKA","Dodge","Grand Caravan","V7RTK7001",0,3.6,4550,6050,5000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",32.58,-0.33790000000000003,0.02792,50.65,0.1557,0.02547,"KCRX10054483","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","4","CO",1.16,1.2,"10.5",0,1,"N",{"$nulls":4},"Dodge: Journey"]
[2019,"FCA US LLC","KCRXT05.75P2","KCRXR0180RK0","RAM","1500 Classic 4X4","V8DS63465",0,5.7,5476,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",35.04,0.2812,0.03343,83.82000000000001,-0.1391,0.041,"KCRX91003897","EPA","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","120","METHANE",0.019100000000000002,0.019,"0.030",0,1,"N",{"$nulls":4},"Dodge: Durango AWD, Durango RWD  Jeep: Grand Cherokee 4X4"]
[2019,"FCA US LLC","KCRXT05.75P4","KCRXR0225RP0","RAM","1500 Classic 4X4","V8DS63459",0,5.7,5477,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",26.77,0.8112,0.0292,57.480000000000004,1.0965,0.029779999999999997,"KCRX10053989","MFR","95","SC03","46","CARB LEV3 E10 Regular Gasoline","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","4","HC-NM+NOX",0.038,0.04,"0.44",0,1,"N",{"$nulls":4},"RAM: 1500 Classic 4X4"]
[2019,"FCA US LLC","KCRXV05.75P4","KCRXR0141PK0","Dodge","Challenger","V8LAD2126",0,5.7,4267,5300,4500,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N",18.43,-0.1015,0.02502,44.6,0.1267,0.02436,"KCRX10054448","MFR","90","US06","47","CARB LEV3 E10 Premium Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B160","Federal Tier 3 Bin 160","4","HC-NM+NOX",0.112,0.11,"0.14",0,1,"N",null,0,0,null,"Dodge: Challenger"]
[2019,"FOMOCO","KFMXD03.76BX","KFMXF0190NBS","Ford","TRANSIT T350 CHASSIS CAB","GTH1-3.7-J-678",1,3.7,6890,9950,8500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",42.043,0.36466,0.06960999999999999,77.3,0.5618000000000001,0.0704,"GFMX10036541","MFR","21","Federal fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","CA","California + CAA Section 177 states","L3ULEV200","California LEV-III ULEV200","150","CO2",999,999,"999",0,{"$nulls":6},"Ford: TRANSIT T250 CHASSIS CAB, TRANSIT T250 CUTAWAY, TRANSIT T350 CHASSIS CAB, TRANSIT T350 CUTAWAY"]
[2019,"FOMOCO","KFMXD06.27BC","KFMXF0250NBS","Ford","F350 4x4","HFE1-6.2-J-790",1,6.2,10462,14000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",29.72,0.8236,0.0678,88.41,1.1380000000000001,0.0758,"HFMX10043095","MFR","52","Fed. fuel 50 F exh.","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","M7","MDV7 (Cal. LEV 2/3 MDV GVW 10001-14000)","CA","California + CAA Section 177 states","L3ULEV270","California LEV-III ULEV270","4","NOX",0.0364,0.036000000000000004,"999.999",0,{"$nulls":6},"Ford: F350 2WD BED DELETE FFV, F350 4WD BED DELETE FFV"]
[2019,"FOMOCO","KFMXT01.01B7","KFMXR0090GDE","Ford","1.0L EcoSport","JBW1-1.0-J-074",1,1,3094,3990,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",4.33,0.0577,0.02512,25.64,0.14300000000000002,0.026189999999999998,"JFMX10051172","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDT1","LDT1 (LVW-3750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",2E-3,0.025,"9.999",0.023,{"$nulls":6},"Ford: ECOSPORT FWD"]
[2019,"FOMOCO","KFMXT02.33MC","KFMXR0135NDV","Ford","Ranger - Chassis Cab","KFG1-2.3-H-366",0,2.3000000000000003,5025,6050,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",15.23,0.03904,0.053869999999999994,30.46,0.1952,0.053869999999999994,"KFMX10055155","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","CO",0.34,0.3,"2.1",0,{"$nulls":6},"Ford: RANGER 2WD INCOMPLETE"]
[2019,"FOMOCO","KFMXT02.72JQ","KFMXR0135NDF","Lincoln","Nautilus","KD92-2.7-H-192",0,2.7,4744,5960,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",14.86,0.60673,0.022959999999999998,44.12,0.7324,0.023819999999999997,"KFMX10053380","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.0027,0.01,"0.070",null,1,{"$nulls":5},"Ford: EDGE AWD, EDGE FWD  Lincoln: NAUTILUS AWD, NAUTILUS FWD"]
[2019,"FOMOCO","KFMXT03.54HF","KFMXR0260NDV","Ford","Expedition","JB81-3.5-F-077",0,3.5,6044,7650,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N",21.04,0.14389,0.03343,44.34,0.2849,0.035969999999999995,"JFMX91003648","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","CO",1,1.5,"1.7",0.51,{"$nulls":6},"Ford: Expedition 2WD, Expedition 4WD, Expedition MAX 2WD, Expedition MAX 4WD  Lincoln: Navigator 2WD, Navigator 4WD, Navigator L 2WD, Navigator L 4WD"]
[2019,"FOMOCO","KFMXT03.54JK","KFMXR0260NDX","Ford","F-150","JFC1-3.5-J-025",0,3.5,5245,7850,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N",21.797,-0.0789,0.03993,44.39,0.1933,0.03931,"JFMX10047955","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","PM",2.8E-3,0.003,"0.006",0,{"$nulls":6},"Ford: F150 2WD BASE PAYLOAD LT TIRE, F150 3.5L 2WD GVWR>7599 LBS, F150 3.5L 4WD GVWR>7599 LBS, F150 4WD BASE PAYLOAD LT TIRE, F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2019,"FOMOCO","KFMXV02.0VZT","KFMXR0145HCE","Lincoln","MKZ (HEV)","HC91-2.0-J-815",0,2,3919,4910,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y",17.54,0.1904,0.015979999999999998,39.67,0.3541,0.01634,"HFMX10040046","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","CREE",999,999,"999",0.4,{"$nulls":6},"Ford: FUSION HYBRID FWD, FUSION TAXI  Lincoln: MKZ HYBRID FWD"]
[2019,"FOMOCO","KFMXV02.0VZT","KFMXR0145HCE","Lincoln","MKZ (HEV)","HC91-2.0-J-815",0,2,3919,4910,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y",17.54,0.1904,0.015979999999999998,39.67,0.3541,0.01634,"HFMX10040378","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","CO",0.41000000000000003,0.7000000000000001,"1.0",0.2525,{"$nulls":6},"Ford: FUSION HYBRID FWD, FUSION TAXI  Lincoln: MKZ HYBRID FWD"]
[2019,"FOMOCO","KFMXV05.2VES","KFMXR0125NDA","Ford","Mustang","FZG2-5.2-J-731",0,5.2,3820,4600,4250,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N",19.77,0.0935,0.02495,37.4,0.4711,0.02275,"FFMX91002713","EPA","3","HWFE","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","120","CREE",314,315,"999.999",0.7000000000000001,{"$nulls":6},"Ford: SHELBY GT350 MUSTANG"]
[2019,"GM","KGMXD06.0395","KGMXR0223841","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","60GCGNT397",0,6,7950,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",29.37,0.3628,0.07293999999999999,56.2,0.7994,0.07175,"GGMX10036370","MFR","35","California fuel 3-day exhaust","46","CARB LEV3 E10 Regular Gasoline","C","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","CA","California + CAA Section 177 states","L3ULEV250","California LEV-III ULEV250","150","PM",1.5E-3,2E-3,"0.008",0,null,"N",{"$nulls":3},1,"Chevrolet: G2500 EXPRESS 2WD CARGO, G2500 EXPRESS 2WD PASS, G3500 EXPRESS 2WD CARGO, G3500 EXPRESS 2WD PASS  GMC: G2500 SAVANA 2WD CARGO, G2500 SAVANA 2WD PASS, G3500 SAVANA 2WD CARGO, G3500 SAVANA 2WD PASS"]
[2019,"GM","KGMXD06.6375",null,"CHEVROLET","K25 SILVERADO 4WD","66KPHV1700",1,6.6000000000000005,7774,10000,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",42.53,0.27190000000000003,0.039169999999999996,85.37,1.0882,0.03422,"HGMX10044696","MFR","3","HWFE","19","Federal Cert Diesel 7-15 PPM Sulfur","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B250","Federal Tier 3 HD Class 2b Bin 250","120","METHANE",3.1000000000000003E-3,0.003,"99.999",null,null,"N",null,0,0,1,"Chevrolet: C25 SILVERADO 2WD, K25 SILVERADO 4WD  GMC: C25 SIERRA 2WD, K25 SIERRA 4WD"]
[2019,"GM","KGMXT02.0100","KGMXR012637A","BUICK","ENVISION AWD","204JXN5313",0,2,4116,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",21.75,0.0658,0.02155,43.49,0.3289,0.02155,"JGMX91003456","EPA","90","US06","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.0165,0.016,"99.999",null,null,"Y",1.03,null,null,1,"Buick: ENVISION AWD"]
[2019,"GM","KGMXT02.5200","KGMXR013835A","GMC","CANYON 4WD","25TPHST708",0,2.5,4189,5600,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",21.5,0.2046,0.030500000000000003,46.83,0.7519,0.026889999999999997,"JGMX10047300","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","METHANE",0.0146,0.015000000000000001,"0.030",null,null,"N",{"$nulls":3},1,"Chevrolet: COLORADO 2WD, COLORADO 4WD  GMC: CANYON 2WD, CANYON 4WD"]
[2019,"GM","KGMXT03.6151","KGMXR014640A","CHEVROLET","TRAVERSE AWD","361JNN5372",0,3.6,4718,6173,5000,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",16.79,0.1487,0.02479,36.11,0.4746,0.02354,"JGMX91003485","EPA","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B50","Federal Tier 3 Bin 50","120","CREE",252,252,"999.9999",0,null,"N",{"$nulls":3},1,"Buick: ENCLAVE, ENCLAVE AWD  Cadillac: XT5, XT5 AWD  Chevrolet: BLAZER AWD, BLAZER FWD, TRAVERSE AWD, TRAVERSE FWD  GMC: ACADIA AWD, ACADIA FWD"]
[2019,"GM","KGMXT05.3385","KGMXR016150A","CHEVROLET","K10 SILVERADO 4WD","53KPKN1424",0,5.3,5140,7000,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",24.86,0.19870000000000002,0.04058,57.910000000000004,0.8028000000000001,0.03872,"KGMX10052586","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.74,0.7000000000000001,"99.9",null,null,"N",{"$nulls":3},1,"Chevrolet: C10 SILVERADO 2WD, C10 SILVERADO 2WD CAB CHASSIS, K10 SILVERADO 4WD, K10 SILVERADO 4WD CAB CHASSIS  GMC: C10 SIERRA 2WD, C10 SIERRA 2WD CAB CHASSIS, K10 SIERRA 4WD, K10 SIERRA 4WD CAB CHASSIS"]
[2019,"GM","KGMXT05.3386","KGMXR016150A","CHEVROLET","K10 SILVERADO 4WD","53KPKN1436",1,5.3,5461,7300,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",19.55,0.1511,0.03249,42.33,0.775,0.028800000000000003,"KGMX10052324","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","CREE",999,999,"999.9999",0,null,"N",{"$nulls":3},1,"Chevrolet: C10 SILVERADO 2WD, C10 SILVERADO 2WD CAB CHASSIS, K10 SILVERADO 4WD, K10 SILVERADO 4WD CAB CHASSIS  GMC: C10 SIERRA 2WD, C10 SIERRA 2WD CAB CHASSIS, K10 SIERRA 4WD, K10 SIERRA 4WD CAB CHASSIS"]
[2019,"GM","KGMXV01.5002","KGMXR0110875","CHEVROLET","MALIBU","151KZN4364",0,1.5,3221,null,3625,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"N",16.46,-0.10840000000000001,0.02047,36.78,-0.0999,0.02156,"KGMX10053654","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B50","Federal Tier 3 Bin 50","150","NMOG+NOX",0.008,0.008,"0.050",null,1,"N",{"$nulls":3},1,"Chevrolet: CRUZE, CRUZE HATCHBACK, CRUZE PREMIER, CRUZE PREMIER HATCHBACK"]
[2019,"GM","KGMXV01.5010","KGMXR011030C","CHEVROLET","MALIBU","151KZN4361",0,1.5,3221,null,3625,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"N",8.41,0.07590000000000001,0.01866,36.78,-0.0999,0.02156,"KGMX10054007","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","CO",0.5700000000000001,0.6,"1.0",null,null,"N",{"$nulls":3},1,"Chevrolet: MALIBU"]
[2019,"GM","KGMXV02.0031","KGMXR0133880","CADILLAC","CTS AWD","206GAE4665",0,2,3947,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",22.45,0.1278,0.01737,54.89,0.4611,0.01609,"JGMX10046498","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.031900000000000005,0.032,"0.070",null,1,"N",{"$nulls":3},1,"Cadillac: CTS, CTS AWD  Chevrolet: CAMARO"]
[2019,"GM","KGMXV03.6048","KGMXR0123702","CADILLAC","XTS","366JGN4763",0,3.6,4088,null,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",16.04,0.1335,0.017849999999999998,38.36,0.3168,0.0182,"JGMX10047201","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","NMOG+NOX",0.010100000000000001,0.01,"0.030",null,1,"N",{"$nulls":3},1,"Cadillac: XTS  Chevrolet: IMPALA"]
[2019,"GM","KGMXV03.6165","KGMXR013030B","CADILLAC","XTS AWD","366JGN4760",3,3.6,4307,null,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",17.14,0.2204,0.018439999999999998,40.68,0.37920000000000004,0.019049999999999997,"KGMX10053384","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",6.6E-3,0.007,"99.999",null,null,"N",{"$nulls":3},1,"Cadillac: CTS, CTS AWD  Chevrolet: CAMARO"]
[2019,"GM","KGMXV04.2088","KGMXR0112835","CADILLAC","CT6 AWD","426KKV4251",0,4.2,4626,null,5000,"A","All Wheel Drive","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",7.75,-0.114,0.020309999999999998,50.1,0.4169,0.02002,"KGMX91004253","EPA","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",6.0000000000000006E-4,1E-3,"99.999",null,null,"Y",1.03,null,null,1,"Cadillac: CT6 AWD"]
[2019,"Honda","KHNXT02.4WS3","KHNXR01221SA","HONDA","CR-V 2.4L","EHPH1C",0,2.4,3437,null,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",4.64,0.4496,0.019469999999999998,47.17,-0.39780000000000004,0.029439999999999997,"HHNX10044032","MFR","95","SC03","46","CARB LEV3 E10 Regular Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",6.3E-3,0.011000000000000001,"999.999",0.0049,null,"N",{"$nulls":4},"Honda: CR-V AWD, CR-V FWD"]
[2019,"Honda","KHNXV01.5CL2","KHNXR0155VSB","HONDA","INSIGHT","EKL21C",1,1.5,3051,null,3250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y",8.16,-0.08650000000000001,0.01791,19.31,0.264,0.01539,"KHNX10051916","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","120","N2O",6.0000000000000006E-4,1E-3,"0.010",0,null,"N",{"$nulls":4},"Honda: INSIGHT, INSIGHT TOURING"]
[2019,"Honda","KHNXV02.06L3","KHNXR0127VSB","HONDA","ACCORD","EJB21A",0,2,3461,4475,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",-4.11,0.6969000000000001,0.012709999999999999,25.66,0.36100000000000004,0.018019999999999998,"JHNX10049815","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG",0.0044,0.009000000000000001,"999.999",4.8000000000000004E-3,null,"Y",1.1,{"$nulls":3},"Honda: ACCORD, ACCORD 2.0T SPORT/TOURING"]
[2019,"Honda","KHNXV02.4KH3","KHNXR0106VFA","ACURA","ILX","EK4H1D",0,2.4,3162,null,3500,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"Y","N",null,null,"N",-0.49,0.3977,0.014929999999999999,26.14,0.108,0.019049999999999997,"KHNX10054585","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",0.008700000000000001,0.012,"999.999",0.003,null,"Y",1.1,{"$nulls":3},"Acura: ILX"]
[2019,"Hyundai","KHYXV01.6AA6","KHYXR0110AAG","Kia","Soul","PS7R6AU01AC",0,1.6,2877,3902,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",9.784,0.08946,0.024381,28.827,0.17948,0.02453,"HKMX10041787","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",0.019200000000000002,0.025,"99.999",0.0056,null,"Y",1.03,{"$nulls":3},"HYUNDAI MOTOR COMPANY: Accent"]
[2019,"Hyundai","KHYXV01.6EC5","KHYXR0143ECG","Hyundai","Sonata","LF8R6HU04AC",0,1.6,3252,4321,3500,"F","2-Wheel Drive, Front","AM","Automated Manual",null,7,"N","N",null,null,"N",9.33,-0.034,0.01855,32.44,-0.03278,0.019660999999999998,"JHYX10046468","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.0109,0.028,"99.999",0.0176,null,"Y",1.1,{"$nulls":3},"HYUNDAI MOTOR COMPANY: Sonata"]
[2019,"Hyundai","KHYXV02.0BE5","KHYXR0115BEG","HYUNDAI","VELOSTER","JS9N0GU01AC",0,2,2844,3748,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",12.09,-0.12560000000000002,0.0222,28.108,0.37488,0.018078999999999998,"KHYX10050969","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.010700000000000001,0.027,"99.999",0.0162,null,"N",{"$nulls":4},"HYUNDAI MOTOR COMPANY: Veloster"]
[2019,"Hyundai","KHYXV02.0GG6","KHYXR0140GGE","Genesis","G70","IK8F0HU07AC",0,2,3827,4828,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",19.1,0.35850000000000004,0.017679999999999998,45.234,0.63154,0.017051999999999998,"KHYX10050164","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.27,0.5,"2.1",0.26,{"$nulls":6},"GENESIS: G70 AWD, G70 RWD"]
[2019,"Hyundai","KHYXV02.0MG5","KHYXR0135MGG","Hyundai","Santa Fe","TM9F0HU03AC",0,2,4085,4960,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.39,0.4635,0.02235,43.283,0.28686,0.025268,"KHYX10052291","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","METHANE",0.005200000000000001,0.013000000000000001,"0.030",0.0081,null,"N",{"$nulls":4},"HYUNDAI MOTOR COMPANY: Santa Fe AWD, Santa Fe FWD"]
[2019,"Hyundai","KHYXV03.3GK6","KHYXR0140GKE","Genesis","G70","IK8L3HU07AC",0,3.3000000000000003,3913,4993,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",24.012,0.38855999999999996,0.014718,45.499,0.9397099999999999,0.010969,"KHYX10050223","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",0.021500000000000002,0.03,"99.999",8.6E-3,null,"Y",1.1,{"$nulls":3},"GENESIS: G70 AWD, G70 RWD"]
[2019,"Jaguar Land Rover L","KJLXJ02.0RTX","KJLXR0160P1Z","Jaguar","F-Pace","4AJTT050",0,2,4159,5423,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-17.1,0.0847,0.027309999999999997,45.835,-0.01748,0.031211,"JJLX10048228","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG+NOX",0.020200000000000003,0.028,"0.050",null,1,"N",{"$nulls":4},"Jaguar: F-TYPE Convertible, F-TYPE Coupe, XE, XE AWD, XF, XF AWD, XF Sportbrake AWD"]
[2019,"Jaguar Land Rover L","KJLXJ05.0FSM","KJLXR0160P1Y","Jaguar","F-PACE SVR","4AKTT210",0,5,4645,5620,5000,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-19.064,0.22033,0.02515,52.550000000000004,0.09655999999999999,0.02822,"KJLX10055075","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","N2O",1.2000000000000001E-3,1E-3,"0.010",0,null,"N",{"$nulls":4},"Jaguar: F-TYPE R AWD Convertible, F-TYPE R AWD Coupe"]
[2019,"Jaguar Land Rover L","KJLXT05.0FSN","KJLXR0175001","Land Rover","Range Rover LWB","LG366679",0,5,6028,7055,6500,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",51.186,0.10990000000000001,0.031400000000000004,61.42,0.11570000000000001,0.03279,"JJLX10052063","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","METHANE",0.0103,0.021,"0.030",0.0103,null,"N",{"$nulls":4},"Land Rover: Range Rover, Range Rover LWB, Range Rover Sport"]
[2019,"Kia","KKMXV01.6AA6","KKMXR0120AAG","Kia","Soul","PS7R6AU01AC",0,1.6,2877,3902,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",9.784,0.08946,0.024381,28.827,0.17948,0.02453,"HKMX10041791","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CREE",208,208,"999",0.35200000000000004,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Rio"]
[2019,"Kia","KKMXV02.0BF5","KKMXR0110BFG","Kia","Soul","PS7N0AU05AC",0,2,3116,4101,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",4.966,0.06066,0.025731999999999998,35.023,-0.02949,0.027403,"HKMX10041771","MFR","51","CA fuel 50 Deg(F) exhaust test","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","4","NOX",0.0137,0.014,"99.999",null,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Soul"]
[2019,"Kia","KKMXV02.0DG5","KKMXR0143DGG","Kia","Optima","JF9F0HU03AC",0,2,3585,4630,3875,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",14.242,0.04591,0.017685,34.56,0.39394999999999997,0.015463999999999999,"KKMX10053424","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.013300000000000001,0.029,"0.070",0,{"$nulls":6},"KIA MOTORS CORPORATION: Optima"]
[2019,"Kia","KKMXV02.4DH3","KKMXR0143DHG","Kia","Optima","JF9F4AU07AC",0,2.4,3298,4497,3625,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",8.818,-0.06538,0.019788999999999998,31.669,0.29441999999999996,0.017006999999999998,"KKMX10052404","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG+NOX",0.014100000000000001,0.021,"99.999",0,{"$nulls":6},"KIA MOTORS CORPORATION: Optima, Optima FE"]
[2019,"Maserati","KMAXT03.8AWD","KMAXR0110161","MASERATI","LEVANTE GTS","293914",0,3.8000000000000003,5070,null,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",29.54,0.39038,0.02533,65.777,0,0.030279999999999998,"KMAX10054119","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3LEV160","California LEV-III LEV160","150","NMOG",0,0,"999",0.019200000000000002,{"$nulls":6},"MASERATI: LEVANTE GTS, LEVANTE Trofeo"]
[2019,"MAZDA","KTKXT02.2GEA",null,"MAZDA","CX-5","8EBSHG2-010",0,2.2,3913,4907,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",13.71,0.15800999999999998,0.023222,31.388,0.44200999999999996,0.022593,"JTKX91003726","EPA","2","CVS 75 and later (w/o can. load)","19","Federal Cert Diesel 7-15 PPM Sulfur","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B160","Federal Tier 3 Bin 160","120","CREE",299,300,"999.9999",1,{"$nulls":3},0,0,null,"MAZDA: CX-5 2WD, CX-5 4WD"]
[2019,"MAZDA","KTKXV02.5FFA","KTKXR0120GAK","MAZDA","CX-9","8EBPYTG1-016",0,2.5,4361,5816,4750,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",21.82,0.09824,0.025592,41.078,0.33576,0.025508,"JTKX10047426","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0,0.017,"99.999",0.0167,null,"Y",1.03,{"$nulls":3},"MAZDA: MAZDA6"]
[2019,"Mercedes-Benz","KMBXJ03.0U2A","KMBXR0155LNC","Mercedes-Benz","E 450 4MATIC (station wagon)","S213E30DETC-Z9015-1",0,2.996,4429,5909,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",35.9,0.2622,0.01569,56.86,0.3435,0.016579999999999998,"KMBX91003906","EPA","3","HWFE","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.0239,0.035,"0.070",0,{"$nulls":6},"Mercedes-Benz: AMG C 43 4MATIC, AMG C 43 4MATIC (convertible), AMG C 43 4MATIC (coupe), AMG C 43 4MATIC (station wagon), AMG GLC 43 4MATIC, AMG GLC 43 4MATIC (coupe), E 450 (convertible), E 450 (coupe), E 450 4MATIC, E 450 4MATIC (convertible), E 450 4MATIC (coupe), E 450 4MATIC (station wagon)"]
[2019,"Mercedes-Benz","KMBXT02.0HY1","KMBXR0155LNP","Mercedes-Benz","GLC 350e 4MATIC","X253E20DETC-Z8026",0,1.991,4671,5743,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"Y",24.48,-0.07980000000000001,0.02685,44.27,0.7051000000000001,0.01868,"JMBX10050904","MFR","95","SC03","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B30","Federal Tier 3 Bin 30","4","HC-NM+NOX",2E-3,0,"0.25",{"$nulls":7},"Mercedes-Benz: GLC 350e 4MATIC"]
[2019,"Mercedes-Benz","KMBXV02.0U2B","KMBXR0095LNA","Mercedes-Benz","A 220 4MATIC","V177E20DETC-Z9025",0,1.991,3422,4519,3750,"F","2-Wheel Drive, Front","A","Automatic",null,7,"Y","N",null,null,"N",18.400000000000002,0.2726,0.01499,34.61,0.44470000000000004,0.01478,"KMBX10055274","MFR","3","HWFE","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","CREE",999,999,"999",0.137,{"$nulls":6},"Mercedes-Benz: A 220, A 220 4MATIC, A 250, A 250 4MATIC"]
[2019,"Mercedes-Benz","KMBXV03.0HY3","KMBXR0155LNA","Mercedes-Benz","AMG GT 53 4MATIC+","X290E30DETC-Z9021",0,2.999,4692,5622,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"Y",32.732,0.33412,0.019931,59.57,0.5064000000000001,0.02054,"KMBX10057478","MFR","90","US06","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV50","California LEV-III ULEV50","150","NOX",0.0047,0.009000000000000001,"99.999",4.3E-3,{"$nulls":6},"Mercedes-Benz: AMG GT 53 4MATIC+"]
[2019,"Mercedes-Benz","KMBXV04.0U2B","KMBXR0155LNA","Mercedes-Benz","AMG GT 63 S 4MATIC+","X290E40DETC-Z9018",0,3.982,4874,5820,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",32.372,0.24935,0.020728,65.17,0.5062,0.02054,"KMBX10056488","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","METHANE",0.0011,1E-3,"0.030",0,{"$nulls":6},"Mercedes-Benz: AMG GT 63 4MATIC+, AMG GT 63 S 4MATIC+"]
[2019,"Mitsubishi Motors Co","KMTXT02.4G9X","KMTXR0135A1D","MITSUBISHI","OUTLANDER 2WD","PT-N76",0,2.36,3419,4795,3750,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,6,"Y","N",null,null,"N",15.71,-0.09240000000000001,0.024411,38.611000000000004,-0.13385,0.025854,"JMTX10050118","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","FA","Federal","T3B160","Federal Tier 3 Bin 160","120","CREE",284,285,"235",0.9656,null,"N",{"$nulls":4},"Mitsubishi Motors Corporation: OUTLANDER 2WD"]
[2019,"Mitsubishi Motors Co","KMTXV01.2G5P","KMTXR0078A2F","MITSUBISHI","MIRAGE G4","EB19-LD5A",0,1.193,2204,3108,2500,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",4.67,0.1326,0.015000000000000001,20.85,0.1918,0.016312999999999998,"KMTX10051841","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","PM",0.00057,6.0000000000000006E-4,"0.0030",0,null,"N",{"$nulls":4},"Mitsubishi Motors Corporation: MIRAGE, MIRAGE G4"]
[2019,"Nissan","KNSXT05.6N9C","KNSXR0174PBA","NISSAN","ARMADA 4WD","TWE400",3,5.6000000000000005,5976,7500,6500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N",11.81,0.33380000000000004,0.02973,39.59,0.9681000000000001,0.02572,"JNSX10046418","MFR","90","US06","23","CARB Phase II Gasoline","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CO",5.47,5.57,"999.999",0.1,{"$nulls":6},"INFINITI: QX80 2WD  NISSAN: ARMADA 2WD, ARMADA 4WD"]
[2019,"Nissan","KNSXV01.6P4A","KNSXR0087PCA","NISSAN","VERSA","HJE824",0,1.6,2554,null,2875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",3.95,0.09040000000000001,0.01758,17.490000000000002,0.21860000000000002,0.01795,"JNSX10047896","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.0088,0.013000000000000001,"999.999",0.004200000000000001,null,"Y",1.03,null,null,1,"NISSAN: VERSA"]
[2019,"Nissan","KNSXV03.7NAA","KNSXR0120MBA","INFINITI","Q70","DNEG80",1,3.7,4060,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N",17.68,-0.23440000000000003,0.02514,36.59,0.3821,0.01638,"KNSX10050309","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",0.0061,0.008,"999.999",0.0022,1,"Y",1.03,null,null,1,"INFINITI: Q70  NISSAN: 370Z, 370Z Roadster"]
[2019,"Porsche","KPRXT03.0CV6","KPRXR0140RMA","Porsche","Cayenne","EC-9YA-19",0,3,4696,6239,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",49.458000000000006,0.71636,0.01991,49.458000000000006,0.71636,0.01991,"KPRX10054420","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",0.015000000000000001,0.02,"999.99",0.0082,null,"Y",1.1,{"$nulls":3},"Porsche: Macan S"]
[2019,"Porsche","KPRXV03.0C91","KPRXR0150R92","Porsche","911 Targa 4S","EC-991IIS-PDK-17",0,3,3664,4497,4000,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N",21.784000000000002,-0.11179,0.017117999999999998,43.163000000000004,0.35094,0.014091,"HPRX91003001","EPA","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","FA","Federal","T3B160","Federal Tier 3 Bin 160","150","N2O",1.4E-3,0.004,".010",3.1000000000000003E-3,{"$nulls":6},"Porsche: 911 Carrera, 911 Carrera 4, 911 Carrera 4 Cabriolet, 911 Carrera 4 GTS, 911 Carrera 4 GTS Cabriolet, 911 Carrera 4S, 911 Carrera 4S Cabriolet, 911 Carrera Cabriolet, 911 Carrera GTS, 911 Carrera GTS Cabriolet, 911 Carrera S, 911 Carrera S Cabriolet, 911 Carrera T, 911 Targa 4, 911 Targa 4 GTS, 911 Targa 4S"]
[2019,"Roush","KRIIV05.0VKN","KRIIR0125NDA","Roush","Stage 3 Mustang","C191",0,5,4126,null,4500,"R","2-Wheel Drive, Rear","M","Manual","Driver select shifting",6,"N","N",null,null,"N",41.24,-0.0717,0.026439999999999998,62.58,0.21580000000000002,0.025349999999999998,"KRII10054838","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CREE",576,577,"999",0.5932000000000001,{"$nulls":6},"Roush Industries, Inc.: Roush Stage 3 Mustang"]
[2019,"Subaru","KFJXV02.0AJM","KFJXR01223AU","SUBARU","BRZ","DBE-MP42",0,2,2822,null,3125,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",8.05,0.0318,0.01755,28.21,0.3113,0.01689,"DFJX10017431","MFR","25","California fuel 2-day exhaust (w/can load)","23","CARB Phase II Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2","California LEV-II LEV","150","CO",0.29,1.2,"4.2",0.96,{"$nulls":6},"Subaru: BRZ, BRZ tS  TOYOTA: 86"]
[2019,"Tesla","KTSLV00.0L23",null,"Tesla Model 3","Long Range AWD","3D218-008371",0,1E-3,4099,null,4500,"A","All Wheel Drive","A","Automatic",null,1,"N","N",null,null,"N",-11.35,0.1804,0.01082,41.72,0.051500000000000004,0.014979999999999999,"JTSL10054423","MFR","81","Charge Depleting UDDS","62","Electricity","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","ZEV","California ZEV","150","CREE",0,0,"0",0,{"$nulls":6},"Tesla Motors: Model 3 Long Range AWD, Model3 LongRange AWD Performance"]
[2019,"Toyota","KTYXV01.5B6B","KTYXR0085P12","TOYOTA","YARIS","12-NP1M",0,1.497,2295,null,2625,"F","2-Wheel Drive, Front","M","Manual",null,5,"N","N","SF","Single Fuel","N",8.763,-0.00467,0.020770999999999998,19.326,0.18783999999999998,0.019996999999999997,"CTYX10014741","MFR","90","US06","23","CARB Phase II Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","4","CO",0.59,0.6,"8.0",null,null,"N",{"$nulls":4},"TOYOTA: YARIS"]
[2019,"Toyota","KTYXV01.8B6A","KTYXR0115P12","TOYOTA","COROLLA","14-ZE4C",2,1.798,2885,null,3125,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",11.422,0.09448,0.018053,37.255,-0.09672,0.021668,"HTYX10042319","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","NOX",0.0183,0.027,"999.999",0.009000000000000001,null,"N",{"$nulls":4},"TOYOTA: COROLLA"]
[2019,"Toyota","KTYXV03.5M5B","KTYXR0130P72","TOYOTA","AVALON","18-GV2A",3,3.456,3670,null,4000,"F","2-Wheel Drive, Front","A","Automatic",null,8,"Y","N",null,null,"N",17.128,-0.15253,0.022448,34.568000000000005,0.24017999999999998,0.01899,"KTYX10051245","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","CO",0.06,0.2,"1.7",0.12,null,"N",{"$nulls":4},"LEXUS: ES 350, ES 350 F SPORT  TOYOTA: AVALON, AVALON XLE, CAMRY, CAMRY XSE"]
[2019,"Volkswagen Group of","KVGAJ03.0N7F","KVGAR0140NCN","AUDI","SQ5","H7NF-SQ5",1,2.995,4398,5732,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.533000000000001,0.20834999999999998,0.021127,60.249,0.30746,0.023105999999999998,"JVGA91003447","EPA","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","CO",0.11,0.3,"1.70",0.19,{"$nulls":6},"Audi: SQ5"]
[2019,"Volkswagen Group of","KVGAV00.0VZZ",null,"VOLKSWAGEN","e-Golf","VW370-7-0722",0,0.1,3489,4321,3750,"A","All Wheel Drive","A","Automatic","Electric drive",1,"N","N",null,null,"N",-6.205,0.045579999999999996,0.017344,32.8,0.38487,0.015597999999999999,"HVGA10046006","MFR","84","Charge Depleting Highway","62","Electricity","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","ZEV","California ZEV","120","CREE",0,0,"0",0,{"$nulls":6},"Volkswagen: e-Golf"]
[2019,"Volkswagen Group of","KVGAV02.0AAB","KVGAR0135ACU","VOLKSWAGEN","Arteon","VW483-09-0346",0,1.984,3953,null,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-1.3940000000000001,0.50713,0.013561,41.994,0.59683,0.015189999999999999,"KVGA10057729","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.0217,0.022000000000000002,"99.999",0,null,"Y",1.1,null,null,1,"Volkswagen: Arteon, Arteon 4Motion"]
[2019,"Volkswagen Group of","KVGAV05.2NBE","KVGAR0155NAL","LAMBORGHINI","Huracan spyder","LB625_10895",0,5.204000000000001,3902,null,4250,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N",6.566000000000001,-0.47890000000000005,0.025533,62.722,0,0.024619,"KVGA10056226","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B160","Federal Tier 3 Bin 160","120","CREE",373,374,"999.9999",0.84,{"$nulls":6},"Lamborghini: Huracan, Huracan 2WD, Huracan Spyder, Huracan Spyder 2WD"]
[2019,"Volvo","KVVXJ02.0U7A","KVVXR0142EV5","Volvo","XC90 T5 AWD","201807",0,1.969,4682,6060,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.5,0.42700000000000005,0.0247,40.756,0.36990999999999996,0.026049,"JVVX10046756","MFR","51","CA fuel 50 Deg(F) exhaust test","47","CARB LEV3 E10 Premium Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","4","NOX",0.011000000000000001,0.011000000000000001,"999.999",0,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 FWD, S90 AWD, S90 FWD, V60 CC AWD, V60 FWD, V90 CC AWD, V90 FWD, XC60 AWD, XC60 FWD"]
[2018,"Altech","JAECD06.27BC","JAECR0250NBS","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046552","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","NOX",0.006900000000000001,0.057,"999.999",0.05,{"$nulls":6},"Altech-Eco Corporation: F350 Pickup 2WD, F350 Pickup 4WD"]
[2018,"Auto Gas America","JAGTD06.0B99","JAGTF0223850","CHEVROLET","SILVERADO","1GC4KZCGOGF242304",0,6,6695,10800,9500,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N",74.391,-0.26880000000000004,0.09723599999999999,98.9,0.8639,0.08803,"HAGT10052040","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B400","Federal Tier 3 HD Class 3 Bin 400","150","NOX",0.016,0.07,"99.99",0.05,null,"N",{"$nulls":4},"Auto Gas America: C35 CHEV CAB CHASSIS 2WD, C35 GMC CAB CHASSIS 2WD, Chevrolet C35 SILVERADO 2WD, Chevrolet K35 SILVERADO 4WD, GMC C35 SIERRA 2WD, GMC K35 SIERRA 4WD, K35 CHEV CAB CHASSIS 4WD, K35 GMC CAB CHASSIS 4WD"]
[2018,"BMW","JBMXJ02.0B4X","JBMXR0130F3X","BMW","X3 xDrive30i","LA13758",0,2,4156,5258,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.5,0.154,0.02201,64,-0.34700000000000003,0.029529999999999997,"JBMX10048188","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NOX",0.0094,0.012,"99.999",3.1000000000000003E-3,{"$nulls":6},"BMW: 230i Convertible, 230i Coupe, 230i xDrive Convertible, 230i xDrive Coupe, 330i, 330i xDrive, 330i xDrive Gran Turismo, 330i xDrive Sports Wagon, 430i Convertible, 430i Coupe, 430i Gran Coupe, 430i xDrive Convertible, 430i xDrive Coupe, 430i xDrive Gran Coupe"]
[2018,"BMW","JBMXJ03.0F16","JBMXR0170N63","BMW","X6 xDrive 35i","0H21655",4,3,4750,6100,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",17.5,-0.17900000000000002,0.03358,60.7,-0.498,0.038200000000000005,"GBMX91002855","EPA","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","METHANE",2.6000000000000003E-3,0.005,"0.030",0.0025,{"$nulls":6},"BMW: X5 sDrive35i, X5 xDrive35i, X6 sDrive35i, X6 xDrive35i"]
[2018,"BMW","JBMXV00.6I3R","JBMXR0035I3R","BMW","I3s REX","VB86646",0,0.6,3278,3951,3625,"R","2-Wheel Drive, Rear","OT","Other","Fixed Gear",1,"Y","N",null,null,"Y",16.3,-0.096,0.0229,29.6,0.298,0.01908,"JBMX10050105","MFR","81","Charge Depleting UDDS","62","Electricity","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","NMOG",2.8E-3,0.003,"99.999",0,null,"Y",1.1,{"$nulls":3},"BMW: I3 (94Ah) with Range Extender, I3s (94Ah) with Range Extender"]
[2018,"BMW","JBMXV02.0M46","JBMXR0130F45","Mini","Mini Cooper S Countryman ALL4","3B66514",0,2,3671,4696,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",17.900000000000002,0.14,0.02034,44.300000000000004,0.051000000000000004,0.022029999999999998,"HBMX10043734","MFR","52","Fed. fuel 50 F exh.","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","4","NOX",0.006500000000000001,0.006,"99.999",{"$nulls":7},"Mini: COOPER S CLUBMAN, COOPER S CLUBMAN ALL4, COOPER S COUNTRYMAN, COOPER S COUNTRYMAN ALL4"]
[2018,"Ensida Energy","JIMIV03.68LP","JIMIR0141PKA","Chrysler","Dodge Charger Police","2C3CDXAG5HH602880",0,3.6,4324,5350,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",49.160000000000004,0.015600000000000001,0.02404,49.160000000000004,0.015600000000000001,0.02404,"HIMI10051381","MFR","21","Federal fuel 2-day exhaust (w/can load)","42","LPG","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","120","NOX",0.006,0.02,"0.04",0.018000000000000002,{"$nulls":6},"Chrysler: 300, 300 AWD  Dodge: Charger, Charger AWD"]
[2018,"FCA US LLC","JCRXD06.45V4","JCRXF0272TC2","RAM","3500 Cab Chassis 4X4","V5DD83315",3,6.4,8751,10000,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",28.95,1.3957000000000002,0.11774,77.11,1.6371,0.11625999999999999,"JCRX10047534","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B395","Federal Tier 3 HD Class 2b Transitional Bin 395","150","METHANE",0.024,0.02,"999.99",0,1,"N",{"$nulls":4},"RAM: 3500 Cab Chassis 4X2, 3500 Cab Chassis 4X4"]
[2018,"FCA US LLC","JCRXJ01.45P0","JCRXR0137PK0","Jeep","Renegade 4x4","V6BUJ8467",0,1.4000000000000001,3214,4586,3500,"F","2-Wheel Drive, Front","M","Manual",null,6,"N","N",null,null,"N",10.22,0.0236,0.02516,27.39,0.468,0.02307,"JCRX10047310","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","METHANE",0.0128,0.013000000000000001,"0.030",0,1,"N",{"$nulls":4},"FIAT: 500L"]
[2018,"FCA US LLC","JCRXT02.45P0","JCRXR0118PP0","Jeep","Cherokee 4X4","V4KLJ4102",4,2.4,4035,5500,4250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",8.33,0.1719,0.023389999999999998,27.85,0.47350000000000003,0.022449999999999998,"HCRX10043827","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","CA","California + CAA Section 177 states","T3B110","Federal Tier 3 Transitional Bin 110","120","METHANE",0.012400000000000001,0.012,"0.030",0,1,"N",{"$nulls":4},"Jeep: Cherokee 4X4"]
[2018,"FCA US LLC","JCRXT02.45P1","JCRXR0118FE2","Jeep","Cherokee Trailhawk 4X4","L5KLJ9441",3,2.4,4035,5500,4250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",18.42,-0.1009,0.029759999999999998,37.83,0.2972,0.029429999999999998,"HCRX10042805","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","CO",2.21,2.2,"999.9",0,1,"N",{"$nulls":4},"Jeep: Cherokee 4X4, Cherokee 4x4 Active Drive II, Cherokee FWD, Cherokee Trailhawk 4X4"]
[2018,"FCA US LLC","JCRXT03.05PV",null,"RAM","1500 4X4","V6DS66277",7,3,5829,6950,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",31.04,0.2888,0.03297,79.07000000000001,0.13290000000000002,0.038149999999999996,"HCRX10051569","MFR","2","CVS 75 and later (w/o can. load)","19","Federal Cert Diesel 7-15 PPM Sulfur","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2","California LEV-II LEV","50","NMOG",0.0216,0.047,"0.075",0.0154,1,"N",null,0.01,0,null,"Jeep: Grand Cherokee 4X2, Grand Cherokee 4X4  RAM: 1500 4X2, 1500 4X4, 1500 HFE 4X2"]
[2018,"FCA US LLC","JCRXT03.65P4","JCRXR0170PK0","Chrysler","Town & Country","L4RTK1777",2,3.6,5159,6050,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-0.168,0.1812,0.02623,38.04,0.4813,0.024239999999999998,"FCRX10032290","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","120","NOX",0.053000000000000005,0.053000000000000005,"999.999",0,1,"N",{"$nulls":4},"Jeep: Wrangler Unlimited 4X4"]
[2018,"FCA US LLC","JCRXT03.65PB","JCRXR0183RPA","RAM","1500 4X4","V7DS61973",2,3.6,5159,6800,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",32.87,0.3335,0.03252,79.72,-0.1459,0.04001,"JCRX10050676","MFR","3","HWFE","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","120","CREE",322,322,"999.9",0,1,"N",{"$nulls":4},"RAM: 1500 4X2, 1500 4X4"]
[2018,"FCA US LLC","JCRXT05.75P2","JCRXR0180RK0","RAM","1500 4X4","V7DS61971",1,5.7,5675,6900,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",35.58,0.4854,0.030600000000000002,85.82000000000001,-0.1391,0.041,"JCRX91003568","EPA","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","T3B110","Federal Tier 3 Transitional Bin 110","120","NMOG",0.0106,0.011000000000000001,"999.999",0,1,"N",{"$nulls":4},"Dodge: Durango AWD, Durango RWD  Jeep: Grand Cherokee 4X4"]
[2018,"FCA US LLC","JCRXV05.75P1","JCRXR0141PK0","Chrysler","300","L5LXC7820",1,5.7,4437,5350,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",16.32,-0.0597,0.02273,49.5,-0.0172,0.02334,"HCRX10044377","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","T3B110","Federal Tier 3 Transitional Bin 110","4","CO",1.62,1.6,"8.0",0,1,"N",{"$nulls":4},"Chrysler: 300  Dodge: Challenger, Charger"]
[2018,"FOMOCO","JFMXD03.76BK","JFMXR0190NBS","Ford","TRANSIT T350 CHASSIS CAB FFV","JTH1-3.7-J-070",0,3.7,6606,9500,8000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",39.293,0.09701,0.07045,62.13,0.48800000000000004,0.06915,"JFMX10047305","MFR","3","HWFE","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","B","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","CO2",467,467,"999",0,{"$nulls":6},"Ford: TRANSIT T150 VAN FFV, TRANSIT T250 VAN 2WD FFV, TRANSIT T250 WAGON 2WD FFV, TRANSIT T350 VAN 2WD FFV, TRANSIT T350 WAGON 2WD FFV"]
[2018,"FOMOCO","JFMXD06.26CH","JFMXF0265NAS","Ford","F350 4x4","HFE1-6.2-J-791",0,6.2,8775,10000,9500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",46.4,0.5552,0.11646999999999999,87.81,0.8608,0.12465999999999999,"HFMX10043079","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","CA","California + CAA Section 177 states","L3ULEV200","California LEV-III ULEV200","150","PM",0.0004,0,"0.008",0,{"$nulls":6},"Ford: F350 INCOMPLETE 2WD FFV, F350 INCOMPLETE 4WD FFV"]
[2018,"FOMOCO","JFMXT01.01B7","JFMXR0090GDE","Ford","1.0L EcoSport","JBW1-1.0-J-074",1,1,3094,3990,3375,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",4.33,0.0577,0.02512,25.64,0.14300000000000002,0.026189999999999998,"JFMX10051188","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDT1","LDT1 (LVW-3750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","4","CO",0.68,0.7000000000000001,"2.7",0,{"$nulls":6},"Ford: ECOSPORT FWD"]
[2018,"FOMOCO","JFMXT02.52FA","JFMXR0130NDF","Ford","Escape FWD FFV","HM21-2.5-J-848",1,2.5,3552,4620,3875,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",14.16,-0.017,0.02277,31.86,0.0216,0.02608,"HFMX10048040","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","PM",0.0002,0,"0.003",{"$nulls":7},"Ford: ESCAPE FWD FFV"]
[2018,"FOMOCO","JFMXT02.73JK","JFMXR0260NDP","Ford","F-150","JFC1-2.7-J-027",0,2.7,4903,7000,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",22.56,-0.16240000000000002,0.03888,41.96,0.2104,0.03763,"JFMX91003505","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","METHANE",0.0159,0.022000000000000002,"0.030",0.0057,{"$nulls":6},"Ford: F150 2.7L 2WD GVWR>6649 LBS, F150 2.7L 4WD GVWR>6799 LBS, F150 2WD BASE PAYLOAD LT TIRE, F150 4WD BASE PAYLOAD LT TIRE, F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2018,"FOMOCO","JFMXT03.54HF","JFMXR0260NDV","Ford","Expedition","JB81-3.5-F-077",0,3.5,6044,7650,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,10,"Y","N",null,null,"N",21.04,0.14389,0.03343,44.34,0.2849,0.035969999999999995,"JFMX10049740","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",0.014700000000000001,0.023,"9.999",0.008,{"$nulls":6},"Ford: Expedition 2WD, Expedition 4WD, Expedition MAX 2WD, Expedition MAX 4WD  Lincoln: Navigator 2WD, Navigator 4WD, Navigator L 2WD"]
[2018,"FOMOCO","JFMXT03.73E8","JFMXR0145GBC","Ford","Explorer Police FFV, AWD","DUB1-3.7-J-203",0,3.7,4752,6300,5000,"A","All Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N",22.759,0.03837,0.025769999999999998,51.480000000000004,0.6957,0.02541,"DFMX10017613","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","CO",1.1500000000000001,1.3,"1.7",0.19,{"$nulls":6},"Ford: EXPLORER AWD, EXPLORER FWD, Interceptor Utility AWD"]
[2018,"FOMOCO","JFMXT05.03DP","JFMXR0260NDG","Ford","F150 SuperCrew Cab 4X4","JFA00114",1,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",17.75,0.2576,0.0357,44.39,0.1933,0.03931,"JFMX10050023","MFR","3","HWFE","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","CREE",370,370,"999",0.2,{"$nulls":6},"Ford: F150 2WD BASE PAYLOAD LT TIRE, F150 4WD BASE PAYLOAD LT TIRE, F150 5.0L 2WD GVWR>7599 LBS, F150 5.0L 4WD GVWR>7599 LBS, F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2018,"FOMOCO","JFMXT05.03DP","JFMXR0260NDV","Ford","F150 Super Cab 4X4","JFC1-5.0-J-029",0,5,5217,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",26.94,0.11170000000000001,0.0368,44.39,0.1933,0.03931,"JFMX10048056","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.0007,0.01,"9.999",0.0088,null,"Y",1.1,{"$nulls":3},"Ford: F150 2WD FFV BASE PAYLOAD LT, F150 4WD FFV BASE PAYLOAD LT, F150 5.0L 2WD FFV GVWR>7599 LBS, F150 5.0L 4WD FFV GVWR>7599 LBS, F150 PICKUP 2WD FFV, F150 PICKUP 4WD FFV"]
[2018,"FOMOCO","JFMXV03.7VE8","JFMXR0145GBA","Lincoln","MKT","DP43-3.7-J-319",0,3.7,4839,6210,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",2.97,0.3936,0.026269999999999998,32.63,0.6827000000000001,0.025929999999999998,"DFMX10017258","MFR","95","SC03","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","4","CO",1.26,1.3,"2.7",0,{"$nulls":6},"Ford: FLEX AWD, Flex FWD, Police Interceptor Sedan AWD, Police Interceptor Sedan FWD, TAURUS AWD, TAURUS FWD  Lincoln: MKT FWD, MKT LIVERY AWD"]
[2018,"FOMOCO","JFMXV05.0VKN","JFMXR0125NDA","Ford","Mustang","JZG1-5.0-J-087",1,5,3884,4860,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",30.400000000000002,0.15583,0.022019999999999998,54.94,0.27240000000000003,0.022779999999999998,"JFMX10049529","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","OPT-CREE",999,1001,"999",1.95,{"$nulls":6},"Ford: MUSTANG, MUSTANG CONVERTIBLE"]
[2018,"GM","JGMXD06.0398","JGMXF0176860","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","60PGGNT394",0,6,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",53.53,0.526,0.08673,98.9,0.8639,0.08803,"GGMX10036662","MFR","35","California fuel 3-day exhaust","46","CARB LEV3 E10 Regular Gasoline","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B400","Federal Tier 3 HD Class 3 Bin 400","120","METHANE-COMB",0.032,0.03,"0.05",0,null,"N",{"$nulls":4},"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, G4500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH, G4500 SAVANA 2WD CUTAWAY CH"]
[2018,"GM","JGMXD06.0399","JGMXF0176860","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","60PGGNT394",0,6,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",53.53,0.526,0.08673,98.9,0.8639,0.08803,"GGMX10043947","MFR","16","Hot 1435 LA92","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","M7","MDV7 (Cal. LEV 2/3 MDV GVW 10001-14000)","CA","California + CAA Section 177 states","L3ULEV400","California LEV-III ULEV400","150","NMOG+NOX",0.055400000000000005,0.13,"99.999",0,null,"N",{"$nulls":3},1,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, G4500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH, G4500 SAVANA 2WD CUTAWAY CH"]
[2018,"GM","JGMXT01.5095","JGMXR009537B","GMC","TERRAIN AWD","15TJXV4100",0,1.5,3697,4630,4000,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",17.97,0.0123,0.023629999999999998,37.13,0.322,0.022000000000000002,"JGMX10047389","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.0102,0.01,"99.999",null,1,"N",{"$nulls":3},1,"GMC: TERRAIN AWD"]
[2018,"GM","JGMXT02.0100","JGMXR009537B","BUICK","ENVISION AWD","204JXN5313",0,2,4116,5247,4500,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",21.75,0.0658,0.02155,43.49,0.3289,0.02155,"JGMX91003459","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG+NOX",0.0236,0.024,"0.070",null,1,"N",{"$nulls":3},1,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN, TERRAIN AWD"]
[2018,"GM","JGMXT03.6151","JGMXR014640A","CHEVROLET","TRAVERSE AWD","361JNN5372",0,3.6,4718,6173,5000,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",16.17,0.1486,0.02477,36.11,0.4746,0.02354,"JGMX10047276","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.0253,0.025,"99.999",null,null,"N",{"$nulls":3},1,"Buick: ENCLAVE, ENCLAVE AWD  Cadillac: XT5, XT5 AWD  Chevrolet: TRAVERSE, TRAVERSE AWD  GMC: ACADIA AWD, ACADIA FWD"]
[2018,"GM","JGMXT05.3382","JGMXR016150A","CHEVROLET","K1500 SUBURBAN 4WD","53KPHN1323",0,5.3,5992,7500,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",26.35,0.1885,0.03174,57.17,0.7254,0.02903,"HGMX10043949","MFR","90","US06","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.005200000000000001,0.005,"99.999",null,null,"N",{"$nulls":3},1,"Chevrolet: C15 SILVERADO 2WD, C1500 TAHOE 2WD, K15 SILVERADO 4WD, K1500 TAHOE 4WD  GMC: C15 SIERRA 2WD, C1500 YUKON 2WD, K15 SIERRA 4WD, K1500 YUKON 4WD"]
[2018,"GM","JGMXT06.2374","JGMXR021250B","GMC","K1500 YUKON XL 4WD","62CUHNT296",0,6.2,5990,7500,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",26.6,0.3014,0.02886,53.38,0.5637,0.02871,"HGMX10040560","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","METHANE",0.0131,0.013000000000000001,"0.030",null,null,"N",{"$nulls":3},1,"Cadillac: ESCALADE 2WD, ESCALADE 4WD  GMC: C1500 YUKON XL 2WD, K1500 YUKON XL 4WD"]
[2018,"GM","JGMXV01.4001","JGMXR0095805","BUICK","ENCORE AWD","143SV855DA",0,1.4000000000000001,3344,null,3625,"F","2-Wheel Drive, Front","SA","Semi-Automatic","T6",6,"Y","N",null,null,"N",1.77,0.1268,0.02197,27.3,0.35750000000000004,0.02362,"GGMX10039063","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","T3B110","Federal Tier 3 Transitional Bin 110","120","NOX",1.5E-3,2E-3,"99.999",null,null,"N",{"$nulls":3},1,"Buick: ENCORE, ENCORE AWD"]
[2018,"GM","JGMXV01.5030","JGMXR0060600","CHEVROLET","VOLT","151GRN4058",1,1.5,3560,null,3875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y",10.11,0.1335,0.01457,27.1,0.21730000000000002,0.01559,"GGMX10036203","MFR","35","California fuel 3-day exhaust","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","NMOG",0.013600000000000001,0.014,"99.999",null,null,"Y",1.1,null,null,1,"Chevrolet: VOLT"]
[2018,"GM","JGMXV02.0031","JGMXR0112830","CADILLAC","CTS AWD","206GAE4665",0,2,3947,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",22.45,0.1278,0.01737,54.89,0.4611,0.01609,"JGMX10046586","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","CREE",241,241,"999.9999",0,null,"N",{"$nulls":3},1,"Cadillac: CT6"]
[2018,"GM","JGMXV02.5001","JGMXR0133810","CHEVROLET","IMPALA","251G1V4501",0,2.5,3764,null,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",7,0.016300000000000002,0.018619999999999998,44.83,0.1689,0.021179999999999997,"HGMX10041625","MFR","11","Cold CO","26","Cold CO Regular (Tier 2)","C","LDV","LDV/Passenger Car","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","50","CO",2.5500000000000003,2.6,"10.0",null,null,"N",{"$nulls":3},1,"Chevrolet: IMPALA"]
[2018,"GM","JGMXV03.6167","JGMXR0133810","CADILLAC","XTS","366DGN4270",0,3.6,5940,null,6000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",21.03,0.1153,0.02989,62.980000000000004,0.4792,0.028909999999999998,"DGMX10021841","MFR","11","Cold CO","24","Cold CO Regular (CERT)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","T3B110","Federal Tier 3 Transitional Bin 110","50","CO",2.9,2.9,"10.0",null,null,"N",{"$nulls":3},1,"Cadillac: XTS HEARSE, XTS LIMO"]
[2018,"Honda","JHNXV01.5362","JHNXR0113VSB","HONDA","CIVIC 5DR","EHAA3C",0,1.5,2965,null,3250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",10.82,-0.0114,0.01774,44.9,-0.6173000000000001,0.025169999999999998,"HHNX10042098","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","NMOG+NOX",0.011600000000000001,0.016,"0.030",null,1,"Y",1.04,{"$nulls":3},"Honda: CIVIC 2Dr, CIVIC 4Dr, CIVIC 5Dr"]
[2018,"Honda","JHNXV01.5TH2","JHNXR0113VSB","HONDA","CIVIC 5DR","EHAA2C",0,1.5,2965,null,3250,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,7,"Y","N",null,null,"N",7.38,0.2609,0.01624,51.27,-0.605,0.02642,"HHNX10041123","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.0114,0.017,"999.999",5.3E-3,null,"N",{"$nulls":4},"Honda: CIVIC 2Dr, CIVIC 4Dr, CIVIC 5Dr"]
[2018,"Honda","JHNXV02.0C63","JHNXR0113VSA","HONDA","CIVIC 4DR SEDAN 2.0L","EGBB3C",1,2,2805,null,3125,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",1.67,0.1996,0.014549999999999999,30.13,-0.13820000000000002,0.01882,"GHNX10038018","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","120","CREE",999,999,"999.999",0.01,null,"N",{"$nulls":4},"Honda: CIVIC 2Dr, CIVIC 4Dr"]
[2018,"Honda","JHNXV02.4NH3","JHNXR0106VFA","ACURA","ILX","EG4H1D",1,2.4,3090,null,3375,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"Y","N",null,null,"N",1.54,0.3514,0.01453,25.92,0.1726,0.01753,"GHNX10034065","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","CO",0.039,0.069,"999.9999",0.03,null,"N",{"$nulls":4},"Acura: ILX"]
[2018,"Hyundai","JHYXV01.61Y5","JHYXR01101YE","HYUNDAI","Kona","OS8R6HU07AC",0,1.6,3256,4255,3500,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N",11.579,0.31106,0.021176999999999998,34.778,0.42984,0.021078,"JHYX10049630","MFR","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",1.2000000000000001E-3,0.009000000000000001,"99.999",7.8000000000000005E-3,{"$nulls":6},"HYUNDAI MOTOR COMPANY: Kona AWD, Kona FWD"]
[2018,"Hyundai","JHYXV01.61Y5","JHYXR01101YE","HYUNDAI","Kona","OS8R6HU07AC",0,1.6,3256,4255,3500,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N",11.579,0.31106,0.021176999999999998,34.778,0.42984,0.021078,"JHYX10049636","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","120","CREE",208,208,"999",0,{"$nulls":6},"HYUNDAI MOTOR COMPANY: Kona AWD, Kona FWD"]
[2018,"Hyundai","JHYXV02.01G6","JHYXR01201GE","Hyundai","Elantra GT","PD8N0AU01AC",0,2,2943,3968,3250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",8.934000000000001,-0.09489,0.020624999999999998,30.435000000000002,0.09139,0.019884,"JHYX10045160","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.042300000000000004,0.057,"99.999",0,null,"N",{"$nulls":4},"HYUNDAI MOTOR COMPANY: Elantra GT"]
[2018,"Hyundai","JHYXV02.4AJ5","JHYXR0140AHG","HYUNDAI","Sonata","LF6F4AU03AC",0,2.4,3463,4497,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",12.24,0.08957999999999999,0.01834,31.712,0.26631,0.017547999999999998,"GHYX10035945","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.015300000000000001,0.029,"0.070",0,{"$nulls":6},"HYUNDAI MOTOR COMPANY: Sonata, Sonata SE  KIA MOTORS CORPORATION: Optima, Optima FE, Optima S"]
[2018,"Hyundai","JHYXV05.01S5","JHYXR0140ASE","Hyundai","G90","HI7T0AU13AC",0,5,4905,5864,5250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",24.223000000000003,-0.30834,0.02557,58.581,0.26883999999999997,0.020479,"HHYX10039557","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.004200000000000001,0.016,"0.070",0,{"$nulls":6},"GENESIS: G90 AWD, G90 RWD"]
[2018,"Jaguar Land Rover L","JJLXT03.0GTR",null,"Land Rover","Range Rover Sport","LXFTT208",0,3,5140,6614,5500,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-0.42700000000000005,-0.04342,0.026779999999999998,49.47,0.2621,0.02684,"GJLX10037450","MFR","2","CVS 75 and later (w/o can. load)","19","Federal Cert Diesel 7-15 PPM Sulfur","B","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3LEV160","California LEV-III LEV160","150","NMOG",0.0172,0.043000000000000003,"999.999",0.0257,null,"Y",1,0.0002,0.0035,null,"Land Rover: Discovery, Range Rover, Range Rover Sport"]
[2018,"Kia","JKMXT02.44N3","JKMXR0133DNG","Kia","Sportage","QL7F4AU07AC",0,2.4,3617,4740,3875,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",15.442,0.016309999999999998,0.028704999999999998,36.071000000000005,0.35549,0.025939999999999998,"HKMX10038269","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG+NOX",3.4000000000000002E-3,0.008,"0.030",0,null,"Y",1.1,{"$nulls":3},"KIA MOTORS CORPORATION: Sportage AWD, Sportage FE AWD, Sportage FE FWD, Sportage FWD"]
[2018,"Kia","JKMXV02.0426","JKMXR014042E","HYUNDAI","SONATA HYBRID","HLF6NAUP13A",0,2,3649,4630,4000,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"N","N",null,null,"Y",9.153,0.044809999999999996,0.017346999999999998,29.576,0.21364,0.016543,"GHYX10033916","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",5.3E-3,0.021,"99.999",0.015600000000000001,null,null,1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Optima Hybrid"]
[2018,"Kia","JKMXV02.04E3","JKMXR01344EG","Kia","Forte","YD7N0GU11AC",0,2,2873,3880,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",6.378,0.029509999999999998,0.018851,21.93,0.27138,0.017078,"HKMX91003031","EPA","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","120","N2O",1.7000000000000001E-3,2E-3,"0.010",0.0007,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Forte"]
[2018,"Kia","JKMXV03.34Y6","JKMXR0140DYE","KIA","CK","CK8L3HU07AC",0,3.3000000000000003,4007,5148,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",30.528000000000002,-0.28442999999999996,0.02252,54.658,0.62018,0.014653999999999999,"JKMX10047821","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",4.3E-3,0.013000000000000001,"99.999",8.6E-3,null,"Y",1.03,{"$nulls":3},"KIA MOTORS CORPORATION: Stinger"]
[2018,"MAZDA","JTKXT02.2GEA",null,"MAZDA","CX-5","8EBSHG2-010",0,2.2,3913,4907,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",13.71,0.15800999999999998,0.023222,31.388,0.44200999999999996,0.022593,"JTKX91003726","EPA","2","CVS 75 and later (w/o can. load)","19","Federal Cert Diesel 7-15 PPM Sulfur","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3LEV160","California LEV-III LEV160","150","NMOG",0.02,0.036000000000000004,"99.999",0.0165,null,"N",null,-1E-4,1.7000000000000001E-3,null,"MAZDA: CX-5 2WD, CX-5 4WD"]
[2018,"MAZDA","JTKXT02.5CDA","JTKXR0117GCQ","MAZDA","CX-5","8EBPYUDG1-002",2,2.5,3693,4669,4000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",12.773000000000001,0.09493,0.024295,36.338,0.11446999999999999,0.025809,"JTKX91003674","EPA","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","NMOG",0.007500000000000001,0.01,"99.999",2.6000000000000003E-3,null,"Y",{"$nulls":4},"MAZDA: CX-5 2WD, CX-5 4WD"]
[2018,"MAZDA","JTKXV02.5CDB","JTKXR0125GCM","MAZDA","MAZDA6","7EBPYS1-003",2,2.5,3305,4356,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",10.262,0.10912,0.017396,29.701,0.21558,0.017971,"HTKX10040952","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG",0,1E-3,"99.999",0.0008,null,"Y",1.03,{"$nulls":3},"MAZDA: MAZDA3 4-Door, MAZDA3 5-Door"]
[2018,"Mercedes-Benz","JMBXJ02.0U2C","JMBXR0155LNC","Mercedes-Benz","GLC 300 4MATIC","X253E20DETC-Z6015-1",0,1.991,4107,5214,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",23.852,0.2687,0.022602999999999998,45.436,0.30457,0.023354,"GMBX10039058","MFR","90","US06","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","PM",2E-3,0,"0.01",0.00015,{"$nulls":6},"Mercedes-Benz: C 300, C 300 (Coupe), C 300 (convertible), C 300 4MATIC, C 300 4MATIC (Coupe), C 300 4MATIC (Station Wagon), C 300 4MATIC (convertible), E 300, E 300 4MATIC, GLC 300, GLC 300 4MATIC, GLC 300 4MATIC (Coupe)"]
[2018,"Mercedes-Benz","JMBXJ06.0U2A","JMBXR0155LNS","Mercedes-Benz","AMG G65","G463E60TC-Z6021",0,5.98,5935,7050,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N",32.755,0.11678999999999999,0.040496,65.494,0.5838599999999999,0.040493,"GMBX10038362","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CREE",482,482,"999",0.3,{"$nulls":6},"Mercedes-Benz: AMG SL 65"]
[2018,"Mercedes-Benz","JMBXT04.0U2A","JMBXR0170LND","Mercedes-Benz","G 550 4x4","G463E40DETC-Z7044",0,3.982,6664,7694,7000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N",36.486000000000004,0.9276000000000001,0.052508,70.79,2.40816,0.039464,"HMBX10045555","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CREE",999,999,"999",0.4082,{"$nulls":6},"Mercedes-Benz: G 550, G 550 4x4"]
[2018,"Mercedes-Benz","JMBXV04.0U2A","JMBXR0155LNA","Mercedes-Benz","AMG E 63 S 4MATIC (station wagon)","W213E40DETC-Z8023-3",0,3.982,4640,5800,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",40.061,-0.10980000000000001,0.021665999999999998,64.95,0.2748,0.019719999999999998,"JMBX91003604","EPA","90","US06","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG+NOX",0.0229,0.038,"99.999",0.0146,{"$nulls":6},"Mercedes-Benz: AMG C 63, AMG C 63 (convertible), AMG C 63 (coupe), AMG C 63 S, AMG C 63 S (convertible), AMG C 63 S (coupe), AMG E 63 S 4MATIC, AMG E 63 S 4MATIC (Station Wagon"]
[2018,"Mitsubishi Motors Co","JMTXT02.4G9X","JMTXR0135A1D","MITSUBISHI","OUTLANDER 2WD","PT-N76",0,2.36,3419,4795,3750,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,6,"Y","N",null,null,"N",15.71,-0.09240000000000001,0.024411,38.611000000000004,-0.13385,0.025854,"JMTX10050117","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","CA","California + CAA Section 177 states","L2","California LEV-II LEV","120","NOX",0.003,0.029,"0.090",0.0263,null,"N",{"$nulls":4},"Mitsubishi Motors Corporation: OUTLANDER 2WD"]
[2018,"Nissan","JNSXT02.5P5A","JNSXR0120PBB","NISSAN","ROGUE AWD","BTB832",5,2.5,3683,4720,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",14.25,-0.338,0.02469,38.43,-0.161,0.02803,"JNSX10049450","MFR","51","CA fuel 50 Deg(F) exhaust test","46","CARB LEV3 E10 Regular Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","4","CO",0.49,0.5,"1.7",0,1,{"$nulls":5},"NISSAN: ROGUE AWD, ROGUE FWD"]
[2018,"Nissan","JNSXV01.6N4A","JNSXR0087PCA","NISSAN","VERSA","HKDG63",1,1.6,2536,null,2875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",4.51,0.11410000000000001,0.01569,17.34,0.2192,0.01613,"JNSX10047714","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0,1E-3,"999.999",1.3000000000000002E-3,1,{"$nulls":5},"NISSAN: VERSA"]
[2018,"Nissan","JNSXV02.5R5A","JNSXR0126PCA","NISSAN","ALTIMA SR","FPE825",1,2.5,3262,null,3500,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",7.97,0.07350000000000001,0.01486,37.46,-0.182,0.01917,"JNSX10048400","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","120","CREE",253,253,"999.999",0.030723,1,{"$nulls":5},"NISSAN: ALTIMA, ALTIMA SR"]
[2018,"Nissan","JNSXV03.7NAB","JNSXR0120MBA","INFINITI","INFINITI Q70 3.7 AWD","DNE673",0,3.7,4114,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N",19.55,0.15860000000000002,0.01952,43.050000000000004,0.46340000000000003,0.01781,"ENSX10025316","MFR","35","California fuel 3-day exhaust","23","CARB Phase II Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","CO",0.26,0.4,"1.7",0.09,1,{"$nulls":5},"INFINITI: Q70 AWD"]
[2018,"Pagani Automobili S","JPGNV06.0ABC","JPGNR0220AA1","Pagani Automobili","PT4","EDV14PAG01",1,6,3197,null,3500,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"N",33.55,0.7075,-0.00477,61.31,0.8544,0.0148,"EPGN10034052","MFR","11","Cold CO","25","Cold CO Premium (CERT)","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","CO",0.66,0.8,"10.0",0.11,{"$nulls":6},"Pagani Automobili S.p.A.: Huayra"]
[2018,"Rolls-Royce","JRRGV06.8N74","JRRGR0170N63","Rolls Royce","Phantom","U104509",0,6.7,5862,6967,6000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",33.4,-0.054,0.02626,76,-0.512,0.03161,"JRRG10048196","MFR","31","Federal fuel 3-day exhaust","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG",0.0164,0.026000000000000002,"99.999",0.0095,null,"Y",1.1,{"$nulls":3},"Rolls-Royce Motor Cars Limited: Dawn, Ghost, Ghost EWB, Wraith"]
[2018,"Roush","JRIIT05.03DN","JRIIR0260NDV","Roush","F150","T181",0,5,5443,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,10,"Y","N",null,null,"N",28.29,0.1515,0.046009999999999995,54.910000000000004,0.24,0.04792,"JRII10055111","MFR","52","Fed. fuel 50 F exh.","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","4","HCHO",0.007500000000000001,0.008,".016",{"$nulls":7},"Roush Industries, Inc.: F150 Pickup 2WD, F150 Pickup 4WD"]
[2018,"Subaru","JFJXV02.5JHZ","JFJXR01303BC","SUBARU","WRX STI","JBE-ZC741",1,2.5,3395,4409,3875,"F","2-Wheel Drive, Front","M","Manual",null,6,"N","N",null,null,"N",9.200000000000001,0.1757,0.0234,45.44,0.6769000000000001,0.020989999999999998,"JFJX10050274","MFR","11","Cold CO","29","Cold CO E10 Premium Gasoline (Tier 3)","C","LDV","LDV/Passenger Car","FA","Federal","T3B160","Federal Tier 3 Bin 160","120","HC-NM",0.35000000000000003,0.4,"0.6",0.02,{"$nulls":6},"Subaru: WRX STI TYPE RA"]
[2018,"Toyota","JTYXT04.6B6W","JTYXR0190P32","TOYOTA","TUNDRA 4WD","14-UK2A",4,4.6080000000000005,5675,7000,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",19.35,0.2338,0.039509999999999997,47.209,0.42413999999999996,0.040705,"JTYX10047770","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","4","CO",2.89,2.9,"11.8",null,null,"N",{"$nulls":4},"TOYOTA: TUNDRA 2WD, TUNDRA 4WD"]
[2018,"Toyota","JTYXV01.8P35","JTYXR0130J72","TOYOTA","PRIUS PRIME","17-ZW2H",0,1.798,3365,null,3625,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y",8.965,0.12236999999999999,0.014282,18.816000000000003,0.38688999999999996,0.012501,"HTYX10042407","MFR","21","Federal fuel 2-day exhaust (w/can load)","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG",0.0092,0.014,"999.999",0.0047,null,"Y",1.1,null,null,1,"TOYOTA: PRIUS PRIME"]
[2018,"Toyota","JTYXV05.0M5A","JTYXR0180A72","LEXUS","GS F","16-UL2A",2,4.969,4090,null,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",27.477,3.62E-3,0.022243,56.717000000000006,0.43532,0.020493,"GTYX10039328","MFR","11","Cold CO","29","Cold CO E10 Premium Gasoline (Tier 3)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","50","CO",0.58,0.6,"10.0",0.01,null,"N",{"$nulls":4},"LEXUS: LC 500"]
[2018,"Volkswagen Group of","JVGAJ02.0AAC","JVGAR0155AAM","AUDI","Q7","HAAC-Q7A",0,1.984,4771,6221,5000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-4.159,0.04521,0.023337999999999998,46.311,0.25682,0.025317,"HVGA10040590","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","N2O",2E-3,0.006,"0.010",4.3E-3,{"$nulls":6},"Audi: Q7"]
[2018,"Volkswagen Group of","JVGAT02.0VUD","JVGAR0125VAT","VOLKSWAGEN","Tiguan","VW316-6-0055/17",0,1.984,3816,5004,4000,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",4.878,0.29299,0.02555,43.613,0.58598,0.02328,"HVGA10042232","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","4","CO",1.082,1.08,"3.50",{"$nulls":7},"Volkswagen: Tiguan Limited, Tiguan Limited 4Motion"]
[2018,"Volkswagen Group of","JVGAT06.0EAR","JVGAR0155ECR","BENTLEY","Bentayga","BY636060021",0,5.95,6000,null,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",5.912,0.37655,0.02136,51.706,0.64856,0.02136,"HVGA10043676","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",0.0173,0.035,"99.999",0.0176,{"$nulls":6},"Bentley: Bentayga"]
[2018,"Volkswagen Group of","JVGAV02.0V3R","JVGAR0110VBD","VOLKSWAGEN","Beetle","VW324-17-0129/18",0,1.984,3289,null,3625,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",2.271,0.04919,0.023861999999999998,30.597,0.17833,0.023164,"JVGA10047246","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG",3.6000000000000003E-3,0.009000000000000001,"99.999",0.005,null,"Y",1.1,{"$nulls":3},"Volkswagen: Beetle, Beetle Convertible, Beetle Dune, Beetle Dune Convertible"]
[2018,"Volkswagen Group of","JVGAV08.0GLB","JVGAR0200GCB","BUGATTI","Bugatti Chiron","BG744 5008",0,7.993,4519,null,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,7,"Y","N",null,null,"N",-23.056,-0.4423,0.030031,64.453,0.49989,0.023164,"HVGA10044865","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B160","Federal Tier 3 Bin 160","150","NMOG",0.0398,0.055,"99.999",0.0155,null,"Y",1.1,{"$nulls":3},"Bugatti: Chiron"]
[2018,"Volvo","JVVXJ02.0A70","JVVXR0142EV4","Volvo","XC90 T5 AWD","201807",0,1.969,4682,6060,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",10.5,0.42700000000000005,0.0247,40.756,0.36990999999999996,0.026049,"JVVX10046754","MFR","3","HWFE","47","CARB LEV3 E10 Premium Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",1E-3,1E-3,"999.999",0,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: XC90 AWD, XC90 FWD"]
[2017,"Altech","HAECD06.26BA","HAECR0000NB1","Ford","F250 Super Cab","1FT7X2A61HEB19084",0,6.2,6079,10000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",52.86,0.9420000000000001,0.07513,88.41,1.1380000000000001,0.0758,"HAEC10046551","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG+NOX",0.022000000000000002,0.11,"0.200",null,1,{"$nulls":5},"Altech-Eco Corporation: F250 Pickup 2WD, F250 Pickup 4WD, F350 Pickup 2WD, F350 Pickup 4WD"]
[2017,"Auto Gas America","HAGTD06.0D95","HAGTR0223842","CHEVROLET","SILVERADO","1GC4KZCGOGF242304",0,6,6695,10800,9500,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N",74.391,-0.26880000000000004,0.09723599999999999,98.9,0.8639,0.08803,"HAGT10046376","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B150","Federal Tier 3 HD Class 2b Bin 150","150","NMOG+NOX",0.01,0.1,"0.15",0,null,"N",{"$nulls":4},"Auto Gas America: Chevrolet C25 SILVERADO 2WD, Chevrolet C35 SILVERADO 2WD, Chevrolet G2500 EXPRESS 2WD CARG, Chevrolet G2500 EXPRESS 2WD PASS, Chevrolet G3500 EXPRESS 2WD CARG, Chevrolet G3500 EXPRESS 2WD CUT, Chevrolet G3500 EXPRESS 2WD PASS, Chevrolet K25 SILVERADO 4WD, Chevrolet K35 SILVERADO 4WD, GMC C25 SIERRA 2WD, GMC C35 SIERRA 2WD, GMC G2500 SAVANA 2WD CARGO, GMC G2500 SAVANA 2WD PASS, GMC G3500 SAVANA 2WD CARGO, GMC G3500 SAVANA 2WD PASS, GMC G3500 SAVANNA 2WD CUTAWAY CH, GMC K25 SIERRA 4WD, GMC K35 SIERRA 4WD"]
[2017,"BMW","HBMXT02.0H20","HBMXR0190F15","BMW","X5 xDrive40e","0F74534",0,2,5220,6570,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y",17.1,-0.319,0.03374,56.2,-0.432,0.035339999999999996,"GBMX91002729","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","NOX",0.014,0.02,"0.07",null,1.2,{"$nulls":5},"BMW: X5 xDrive40e"]
[2017,"BMW","HBMXV02.0M48","HBMXR0100F56","Mini","JOHN COOPER WORKS CLUBMAN ALL4","2D66206",0,2,3485,4564,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",11.700000000000001,0.077,0.019389999999999998,42,0.045000000000000005,0.02028,"HBMX10044234","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","NMOG",0.0054,0.007,"99.999",null,1.375,"Y",1.04,{"$nulls":3},"Mini: JOHN COOPER WORKS CONVERTIBLE, JOHN COOPER WORKS HARDTOP"]
[2017,"CMI","HCEXD05.08VV",null,"Nissan","Titan","PA10",0,5,6712,8990,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",49.980000000000004,-0.6118,0.04842,83.15,0.35450000000000004,0.040209999999999996,"HCEX10041188","MFR","2","CVS 75 and later (w/o can. load)","19","Federal Cert Diesel 7-15 PPM Sulfur","B","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","FA","Federal","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","120","HC-NM",0.0912,0.094,"0.195",0,null,"N",null,0.0027,0,null,"Nissan: Titan XD 2WD, Titan XD 4WD"]
[2017,"FCA US LLC","HCRXD06.45V0","HCRXR0272TC1","RAM","2500 Cab Chassis 4X4","L4DJ77302",7,6.4,8751,9900,9000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",17.31,1.2895,0.13924999999999998,62.49,2.06,0.133,"HCRX10042171","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B340","Federal Tier 3 HD Class 2b Transitional Bin 340","150","NMOG",0.040400000000000005,0.04,"999.999",0,1,"N",{"$nulls":4},"RAM: 2500 4X2, 2500 4X4"]
[2017,"FCA US LLC","HCRXJ01.45P0","HCRXR0116PK0","Dodge","Dart","L5PFD1574",1,1.4000000000000001,3248,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"Y","N",null,null,"N",-2.5500000000000003,0.379,0.01466,18.44,0.402,0.016139999999999998,"GCRX10036194","MFR","95","SC03","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NMOG+NOX",0.0737,0.07400000000000001,"999.999",0,1,"N",{"$nulls":4},"Dodge: Dart, Dart Aero"]
[2017,"FCA US LLC","HCRXJ01.45P0","HCRXR0116PK1","Dodge","Dart","L5PFD1574",1,1.4000000000000001,3248,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"Y","N",null,null,"N",-2.5500000000000003,0.379,0.01466,18.44,0.402,0.016139999999999998,"GCRX10036194","MFR","95","SC03","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","150","NOX",0.061000000000000006,0.06,"999.99",0,1,"N",{"$nulls":4},"FIAT: 500X  Jeep: Renegade 4x2, Renegade 4x4"]
[2017,"FCA US LLC","HCRXJ02.45P1","HCRXR0137PK0","Jeep","Cherokee 4X4","V4KLJ4102",3,2.4,4035,5500,4250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",8.33,0.1719,0.023389999999999998,27.85,0.47350000000000003,0.022449999999999998,"HCRX10041436","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","120","N2O",1E-3,1E-3,"0.010",0,1,"N",{"$nulls":4},"RAM: Promaster City"]
[2017,"FCA US LLC","HCRXJ03.65PA","HCRXR0116PKA","Chrysler","Town & Country","L4RTK1777",1,3.6,4567,6050,5000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-4.25,0.18810000000000002,0.02673,36.38,0.4693,0.024229999999999998,"FCRX10032293","MFR","21","Federal fuel 2-day exhaust (w/can load)","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","LDV","LDV/Passenger Car","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","120","NOX",0.011000000000000001,0.01,"999.99",0,1,"N",{"$nulls":4},"Chrysler: 200, 200 AWD"]
[2017,"FCA US LLC","HCRXT02.45P4","HCRXR0112PK0","Jeep","Compass 4X4","V4MKJ9222",1,2.4,3257,4575,3625,"F","2-Wheel Drive, Front","M","Manual",null,5,"N","N",null,null,"N",13.32,0.2911,0.0219,32.75,0.5733,0.02059,"GCRX10036744","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","CA","California + CAA Section 177 states","L2","California LEV-II LEV","50","NMOG",0.025500000000000002,0.026000000000000002,"0.075",0,1,"N",{"$nulls":4},"Jeep: Compass X 4X4, Patriot X 4X4"]
[2017,"FCA US LLC","HCRXT03.65P1","HCRXR0140RK0","Chrysler","Town & Country","L4RTK1777",2,3.6,5159,6050,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-0.168,0.1812,0.02623,38.04,0.4813,0.024239999999999998,"FCRX10032290","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","T3B110","Federal Tier 3 Transitional Bin 110","120","CO",1.25,1.2,"5.6",0,1,"N",{"$nulls":4},"Chrysler: Pacifica"]
[2017,"FCA US LLC","HCRXT03.65P1","HCRXR0170PK0","Chrysler","Town & Country","L4RTK1777",2,3.6,5159,6050,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-0.168,0.1812,0.02623,38.04,0.4813,0.024239999999999998,"FCRX10032290","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","120","CO",1.25,1.2,"5.6",0,1,"N",{"$nulls":4},"Jeep: Wrangler Unlimited 4X4"]
[2017,"FCA US LLC","HCRXV03.65PB","HCRXR0141PKA","Chrysler","300 AWD","L5LXF1270",2,3.6,4324,5350,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",6.84,0.45020000000000004,0.01815,49.160000000000004,0.015600000000000001,0.02404,"HCRX10044779","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","120","CO",0.35000000000000003,0.4,"2.1",0,1,"N",{"$nulls":4},"Chrysler: 300, 300 AWD  Dodge: Charger, Charger AWD"]
[2017,"FOMOCO","HFMXD03.56BZ","HFMXR0190NBS","Ford","T350 TRANSIT VAN","GTH1-3.5-J-689",0,3.5,6883,10360,8500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",47.300000000000004,0.013600000000000001,0.0478,75.99,0.5780000000000001,0.044649999999999995,"GFMX10035554","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B340","Federal Tier 3 HD Class 2b Transitional Bin 340","120","NOX",0.006,0.006,"0.266",0,{"$nulls":6},"Ford: TRANSIT T150 VAN, TRANSIT T250 VAN, TRANSIT T350 VAN, TRANSIT T350 WAGON"]
[2017,"FOMOCO","HFMXD03.77BX","HFMXF0190NBS","Ford","TRANSIT T350 CHASSIS CAB","GTH1-3.7-H-715",0,3.7,7610,10360,9000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",45.782000000000004,0.19374,0.07808,80.85000000000001,0.5728,0.07771,"GFMX10043806","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","M7","MDV7 (Cal. LEV 2/3 MDV GVW 10001-14000)","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","120","NOX",0.01,0.2,"0.4",0.16,null,"N",{"$nulls":4},"Ford: TRANSIT T350 CHASSIS CAB, TRANSIT T350 CUTAWAY"]
[2017,"FOMOCO","HFMXT01.52GA","HFMXR0130NDF","Ford","Escape FWD","HM21-1.5-J-847",0,1.5,3701,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",18.01,0.1428,0.023649999999999997,43.69,0.14780000000000001,0.025929999999999998,"HFMX91003042","EPA","3","HWFE","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NMOG",0.0005,0.004,"9.999",0.003,null,"Y",1.1,{"$nulls":3},"Ford: ESCAPE AWD, ESCAPE FWD"]
[2017,"FOMOCO","HFMXT02.32ED","HFMXR0125NBB","Lincoln","MKC","EME3-2.3-H-537",0,2.3000000000000003,4157,5020,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",4.53,0.4194,0.02114,33.94,0.4007,0.02376,"FFMX91002082","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","METHANE",0.013600000000000001,0.025,"0.030",0.0117,{"$nulls":6},"Lincoln: MKC  AWD"]
[2017,"FOMOCO","HFMXT02.73JJ","HFMXR0235NBC","Ford","F-150 Super Cab Max","FFC1-2.7-J-546",0,2.7,4932,7000,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",25.675,0.56419,0.02852,55.120000000000005,0.6481,0.03015,"FFMX10031868","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.0264,0.032,"999.999",5.5000000000000005E-3,null,"Y",1.1,{"$nulls":3},"Ford: F150 2.7L 2WD GVWR>6649 LBS, F150 2.7L 4WD GVWR>6649 LBS, F150 2WD BASE PAYLOAD LT TIRE, F150 4WD BASE PAYLOAD LT TIRE, F150 PICKUP 2WD, F150 PICKUP 4WD"]
[2017,"FOMOCO","HFMXT03.73DM","HFMXR0145GBC","Ford","Explorer Police FFV, AWD","DUB1-3.7-J-203",0,3.7,4752,6300,5000,"A","All Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N",22.759,0.03837,0.025769999999999998,51.480000000000004,0.6957,0.02541,"DFMX10017614","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","NOX",0.003,0.03,"0.09",0.031,{"$nulls":6},"Ford: EXPLORER FFV 2WD, EXPLORER FFV AWD, Interceptor Utility FFV AWD"]
[2017,"FOMOCO","HFMXV02.0VZ2","HFMXR0110GBX","Ford","FOCUS","CDH3-2.0-H-195",0,2,2948,3250,3250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N",8.667,0.24025,0.01883,31.88,0.28150000000000003,0.01943,"CFMX10012361","MFR","90","US06","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B85","Federal Tier 3 Transitional Bin 85","4","HC-NM+NOX",0.007,0.01,"0.14",{"$nulls":7},"Ford: FOCUS FWD"]
[2017,"FOMOCO","HFMXV03.5VEP","HFMXR0145GBA","FORD","Explorer","GGA00041",0,3.5,5028,6300,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",26.21,-0.2652,0.03501,51.13,0.3629,0.0307,"GFMX10037124","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CO",0.17,0.6,"2.1",0.39,{"$nulls":6},"Ford: FLEX AWD, Police Interceptor Sedan AWD, TAURUS AWD  Lincoln: MKT AWD"]
[2017,"FOMOCO","HFMXV05.2VES","HFMXR0125NDA","Ford","Mustang","FZG2-5.2-J-731",0,5.2,3820,4600,4250,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N",19.77,0.0935,0.02495,37.4,0.4711,0.02275,"FFMX91002712","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","CO",0.61,0.7000000000000001,"1.7",0.06,{"$nulls":6},"Ford: SHELBY GT350 MUSTANG"]
[2017,"GM","HGMXD06.0398","HGMXF0176860","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","60PGGNT394",0,6,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",53.53,0.526,0.08673,98.9,0.8639,0.08803,"GGMX10037950","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","M7","MDV7 (Cal. LEV 2/3 MDV GVW 10001-14000)","CA","California + CAA Section 177 states","L3ULEV400","California LEV-III ULEV400","150","NMOG+NOX",0.0349,0.11,"0.400",0,null,"N",{"$nulls":3},1,"Chevrolet: G3500 EXPRESS 2WD CUTAWAY CH, G4500 EXPRESS 2WD CUTAWAY CH  GMC: G3500 SAVANA 2WD CUTAWAY CH, G4500 SAVANA 2WD CUTAWAY CH"]
[2017,"GM","HGMXD06.0399","HGMXR021260A","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","60PGGNT394",0,6,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",53.53,0.526,0.08673,98.9,0.8639,0.08803,"GGMX10036662","MFR","35","California fuel 3-day exhaust","46","CARB LEV3 E10 Regular Gasoline","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B400","Federal Tier 3 HD Class 3 Bin 400","120","CO2",999,999,"999.999",0,null,"N",{"$nulls":3},1,"Chevrolet: C35 SILVERADO 2WD, K35 SILVERADO 4WD  GMC: C35 SIERRA 2WD, K35 SIERRA 4WD"]
[2017,"GM","HGMXJ03.6165","HGMXR013030B","CADILLAC","SRX AWD","366FNE5600",0,3.6,4607,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",11.08,0.38930000000000003,0.022109999999999998,40.57,0.4315,0.02506,"GGMX10035187","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","120","NMOG+NOX",0.022500000000000003,0.04,"0.110",0,null,"N",{"$nulls":3},1,"Chevrolet: CAMARO"]
[2017,"GM","HGMXT02.8357",null,"CHEVROLET","COLORADO ZR2 4WD","28SPGV1249",1,2.8000000000000003,5017,6200,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",32.43,0.16090000000000002,0.04078,57.620000000000005,0.5365,0.03908,"HGMX10046200","MFR","2","CVS 75 and later (w/o can. load)","19","Federal Cert Diesel 7-15 PPM Sulfur","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","PM",1E-4,0,"0.003",null,null,"N",null,1E-4,-0.0067,1,"Chevrolet: COLORADO ZR2 4WD"]
[2017,"GM","HGMXT03.6152","HGMXR014640A","CADILLAC","XT5 AWD","366HNN5244",0,3.6,4394,6001,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",18.97,1E-3,0.02777,45.54,0.1434,0.02777,"HGMX10039810","MFR","95","SC03","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B5","Federal Tier 2 Bin 5","4","HC-NM",0.017,0.02,"99.99",null,null,"N",{"$nulls":4},"Cadillac: XT5, XT5 AWD  GMC: ACADIA, ACADIA AWD"]
[2017,"GM","HGMXT04.3187","HGMXR016150A","CHEVROLET","K15 SILVERADO 4WD","43KPHN1301",0,4.3,5674,7200,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",23.86,0.7282000000000001,0.02086,39.51,1.2795,0.01846,"HGMX10041923","MFR","31","Federal fuel 3-day exhaust","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",2.4000000000000002E-3,0.004,"99.999",2E-3,null,"N",{"$nulls":4},"Chevrolet: C15 SILVERADO 2WD, K15 SILVERADO 4WD  GMC: C15 SIERRA 2WD, K15 SIERRA 4WD"]
[2017,"GM","HGMXT05.3383","HGMXR0176820","GMC","K15 SIERRA 4WD","53CPGNT184",0,5.3,5805,7400,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"Y",24.28,0.1981,0.03503,44.410000000000004,0.3769,0.03635,"GGMX91002917","EPA","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",3.3E-3,0.003,"99.999",null,null,"N",{"$nulls":3},1,"Chevrolet: C15 SILVERADO 2WD, K15 SILVERADO 4WD  GMC: C15 SIERRA 2WD, K15 SIERRA 4WD"]
[2017,"GM","HGMXT06.2374","HGMXR0223840","GMC","K1500 YUKON XL 4WD","62CUHNT296",0,6.2,5990,7500,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",26.6,0.3014,0.02886,53.38,0.5637,0.02871,"HGMX10040565","MFR","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","CO",0.31,0.3,"99.9",0,null,"N",{"$nulls":3},1,"Cadillac: ESCALADE 2WD, ESCALADE 4WD  GMC: C1500 YUKON XL 2WD, K1500 YUKON XL 4WD"]
[2017,"GM","HGMXV01.5020","HGMXR0060600","CHEVROLET","VOLT","151GRN4042",0,1.5,3560,null,3875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y",10.33,0.1136,0.01487,27.1,0.21730000000000002,0.01559,"GGMX91002722","EPA","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.034300000000000004,0.034,"0.125",null,1,"N",{"$nulls":3},1,"Chevrolet: VOLT"]
[2017,"GM","HGMXV02.0050","HGMXR0116832","CADILLAC","CT6 HYBRID","20YS16PV68",0,2,4526,null,4750,"R","2-Wheel Drive, Rear","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y",16.09,0.1193,0.01807,44.17,0.019,0.0222,"HGMX10046081","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","120","NMOG",0,0,"99.999",null,null,"N",{"$nulls":3},1,"Cadillac: CT6 HYBRID"]
[2017,"GM","HGMXV03.6167","HGMXR0133810","CADILLAC","XTS","366DGN4270",0,3.6,5940,null,6000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",31.220000000000002,0.2686,0.025339999999999998,57.25,0.43560000000000004,0.026279999999999998,"DGMX10021838","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B110","Federal Tier 3 Transitional Bin 110","120","NOX",0.012400000000000001,0.012,"99.999",null,null,"N",{"$nulls":3},1,"Cadillac: XTS HEARSE, XTS LIMO"]
[2017,"Honda","HHNXT01.54R3","HHNXR01221SB","HONDA","CR-V 1.5L TC","DHPA1C",0,1.5,3562,null,3875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",3.46,0.42710000000000004,0.02062,46.53,-0.3808,0.03024,"HHNX10044401","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NMOG",0.0002,0.016,"999.999",0.015300000000000001,null,"Y",1.03,{"$nulls":3},"Honda: CR-V AWD, CR-V FWD"]
[2017,"Honda","HHNXV02.0B63","HHNXR0113VSA","HONDA","CIVIC 4DR SEDAN 2.0L","EGBB3C",0,2,2805,null,3125,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",-3.06,0.3884,0.01367,33.14,-0.152,0.0207,"GHNX10038017","MFR","11","Cold CO","26","Cold CO Regular (Tier 2)","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","50","CO",0.39,0.4,"10.0",0,null,"N",{"$nulls":4},"Honda: CIVIC 2Dr, CIVIC 4Dr"]
[2017,"Honda","HHNXV02.4SH3","HHNXR0106VFA","ACURA","ILX","EG4H1D",1,2.4,3090,null,3375,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,8,"Y","N",null,null,"N",2.45,0.2978,0.016919999999999998,28.8,0.1918,0.01948,"GHNX10034066","MFR","11","Cold CO","26","Cold CO Regular (Tier 2)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","HC-NM",0.18,0.2,"0.3",0,null,"N",{"$nulls":4},"Acura: ILX"]
[2017,"Honda","HHNXV03.0HH3","HHNXR0150VFA","HONDA","MDX HYBRID","EHWS1D",0,3,4572,null,5000,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"Y",-8.25,0.2565,0.024669999999999997,37.82,0.2202,0.024900000000000002,"HHNX10043897","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CREE",999,999,"999.9999",0.22,null,"N",{"$nulls":4},"Acura: MDX AWD"]
[2017,"Honda","HHNXV03.5VH3","HHNXR0151VFA","HONDA","PILOT","EHLV1A",0,3.5,4372,5842,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,9,"Y","N",null,null,"N",6.75,-0.4037,0.03399,28.52,0.5425,0.028069999999999998,"HHNX10043638","MFR","11","Cold CO","28","Cold CO E10 Regular Gasoline (Tier 3)","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","50","CO",0.68,0.7000000000000001,"10.0",0.01,null,"N",{"$nulls":4},"Acura: MDX AWD, MDX FWD  Honda: PILOT AWD, PILOT FWD"]
[2017,"Hyundai","HHYXV02.0A16","HHYXR0140A1E","HYUNDAI","SONATA HYBRID","HLF6NAUP13A",0,2,3649,4630,4000,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"N","N",null,null,"Y",9.153,0.044809999999999996,0.017346999999999998,29.576,0.21364,0.016543,"GHYX10033917","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","NOX",1E-3,0.007,"99.999",0.0056,{"$nulls":6},"HYUNDAI MOTOR COMPANY: Sonata HYBRID, Sonata HYBRID SE  KIA MOTORS CORPORATION: Optima Hybrid"]
[2017,"Hyundai","HHYXV03.31MF","HHYXR0140ASE","Hyundai","G90","HI7L3HU05AC",0,3.3000000000000003,4784,5732,5000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",23.693,0.21792999999999998,0.01791,53.006,0.62629,0.015462,"HHYX10039566","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CO",1.0537,1.254,"99.999",0.2,null,"N",{"$nulls":4},"GENESIS: G90 AWD, G90 RWD"]
[2017,"Jaguar Land Rover L","HJLXJ03.0FSP","HJLXR0140P1Z","Jaguar","XF AWD","U25307",0,3,4314,5240,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-28.1,0.6151,0.012751,36.99,0.6192000000000001,0.015791,"FJLX10031622","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","150","PM",0,0,"0.010",0,null,"N",{"$nulls":4},"Jaguar: F-Pace"]
[2017,"Jaguar Land Rover L","HJLXV02.0FTN","HJLXR0160P1Y","Jaguar","XF","TGT4V016",0,2,3948,4844,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",0.899,0.49200000000000005,0.014400000000000001,36.910000000000004,0.36810000000000004,0.017943999999999998,"EJLX10026677","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","METHANE",3.6000000000000003E-3,0.009000000000000001,"0.030",5.5000000000000005E-3,null,"N",{"$nulls":4},"Jaguar: XE, XF"]
[2017,"Kia","HKMXV01.6DBF","HKMXR01221AF","KIA","Rio ECO","UB3R6AU15A1",0,1.6,2601,3593,2875,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",6.49,-0.07282999999999999,0.019785999999999998,24.5,0.20354,0.017661,"EKMX10027268","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","NMOG+NOX",0.009600000000000001,0.026000000000000002,"0.125",0,null,"N",{"$nulls":4},"HYUNDAI MOTOR COMPANY: Accent"]
[2017,"Kia","HKMXV02.04EP","HKMXR01344EG","Kia","Forte","YD7N0GU11AC",0,2,2873,3880,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",6.378,0.029509999999999998,0.018851,21.93,0.27138,0.017078,"HKMX91003034","EPA","90","US06","48","Tier 3 E10 Regular Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG+NOX",0.0171,0.021,"99.999",0,null,"N",{"$nulls":4},"KIA MOTORS CORPORATION: Forte"]
[2017,"Landi Renzo","HLDRT06.2C16","HLDRF0250NBS","Ford","F350 4x4","1FT7X2B62HEB65702",0,6.2,10462,14000,12500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",47.26,0.9105000000000001,0.07518999999999999,88.41,1.1380000000000001,0.0758,"HLDR10046222","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B270","Federal Tier 3 HD Class 3 Bin 270","150","CO2",773,773,"999",0,null,"N",{"$nulls":4},"Landi Renzo USA: F350 2WD BED DELETE FFV, F350 4WD BED DELETE FFV"]
[2017,"MAZDA","HTKXV02.0CDA","HTKXR0115GDP","MAZDA","MAZDA6","7EBPYS1-003",3,2.5,3305,4356,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",10.262,0.10912,0.017396,29.701,0.21558,0.017971,"HTKX10040962","MFR","95","SC03","46","CARB LEV3 E10 Regular Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG",0.0005,1E-3,"99.999",0.0008,null,"Y",1.03,{"$nulls":3},"MAZDA: MAZDA3 4-Door, MAZDA3 5-Door"]
[2017,"Mercedes-Benz","HMBXJ02.0U2A","HMBXR0110LNF","Mercedes-Benz","GLA 250 4MATIC","X156E20DETC-Z4021-3",0,1.991,3552,4387,3875,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N",3.709,0.3441,0.01727,29.225,0.4631,0.017468,"FMBX10032858","MFR","21","Federal fuel 2-day exhaust (w/can load)","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","120","CREE",295,295,"999",0,{"$nulls":6},"Mercedes-Benz: CLA 250 4MATIC, GLA 250 4MATIC"]
[2017,"Mercedes-Benz","HMBXJ06.0U2A","HMBXR0155LNS","Mercedes-Benz","AMG G65","G463E60TC-Z6021",0,5.98,5935,7050,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N",32.755,0.11678999999999999,0.040496,65.494,0.5838599999999999,0.040493,"GMBX10038363","MFR","95","SC03","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","150","CO",0.12200000000000001,0.49200000000000005,"99.999",0.37,{"$nulls":6},"Mercedes-Benz: AMG SL 65"]
[2017,"Mercedes-Benz","HMBXT03.0HY1","HMBXR0170LNP","Mercedes-Benz","GLE 550 e 4MATIC","W166E30DETC-Z6017",0,2.996,5637,6724,6000,"A","All Wheel Drive","A","Automatic",null,7,"Y","N",null,null,"Y",24.324,0.34790000000000004,0.025986,49.89,1.52951,0.014369999999999999,"GMBX10040338","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B4","Federal Tier 2 Bin 4","120","CREE",271,271,"999",0,{"$nulls":6},"Mercedes-Benz: GLE 550e 4MATIC"]
[2017,"Mercedes-Benz","HMBXV02.0HY1","HMBXR0155LNP","Mercedes-Benz","C 350 e","W205E20DETC-Z6029",0,1.991,4175,5082,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"Y",22.346,-0.30760000000000004,0.021182,41.575,0.45198,0.013614,"GMBX10045234","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG+NOX",0.0004,0.01,"0.030",0,{"$nulls":6},"Mercedes-Benz: C 350e"]
[2017,"Mitsubishi Motors Co","HMTXT02.4G5Y","HMTXR0135A1D","MITSUBISHI","OUTLANDER 4WD","EB17-RB4C",0,2.36,3542,4828,3875,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,6,"Y","N",null,null,"N",16.36,0.0521,0.02332,40.311,-0.012100000000000001,0.025266999999999998,"HMTX10039395","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NMOG",1.7000000000000001E-3,0.01,"999.999",0.0082,null,"Y",1.03,{"$nulls":3},"Mitsubishi Motors Corporation: OUTLANDER 2WD, OUTLANDER 4WD"]
[2017,"Nissan","HNSXD05.6V9B","HNSXF0174PBB","NISSAN","NV2500 Cargo Van","TYB237",0,5.6000000000000005,6406,null,8000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N",12.56,0.38680000000000003,0.04186,45.07,0.8693000000000001,0.038200000000000005,"HNSX10044951","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","NMOG",0.0555,0.058,"999.999",2.4000000000000002E-3,1,"Y",1.03,null,null,1,"NISSAN: NV2500 Cargo Van, NV3500 Cargo Van, NV3500 Passenger Van, TITAN XD 2WD, TITAN XD 4WD"]
[2017,"Nissan","HNSXT04.0N6B","HNSXR0132PBB","NISSAN","FRONTIER 4WD FFV","SRE656",1,4,4590,5600,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,5,"Y","N",null,null,"N",20.990000000000002,0.4666,0.024929999999999997,40.67,1.145,0.02008,"HNSX10042309","MFR","3","HWFE","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","NMOG+NOX",0.008400000000000001,0.028,"0.125",0,1,{"$nulls":5},"NISSAN: FRONTIER 2WD FFV, FRONTIER 4WD FFV"]
[2017,"Nissan","HNSXV02.0N2A","HNSXR0120PBA","NISSAN","NISSAN NV200 NYC Taxi STD","KEC659",1,2,3616,null,3875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",6.9,0.2223,0.02291,38.480000000000004,0.057800000000000004,0.026539999999999998,"ENSX10027528","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","NMOG",0.0222,0.029,"999.999",0.0071,1,"Y",1.04,null,null,1,"NISSAN: NV200 NYC Taxi"]
[2017,"Nissan","HNSXV03.7NAA","HNSXR0120MBA","INFINITI","INFINITI G37x Coupe AWD","MLE432",0,3.7,3906,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N",12.92,0.2766,0.0171,34.52,0.5726,0.015629999999999998,"ENSX10023547","MFR","95","SC03","23","CARB Phase II Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B125","Federal Tier 3 Bin 125","120","CO",0.7264,0.7264,"999.9999",0,1,{"$nulls":5},"INFINITI: Q70  NISSAN: 370Z, 370Z Roadster"]
[2017,"Porsche","HPRXT03.6PV6","HPRXR0230RED","Porsche","Cayenne","EC-92AII-16",0,3.6,4819,6195,5000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",22.728,-0.25687,0.0297,38.892,0.12301,0.02737,"GPRX10034545","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","NOX",0.006,0.01,".09",2E-3,{"$nulls":6},"Porsche: Cayenne, Cayenne Platinum"]
[2017,"Porsche","HPRXT04.8CTD","HPRXR0230RED","Porsche","Cayenne Turbo","EC-92AIIT-15",0,4.8,5243,6382,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",31.608,-0.28944,0.03191,48.334,0.12301,0.029109999999999997,"FPRX10033041","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","L2","California LEV-II LEV","50","NOX",0.021,0.02,".05",0,{"$nulls":6},"Porsche: Cayenne Turbo, Cayenne Turbo S"]
[2017,"Subaru","HFJXT02.0NKR","HFJXR01224EP","SUBARU","OUTBACK WAGON AWD","DBE-DL16",0,2.5,3573,null,3875,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,6,"Y","N",null,null,"N",8.63,0.261,0.022269999999999998,41.63,1.9E-3,0.02617,"DFJX10018908","MFR","90","US06","23","CARB Phase II Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","FA","Federal","T3B85","Federal Tier 3 Transitional Bin 85","150","NMOG",4.3E-3,0.006,"999.999",1.4E-3,null,"Y",1.04,{"$nulls":3},"Subaru: CROSSTREK"]
[2017,"Subaru","HFJXV02.0BUY","HFJXR01155AD","SUBARU","IMPREZA 5-Door","HBE-YU15",0,2,3195,4299,3500,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,7,"Y","N",null,null,"N",10.870000000000001,0.19720000000000001,0.01874,34.4,0.1316,0.02042,"HFJX10042665","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NOX",0.004200000000000001,0.006,"999.999",1.524E-3,{"$nulls":6},"Subaru: IMPREZA 4-Door, IMPREZA 5-Door, IMPREZA SPORT 4-Door, IMPREZA SPORT 5-Door"]
[2017,"Toyota","HTYXT05.7BEW","HTYXR0300P32","TOYOTA","TUNDRA 4WD","12-SK2A",0,5.663,5645,7100,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","SF","Single Fuel","N",36.293,-0.17037,0.048950999999999995,61.816,0.58593,0.045065999999999995,"CTYX10015205","MFR","11","Cold CO","26","Cold CO Regular (Tier 2)","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","CO",0.75,0.8,"12.5",0.04,null,"N",{"$nulls":4},"TOYOTA: TUNDRA 2WD, TUNDRA 4WD"]
[2017,"Toyota","HTYXV01.8B6A","HTYXR0115P12","TOYOTA","COROLLA","14-ZE4C",2,1.798,2885,null,3125,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",11.422,0.09448,0.018053,37.255,-0.09672,0.021668,"HTYX10041731","MFR","51","CA fuel 50 Deg(F) exhaust test","23","CARB Phase II Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","4","NMOG",0.0618,0.062,"0.080",null,null,"Y",1.04,null,null,1,"TOYOTA: COROLLA"]
[2017,"Volkswagen Group of","HVGAJ02.0AAC","HVGAR0140AAP","AUDI","Q7","HAAC-Q7A",0,1.984,4771,6221,5000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-4.159,0.04521,0.023337999999999998,46.311,0.25682,0.025317,"HVGA10040586","MFR","21","Federal fuel 2-day exhaust (w/can load)","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.023700000000000002,0.06,"99.999",0.036000000000000004,{"$nulls":6},"Audi: A4, A4 Ultra, A4 allroad quattro, A4 quattro"]
[2017,"Volkswagen Group of","HVGAV01.4V3B","HVGAR0110VCA","AUDI","A3 e-tron","AU373-6-0813/16",0,1.395,3516,null,3875,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,6,"N","N",null,null,"Y",-6.362,-0.11610000000000001,0.020661,35.295,-0.01375,0.020777999999999998,"GVGA10038581","MFR","90","US06","49","Tier 3 E10 Premium Gasoline (9 RVP @Low Alt.)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","CO",0.35700000000000004,0.35700000000000004,"99.999",0,{"$nulls":6},"Audi: A3 e-tron, A3 e-tron ultra"]
[2017,"Volkswagen Group of","HVGAV02.0APA","HVGAR0110ABB","AUDI","A3","FAPA-AAQ",0,1.984,3396,null,3875,"F","2-Wheel Drive, Front","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,6,"N","N",null,null,"N",20.255000000000003,0.05787,0.017169,40.915,0.21703,0.017110999999999998,"FVGA10028831","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","T3SULEV30","Federal Tier 3 Transitional  LEV-II SULEV30 Carryover","150","PM",2E-3,2E-3,"0.010",0,{"$nulls":6},"Audi: A3 Cabriolet quattro, A3 quattro, TT Coupe quattro, TT Roadster quattro  Volkswagen: GTI, Golf, Golf Alltrack, Golf SportWagen, Golf SportWagen 4Motion"]
[2017,"Volkswagen Group of","HVGAV04.0NUA","HVGAR0130EAN","BENTLEY","Continental GT","E3UJ-BY62",0,3.9930000000000003,5543,null,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-6.16,-0.0661,0.019438999999999998,54.853,0.04883,0.022116,"EADX10028468","MFR","52","Fed. fuel 50 F exh.","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","4","NMOG",0.0708,0.0708,"0.0800",null,null,"Y",1.04,null,null,1,"Bentley: Continental GT, Continental GT Convertible, Flying Spur"]
[2017,"Volvo","HVVXJ02.0U3T","HVVXR0130EB2","Volvo","S90 T6 AWD","201706",0,1.969,4112,5200,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",13.8,0.043000000000000003,0.0236,43.512,0.05336,0.024923999999999998,"HVVX10041385","MFR","3","HWFE","47","CARB LEV3 E10 Premium Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NOX",0.003,0.019,"999.999",0.016,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: XC60 AWD"]
[2016,"Altech","GAECT02.52K8","GAECR0125NBV","Ford","Transit Connect (2016 MY)","NM0LS7E74G1239798",0,2.5,3667,5270,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",2.2,0.6816,0.01789,28.59,0.2911,0.026619999999999998,"GAEC10042758","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B5","Federal Tier 2 Bin 5","50","NOX",1E-3,0.01,"0.05",0.005,{"$nulls":6},"Altech-Eco Corporation: Transit Connect Van, Transit Connect Van 2WD, Transit Connect Wagon, Transit Connect Wagon FWD, Transit Connect Wagon LWB, Transit Connect Wagon LWB FWD"]
[2016,"Altech","GAECT03.75HA","GAECR0000NBD","Ford","Transit T250","1FTYR1ZM5GKA06038",3,3.7,4981,9000,9000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",49.03,0.32680000000000003,0.07771,80.85000000000001,0.5728,0.07771,"GAEC10040974","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","NMOG",0.0085,0.038,"0.125",0.029900000000000003,null,"Y",1,{"$nulls":3},"Altech-Eco Corporation: Transit T150 Wagon"]
[2016,"BMW","GBMXT02.0H20","GBMXR0190F15","BMW","X5 xDrive40e","0F74534",0,2,5220,6570,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y",17.1,-0.319,0.03374,56.2,-0.432,0.035339999999999996,"GBMX10034843","MFR","51","CA fuel 50 Deg(F) exhaust test","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","4","NMOG",0.0572,0.057,"0.080",null,null,"Y",1.04,{"$nulls":3},"BMW: X5 xDrive40e"]
[2016,"BMW","GBMXV02.0H48","GBMXR0120F3H","BMW","330e","K478507",1,2,3920,4750,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"Y",21.2,0.056,0.016319999999999998,52.9,-0.113,0.01826,"GBMX10038547","MFR","81","Charge Depleting UDDS","62","Electricity","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","150","NMOG+NOX",0.0324,0.045000000000000005,"0.125",null,1,{"$nulls":5},"BMW: 330e"]
[2016,"BMW","GBMXV04.4N63","GBMXR0130N54","BMW","Alpina B7 LWB xDrive","DS17300",3,4.4,5050,6190,5250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-9.200000000000001,-0.056,0.02163,58.1,-0.35000000000000003,0.02745,"DBMX10022154","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","120","NOX",0.031,0.03,"0.07",null,1.0430000000000001,{"$nulls":5},"BMW: 550i, 550i xDrive, 550i xDrive Gran Turismo, 650i Convertible, 650i Coupe, 650i Gran Coupe, 650i xDrive Convertible, 650i xDrive Coupe, 650i xDrive Gran Coupe, Alpina B6 Gran Coupe xDrive"]
[2016,"FCA US LLC","GCRXD06.45V1","GCRXF0205TC0","RAM","3500 Cab Chassis 4X4","V5DD83315",0,6.4,8500,10000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",24.68,1.3403,0.17218999999999998,75.08,1.6324,0.17024999999999998,"GCRX10036032","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","CA","California + CAA Section 177 states","L2","California LEV-II LEV","120","NOX",0.1,0.1,"0.2",0,1,"N",{"$nulls":4},"RAM: 3500 Cab Chassis 4X2, 3500 Cab Chassis 4X4"]
[2016,"FCA US LLC","GCRXJ02.45P4","GCRXR0153PK0","Dodge","Journey","L4JCD6340",1,2.4,3857,5005,4250,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N",null,null,"N",9.01,0.23620000000000002,0.02377,29.830000000000002,0.5005000000000001,0.02207,"FCRX10031091","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B4","Federal Tier 2 Bin 4","120","CREE",404,404,"999",null,1,"N",{"$nulls":4},"Dodge: Journey"]
[2016,"FCA US LLC","GCRXJ03.65PA","GCRXR0153PKA","Chrysler","Town & Country","L4RTK1777",2,3.6,5159,6050,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-0.168,0.1812,0.26230000000000003,38.04,0.4183,0.024239999999999998,"FCRX10032291","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B4","Federal Tier 2 Bin 4","4","CO",2.7,2.7,"8.0",0,1,"N",{"$nulls":4},"Dodge: Journey"]
[2016,"FCA US LLC","GCRXT03.65P2","GCRXR0180RK0","Dodge","Durango AWD","L6WKT7873",1,3.6,5774,6500,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",32.15,-0.11370000000000001,0.03139,64.82000000000001,-0.2675,0.03514,"GCRX10039110","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","CO",2.99,3,"16.9",0,1,"N",{"$nulls":4},"Dodge: Durango AWD, Durango RWD  Jeep: Grand Cherokee 4X2, Grand Cherokee 4X4"]
[2016,"FCA US LLC","GCRXV01.85P0","GCRXR0100PK0","Fiat","Alfa 4c","L4MAS7806",0,1.8,2463,2750,2750,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,6,"Y","N",null,null,"N",19.332,0.1017,0.01672,37.63,0.034,0.01891,"EFTG91002146","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","CO",0.6900000000000001,0.7000000000000001,"3.4",0,1,"N",{"$nulls":4},"ALFA ROMEO: 4C"]
[2016,"FCA US LLC","GCRXV06.45P1","GCRXR0145PK0","Dodge","Charger SRT8","L5LAD2953",1,6.4,4431,5450,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",17.25,0.0449,0.02188,65.01,-0.1,0.025689999999999998,"GCRX10037837","MFR","11","Cold CO","26","Cold CO Regular (Tier 2)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2","California LEV-II LEV","50","CO",1.61,1.6,"10.0",0,1,"N",{"$nulls":4},"Dodge: Challenger, Challenger SRT8, Charger, Charger SRT8"]
[2016,"FOMOCO","GFMXD03.76BX","GFMXR0190NBD","Ford","TRANSIT T350 CHASSIS CAB","GTH1-3.7-J-678",1,3.7,6890,9950,8500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",42.043,0.36466,0.06960999999999999,77.3,0.5618000000000001,0.0704,"GFMX10036542","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","HDV1","HDV1 (Federal HD chassis Class 2b GVW 8501-10000)","FA","Federal","HDV2B200","Federal Tier 3 HD Class 2b Bin 200","150","CO2",999,999,"999",0,{"$nulls":6},"Ford: TRANSIT T150 VAN, TRANSIT T250 VAN, TRANSIT T350 VAN, TRANSIT T350 WAGON"]
[2016,"FOMOCO","GFMXT02.32ED","GFMXR0125NBV","Lincoln","MKC","EME3-2.3-H-537",0,2.3000000000000003,4157,5020,4500,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",4.53,0.4194,0.02114,33.94,0.4007,0.02376,"FFMX91002082","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","NOX",0.009000000000000001,0.02,"000.05",0.011000000000000001,{"$nulls":6},"Lincoln: MKC  AWD"]
[2016,"FOMOCO","GFMXT03.54HE","GFMXR0265NBC","Ford","Expedition","FB71-3.5-F-586",0,3.5,6339,7760,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",10.44,0.0682,0.038439999999999995,42.910000000000004,0.5663,0.03739,"FFMX10031782","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",0.54,0.5,"4.2",0,{"$nulls":6},"Ford: Expedition 2WD, Expedition 4WD, Expedition EL 2WD, Expedition EL 4WD  Lincoln: Navigator 2WD, Navigator 4WD, Navigator L 2WD, Navigator L 4WD"]
[2016,"FOMOCO","GFMXT05.03DK","GFMXR0235NBC","Ford","F-150 4X4","FFC1-5.0-J-550",0,5,5260,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",30.981,0.16330999999999998,0.03453,60.550000000000004,0.40800000000000003,0.034929999999999996,"FFMX10033152","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","4","CO",0.4,0.4,"010.5",{"$nulls":7},"Ford: F150 2WD FFV HD PAYLOAD GVWR 760, F150 4WD FFV HD PAYLOAD GVWR 760, F150 PICKUP 2WD FFV, F150 PICKUP 4WD FFV"]
[2016,"FOMOCO","GFMXV02.0VZS","GFMXR0105GCA","Ford","MKZ (HEV)","DC71-2.0-E-383",0,2,3876,4250,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y",11.653,0.17604,0.01478,35.76,0.34090000000000004,0.015269999999999999,"EFMX91001707","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","S2","California LEV-II SULEV","150","NMOG",0.007,0.01,"000.010",2.6000000000000003E-3,null,"Y",1.04,{"$nulls":3},"Ford: C-MAX Hybrid FWD"]
[2016,"G&K","GG1XV06.3FER","GG1XR017512C","FERRARI","F12 BERLINETTA","8089",0,6.3,3593,3893,4750,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"N","N",null,null,"N",18.71,-0.21,0.024800000000000003,49.458000000000006,0.14500000000000002,0.022000000000000002,"FG1X10044493","MFR","21","Federal fuel 2-day exhaust (w/can load)","23","CARB Phase II Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","NOX",0.028,0.05,"0.07",null,1.73,"N",{"$nulls":4},"G&K Automoitve Conversion Inc.: 2013 Ferrari F12 Berlinetta"]
[2016,"GM","GGMXD06.0398","GGMXR0260843","CHEVROLET","G3500 EXPRESS 2WD CUTAWAY CH","60PGGNT394",0,6,12070,14000,13000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",53.53,0.526,0.08673,98.9,0.8639,0.08803,"GGMX10036659","MFR","16","Hot 1435 LA92","46","CARB LEV3 E10 Regular Gasoline","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","HDV3B400","Federal Tier 3 HD Class 3 Bin 400","150","NMOG+NOX",0.11080000000000001,0.185,"99.999",0,null,"N",{"$nulls":3},1,"Chevrolet: K35 SUBURBAN 4WD"]
[2016,"GM","GGMXJ03.6165","GGMXR0133810","CADILLAC","SRX AWD","366FNE5600",0,3.6,4607,null,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",11.08,0.38930000000000003,0.022109999999999998,40.57,0.4315,0.02506,"GGMX10035187","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.005,0.01,"0.04",0.008,null,"N",{"$nulls":3},1,"Cadillac: CTS SEDAN, CTS SEDAN AWD, XTS, XTS AWD  Chevrolet: CAMARO"]
[2016,"GM","GGMXT05.3382","GGMXR0176820","GMC","K1500 YUKON XL 4WD","53XECUE034",2,5.3,6048,7500,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",30.51,0.24180000000000001,0.033159999999999995,56.59,0.7011000000000001,0.03044,"GGMX10035313","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B5","Federal Tier 2 Bin 5","150","CREE",342,342,"999.9999",0,null,"N",{"$nulls":3},1,"Chevrolet: C15 SILVERADO 2WD, C1500 TAHOE 2WD, K15 SILVERADO 4WD, K1500 TAHOE 4WD  GMC: C15 SIERRA 2WD, C1500 YUKON 2WD, K15 SIERRA 4WD, K1500 YUKON 4WD"]
[2016,"GM","GGMXT06.2374","GGMXR0223840","GMC","K1500 YUKON XL 4WD","62XECUE033",0,6.2,6003,7500,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",23.86,0.9324,0.021429999999999998,53.99,1.35,0.02088,"EGMX91001839","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","CO",0.54,0.7000000000000001,"2.1",0.16,null,"N",{"$nulls":3},1,"Cadillac: ESCALADE ESV 2WD, ESCALADE ESV 4WD  GMC: C1500 YUKON XL 2WD, K1500 YUKON XL 4WD"]
[2016,"GM","GGMXV01.4088","GGMXR0060600","CADILLAC","ELR","1464R74887",0,1.4000000000000001,4049,null,4500,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y",13.57,0.3149,0.016149999999999998,44.410000000000004,0.21350000000000002,0.0177,"GGMX10036867","MFR","95","SC03","47","CARB LEV3 E10 Premium Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","CO",0.41000000000000003,0.4,"99.9",null,null,"N",{"$nulls":3},1,"Cadillac: ELR"]
[2016,"GM","GGMXV02.4060","GGMXR0133810","BUICK","LACROSSE","244BGN4226",0,2.4,3832,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"Y",14.700000000000001,0.0785,0.015529999999999999,33.32,0.20800000000000002,0.0164,"CGMX10014353","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",3.15,3.2,"11.1",null,null,"N",{"$nulls":3},1,"Buick: LACROSSE, REGAL"]
[2016,"GM","GGMXV03.6048","GGMXR0123702","CHEVROLET","IMPALA","361EGP4200",2,3.6,3836,null,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",9.16,0.010400000000000001,0.019469999999999998,38.7,0.2752,0.0189,"GGMX10035067","MFR","95","SC03","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B85","Federal Tier 3 Transitional Bin 85","120","CO",0.16,0.2,"99.9",0,null,"N",{"$nulls":3},1,"Buick: LACROSSE  Cadillac: XTS  Chevrolet: IMPALA"]
[2016,"Honda","GHNXT03.5GV3","GHNXR01351FA","HONDA","ODYSSEY TOURING","EBV02A",0,3.5,4560,6019,5000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",5.3100000000000005,0.6217,0.01865,31.66,0.5829,0.01965,"BHNX91000603","EPA","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","NOX",0.005,0.01,"0.09",0.009000000000000001,null,"N",{"$nulls":4},"Acura: RDX 2WD, RDX 4WD"]
[2016,"Honda","GHNXV02.44K3","GHNXR0121VFA","HONDA","ACCORD L4","EGA21C",1,2.4,3397,null,3750,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,7,"Y","N",null,null,"N",15.4,0.0091,0.016819999999999998,46.17,-0.3199,0.02153,"GHNX10036980","MFR","90","US06","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B30","Federal Tier 3 Bin 30","4","NOX",0.0219,0.022000000000000002,"999.999",null,null,"N",{"$nulls":4},"Honda: ACCORD"]
[2016,"Hyundai","GHYXV01.81DE","GHYXR01051DE","Hyundai","Elantra Limited","MD4N8GF01A1",0,1.8,2870,3880,3125,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",8.25,0.18242,0.016397,30.502000000000002,0.21356,0.016527999999999998,"FHYX10031089","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","NMOG",0.0154,0.019,"0.075",3.6000000000000003E-3,null,"Y",1.04,{"$nulls":3},"HYUNDAI MOTOR COMPANY: Elantra, Elantra Limited"]
[2016,"Hyundai","GHYXV03.81NE","GHYXR01401NE","HYUNDAI","Genesis Coupe","BK6L8AU01AC",0,3.8000000000000003,3655,4409,4000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",23.916,0.11087999999999999,0.01869,46.749,0.6277699999999999,0.013977999999999999,"GHYX10034790","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","4","HC-NM+NOX",0.028,0.03,"0.14",{"$nulls":7},"HYUNDAI MOTOR COMPANY: Genesis Coupe"]
[2016,"Jaguar Land Rover L","GJLXT03.0FSP","GJLXR0175P1Z","Land Rover","Range Rover 3.0 PZEV","LKFTT220",0,3,5334,6724,5500,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-19.109,-0.48480999999999996,0.031091999999999998,46.985,-0.06280999999999999,0.032964,"FJLX10033657","MFR","95","SC03","61","Tier 2 Cert Gasoline","B","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","150","NOX",0.012,0.012,"99.999",0,null,"N",{"$nulls":4},"Land Rover: Range Rover, Range Rover LWB, Range Rover Sport"]
[2016,"Kia","GKMXV01.6DDE","GKMXR01281CE","KIA","Forte5","YD3R6AU09A1",0,1.6,3025,4056,3375,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",12.487,0.09512,0.019719999999999998,35.972,0.30882,0.018597,"EKMX91001837","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","NMOG",0.014,0.018000000000000002,"0.075",3.6000000000000003E-3,null,"Y",1.04,{"$nulls":3},"HYUNDAI MOTOR COMPANY: Veloster"]
[2016,"Kia","GKMXV03.34RE","GKMXR01354RE","Kia","Sorento","UM5L3U01AC",0,3.3000000000000003,4317,5622,4750,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",22.529,0.07969,0.02617,46.529,0.32908,0.024984,"GKMX10032743","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","4","HC-NM+NOX",0.026000000000000002,0.03,"0.20",{"$nulls":7},"KIA MOTORS CORPORATION: Sorento AWD, Sorento AWD FE, Sorento FWD"]
[2016,"Maserati","GMAXV03.0RWD","GMAXR0136DFI","MASERATI","QUATTROPORTE S V6 RWD","068553",0,3,4470,null,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",-4.496,0.406,0.017,44.287,0.12240000000000001,0.02,"GMAX10036287","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2","California LEV-II LEV","50","NOX",0.024,0.03,"0.05",2.9000000000000002E-3,{"$nulls":6},"MASERATI: Ghibli  S RWD, QUATTROPORTE S"]
[2016,"Mercedes-Benz","GMBXJ02.0U2C","GMBXR0155LNC","Mercedes-Benz","GLC 300 4MATIC","X253E20DETC-Z6015-1",0,1.991,4107,5214,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,9,"Y","N",null,null,"N",23.852,0.2687,0.022602999999999998,45.436,0.30457,0.023354,"GMBX10039060","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","NOX",0.016,0.02,"0.05",0,{"$nulls":6},"Mercedes-Benz: C 300, C 300 4MATIC, GLC 300, GLC 300 4MATIC"]
[2016,"Mercedes-Benz","GMBXJ06.0U2A","GMBXR0170LNA","Mercedes-Benz","AMG G65","G463E60TC-Z6021",0,5.98,5935,7050,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N",32.755,0.11678999999999999,0.040496,65.494,0.5838599999999999,0.040493,"GMBX10038363","MFR","95","SC03","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",0.12,0.4,"3.7",0.29,{"$nulls":6},"Mercedes-Benz: AMG S 65, AMG S 65 (coupe), Maybach S 600, S 600"]
[2016,"Mercedes-Benz","GMBXV03.0U2A","GMBXR0155LNC","Mercedes-Benz","S 400 4MATIC","V222E30DETC-Z5016-1",0,2.996,4806,null,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N",19.918,-0.09390000000000001,0.019372,40.414,0.71021,0.011313,"FMBX10031943","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","NOX",0.008,0.01,"0.07",2E-3,{"$nulls":6},"Mercedes-Benz: C 450 AMG"]
[2016,"Mercedes-Benz","GMBXV03.5U2C","GMBXR0155LNS","Mercedes-Benz","GLK 350","X204E35DEH-Z3015-1",1,3.498,4142,5225,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N",39.162,-0.43451999999999996,0.029304999999999998,60.33,0.2399,0.022673,"DMBX10021234","MFR","95","SC03","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","4","HC-NM+NOX",0.035,0.04,"0.20",{"$nulls":7},"Mercedes-Benz: SLK 350"]
[2016,"Mitsubishi Motors Co","GMTXV02.0G5P","GMTXR0135A1D","MITSUBISHI","LANCER","EB15-CA6A",0,1.998,2996,3969,3250,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)","AV-S6(w / Paddles ; 6-speed)",6,"Y","N",null,null,"N",6.45,0.0731,0.01755,33.897,-0.07177,0.020155,"FMTX10029678","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","T3B70","Federal Tier 3 Bin 70","150","NOX",6.6E-3,0.016,"999.999",0.0097,null,"N",{"$nulls":4},"Mitsubishi Motors Corporation: LANCER"]
[2016,"Nissan","GNSXT02.5G5D","GNSXR0120PBB","NISSAN","NISSAN ROGUE AWD SL","BTB096",4,2.5,3428,4486,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",6.74,-0.06420000000000001,0.027800000000000002,31.28,-0.1525,0.027800000000000002,"ENSX10027058","MFR","3","HWFE","23","CARB Phase II Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","120","NOX",0.006,0.01,"0.09",2E-3,1,{"$nulls":5},"NISSAN: ROGUE FWD"]
[2016,"Nissan","GNSXV03.8GBA","GNSXR0132MBB","NISSAN","NISSAN GT-R","MNE291",5,3.8000000000000003,3903,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",21.3,0.056100000000000004,0.01856,38.6,0.2803,0.01856,"DNSX10016378","MFR","3","HWFE","23","CARB Phase II Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","NOX",0.005,0,"0.07",0,1,{"$nulls":5},"NISSAN: GT-R"]
[2016,"Porsche","GPRXJ03.0PHV","GPRXR0200RPD","Porsche","Cayenne S e-Hybrid","ECFE-92AIIH-15",0,3,5413,6724,5500,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,8,"Y","N",null,null,"Y",30.016000000000002,0.02301,0.01737,44.962,0.12301,0.02737,"FPRX10033160","MFR","52","Fed. fuel 50 F exh.","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","CO",0.67,0.7000000000000001,"1.7",0,{"$nulls":6},"Porsche: Panamera S E-Hybrid"]
[2016,"Subaru","GFJXJ02.0FPT","GFJXR01303BA","SUBARU","FORESTER","EBE-TF15",0,2,3673,null,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",5.73,0.3699,0.02281,28.330000000000002,0.34900000000000003,0.02378,"EFJX10022619","MFR","25","California fuel 2-day exhaust (w/can load)","23","CARB Phase II Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2","California LEV-II LEV","150","HCHO",1.2000000000000001E-3,1E-3,"0.018",0.0002,{"$nulls":6},"Subaru: WRX"]
[2016,"Subaru","GFJXJ02.0FPT","GFJXR01303BA","SUBARU","FORESTER","EBE-TF15",2,2,3673,null,4000,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",5.73,0.3699,0.02281,28.330000000000002,0.34900000000000003,0.02378,"EFJX10022650","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","4","HC-NM+NOX",0.039,0.04,"0.14",{"$nulls":7},"Subaru: WRX"]
[2016,"Toyota","GTYXT02.5PCM","GTYXR0130A22","LEXUS","NX 300h AWD","15-AZ1H",0,2.494,4180,5335,4500,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"N","N",null,null,"Y",24.423000000000002,-0.19402,0.028308,39.19,0.18162,0.025845999999999997,"FTYX10029455","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG",0.0005,0.003,"999.999",0.0025,null,"Y",1.03,null,null,1,"LEXUS: NX 300h, NX 300h AWD  TOYOTA: RAV4 HYBRID AWD"]
[2016,"Toyota","GTYXT05.7BEY","GTYXR0190P32","TOYOTA","SEQUOIA 4WD","12-SK1A",0,5.663,5985,7300,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",26.34,-0.043000000000000003,0.036534,60.09,0.37781,0.036357,"CTYX10015352","MFR","95","SC03","23","CARB Phase II Gasoline","B","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","B5","Federal Tier 2 Bin 5","4","HC-NM+NOX",0.014,0.01,"0.44",null,null,"N",{"$nulls":4},"LEXUS: LX 570  TOYOTA: LAND CRUISER WAGON 4WD, SEQUOIA 2WD, SEQUOIA 4WD"]
[2016,"Toyota","GTYXV02.0KEA","GTYXR0165P12","LEXUS","GS 200t F SPORT","16-AE1A",0,1.998,3860,null,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",25.695,0.04026,0.017518,51.39,0.20126,0.017518,"GTYX10037039","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","METHANE",0.005,0.011000000000000001,"0.030",0.0061,null,"N",{"$nulls":4},"LEXUS: GS 200t, GS 200t F SPORT, IS 200t, RC 200t"]
[2016,"Volkswagen Group of","GVGAJ03.0AUD","GVGAR0140AAC","AUDI","SQ5","E3UF-SQ5",0,2.995,4432,5645,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",20.345000000000002,0.19171,0.022872999999999998,52.156000000000006,0.13384,0.025026,"FVGA10031474","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","CO",0.56,1.06,"1.70",0.5,{"$nulls":6},"Audi: S4, S5, S5 Cabriolet, SQ5"]
[2016,"Volkswagen Group of","GVGAV02.0AUB","GVGAR0140AAC","AUDI","A4","D3UB-BAF",1,1.984,3925,null,4250,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"N","N",null,null,"N",4.181,0.26044,0.017286,40.466,0.23512,0.018508,"DADX10020136","MFR","95","SC03","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","4","CO",1.17,1.17,"2.70",{"$nulls":7},"Audi: A4, A4 quattro, A5 Cabriolet, A5 quattro"]
[2016,"Volkswagen Group of","GVGAV03.6VUF","GVGAR0125VAF","VOLKSWAGEN","PASSAT CC 4MOTION","VW461 90122/09",0,3.596,3854,null,4250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N",0,0.38,0.017,42,0.47000000000000003,0.017,"9VWX01087099","MFR","95","SC03","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","4","CO",0.2,0.2,"2.70",{"$nulls":7},"Volkswagen: CC 4Motion"]
[2016,"Volvo","GVVXT02.0U3T","GVVXR0130EB2","Volvo","XC90 T6 AWD","201601",0,1.969,4745,6060,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",26.5,0.048,0.0274,50.443000000000005,0.17962999999999998,0.027462,"GVVX10034610","MFR","90","US06","47","CARB LEV3 E10 Premium Gasoline","B","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",0.86,0.98,"14.60",0.12,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: XC60 AWD"]
[2016,"Volvo","GVVXV02.0U3T","GVVXR0130EV3","Volvo","XC60 T6 FWD","201606",0,1.969,3970,5140,4250,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",15.200000000000001,0.24100000000000002,0.021500000000000002,37.481,0.29202,0.022132,"GVVX10035507","MFR","35","California fuel 3-day exhaust","47","CARB LEV3 E10 Premium Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","NMOG",0.013000000000000001,0.0188,"0.0750",5.8000000000000005E-3,null,"Y",1.04,{"$nulls":3},"Volvo Cars of North America, LLC: S60 FWD, S60 Inscription FWD, S80 FWD, V60 FWD, XC60 FWD, XC70 FWD"]
[2015,"BMW","FBMXV00.6I3R","FBMXR0035I3R","BMW","I3 REX","VX62501",0,0.6,3130,3815,3375,"R","2-Wheel Drive, Rear","A","Automatic",null,1,"N","N",null,null,"Y",6.9,-0.067,0.02022,23.7,0.34600000000000003,0.016749999999999998,"EBMX91002231","EPA","90","US06","23","CARB Phase II Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","S2","California LEV-II SULEV","4","CO",4.3500000000000005,4.4,"8.0",{"$nulls":7},"BMW: I3 REX"]
[2015,"BMW","FBMXV01.5B38","FBMXR0100F5X","Mini","Mini Cooper (5-doors)","T826907",0,1.5,2815,3750,3125,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",-0.1,0.40800000000000003,0.014709999999999999,28.3,0.156,0.01833,"FBMX91002447","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2ULEV125","California LEV-II ULEV125","50","CO",0.38,0.4,"1.7",null,1.067,{"$nulls":5},"Mini: Mini Cooper (3-doors), Mini Cooper (5-doors)"]
[2015,"BMW","FBMXV03.0F10","FBMXR0170N63","BMW","535i xDrive Gran Turismo","C200010",1,3,4708,5899,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",16.6,0.36100000000000004,0.01705,58.800000000000004,-0.269,0.02499,"BBMX10010842","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","4","CO",0.78,0.8,"8.0",{"$nulls":7},"BMW: 740Li, 740Li xDrive, 740i"]
[2015,"FCA US LLC","FCRXD05.75VY","FCRXR0272TCY","RAM","2500 Pickup 4WD","L3DJ73472",2,5.7,8353,9000,8500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",26.94,0.9742000000000001,0.03351,65.88,1.7806000000000002,0.02642,"FCRX10032320","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","M6","MDV6 (Cal. LEV 2/3 MDV GVW 8501-10000)","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","120","CO2",471,471,"999",null,1,"N",0,null,null,0,"RAM: 2500 4X4"]
[2015,"FCA US LLC","FCRXJ01.45P0","FCRXR0116PK1","Dodge","Dart","L4PFD6910",1,1.4000000000000001,3262,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"N","N",null,null,"N",-4.471,0.47350000000000003,0.0134,18.44,0.402,0.016139999999999998,"ECRX10030270","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","NOX",0.005,0,"0.07",null,1,"N",0,null,null,0,"Jeep: Renegade 4x2, Renegade 4x4"]
[2015,"FCA US LLC","FCRXJ03.65P0","FCRXR0150RK0","Chrysler","Town & Country","L4RTK1777",0,3.6,4568,6050,5000,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",8.559000000000001,0.026000000000000002,0.02712,40.56,0.4706,0.02412,"ECRX10026888","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B4","Federal Tier 2 Bin 4","120","HCHO",0,0,"0.011",0,1,"N",{"$nulls":4},"Chrysler: Town & Country  Dodge: Grand Caravan  RAM: C/V Tradesman"]
[2015,"FCA US LLC","FCRXT02.45P1","FCRXR0116PK1","Jeep","Cherokee","L4KLJ2642",3,2.4,4054,5500,4250,"F","2-Wheel Drive, Front","A","Automatic",null,9,"Y","N",null,null,"N",15.58,-0.0821,0.030039999999999997,38.980000000000004,0.3002,0.029529999999999997,"ECRX10028942","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",1.76,1.8,"3.7",null,1,"N",0,null,null,0,"Jeep: Cherokee 4x4 Active Drive II, Cherokee Trailhawk 4X4"]
[2015,"FCA US LLC","FCRXV03.65PB","FCRXR0145PKA","Chrysler","300","V2LXF8456",0,3.6,4314,5500,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",23.886000000000003,-0.032,0.021400000000000002,49.160000000000004,0.015600000000000001,0.026439999999999998,"ECRX10026501","MFR","21","Federal fuel 2-day exhaust (w/can load)","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","B4","Federal Tier 2 Bin 4","120","CO",0.51,0.5,"2.1",null,1,"N",0,null,null,0,"Chrysler: 300, 300 AWD  Dodge: Charger, Charger AWD"]
[2015,"FOMOCO","FFMXT01.62E9","FFMXR0125NBV","Ford","Escape AWD","DM21-1.6-F-222",0,1.6,3714,4770,4000,"A","All Wheel Drive","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",-3.3030000000000004,0.34154,0.022959999999999998,28.01,0.5607,0.02308,"DFMX91001249","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","120","NMOG",8.6E-3,0.009000000000000001,"000.055",0.0008,null,"Y",1.04,{"$nulls":3},"Ford: ESCAPE AWD, ESCAPE FWD"]
[2015,"FOMOCO","FFMXT02.52ET","FFMXR0125NBV","Ford","ESCAPE FWD","DM23-2.5-C-227",0,2.5,3596,4680,3875,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",2.17,0.3531,0.0224,23.81,0.5145000000000001,0.02292,"DFMX10019383","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","CO",0.63,0.8,"001.7",0.16,{"$nulls":6},"Ford: ESCAPE FWD"]
[2015,"FOMOCO","FFMXT05.03DK","FFMXR0235NBC","Ford","F-150 4X4","FFC1-5.0-J-550",0,5,5260,7850,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",30.981,0.16330999999999998,0.03453,60.550000000000004,0.40800000000000003,0.034929999999999996,"FFMX10033153","MFR","21","Federal fuel 2-day exhaust (w/can load)","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","B4","Federal Tier 2 Bin 4","120","CO",0.27,0.5,"02.1",0.24,{"$nulls":6},"Ford: F150 PICKUP 2WD FFV, F150 PICKUP 4WD FFV"]
[2015,"FOMOCO","FFMXV01.0VD1","FFMXR0105GBA","Ford","FIESTA","ECT2-1.0-J-565",1,1,2559,3620,2875,"F","2-Wheel Drive, Front","M","Manual",null,5,"N","N",null,null,"N",-0.74,0.227,0.01504,17.52,0.31880000000000003,0.01594,"EFMX10027552","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B4","Federal Tier 2 Bin 4","4","HC-NM+NOX",0.128,0.13,"000.14",{"$nulls":7},"Ford: Fiesta FWD, Fiesta SFE FWD"]
[2015,"FOMOCO","FFMXV02.0VZN","FFMXR0105GCA","Ford","MKZ (HEV)","DR805844",0,2,3876,4250,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y",13.121,0.04162,0.0171,35.76,0.34090000000000004,0.015269999999999999,"EFMX10026694","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","B3","Federal Tier 2 Bin 3","120","CO",2.72,3.4,"11.1",0.65,{"$nulls":6},"Ford: C-MAX Hybrid FWD"]
[2015,"GM","FGMXD06.6365",null,"CHEVROLET","K35 CHEV CAB CHASSIS 4WD","66C2C96074",0,6.6000000000000005,11300,13200,12000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",45.550000000000004,1.4527,0.11223999999999999,83.82000000000001,1.9126,0.11063999999999999,"DGMX10019534","MFR","2","CVS 75 and later (w/o can. load)","19","Federal Cert Diesel 7-15 PPM Sulfur","C","M7","MDV7 (Cal. LEV 2/3 MDV GVW 10001-14000)","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","120","CO",0.14,0.5,"7.3",0.36,null,"N",null,0,0,1,"Chevrolet: C35 CHEV CAB CHASSIS 2WD, C35 SILVERADO 2WD, K35 CHEV CAB CHASSIS 4WD, K35 SILVERADO 4WD  GMC: C35 GMC CAB CHASSIS 2WD, C35 SIERRA 2WD, K35 SIERRA 4WD, K35GMCCAB CHASSIS 4WD"]
[2015,"GM","FGMXJ03.6165","FGMXR0138813","CADILLAC","SRX 2WD","366CNN4028",1,3.6,4544,5555,5000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N","FF","Flex Fuel (fuel premixed and combusted together)","N",14.870000000000001,0.39640000000000003,0.02337,40.57,0.4315,0.02506,"CGMX10012785","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","B4","Federal Tier 2 Bin 4","120","CREE",551,551,"999.9999",0.3619,null,"N",{"$nulls":3},1,"Chevrolet: EQUINOX AWD, EQUINOX FWD  GMC: TERRAIN AWD, TERRAIN FWD"]
[2015,"GM","FGMXT04.3187","FGMXR0223840","CHEVROLET","K15 SILVERADO 4WD","43XECPE061",0,4.3,5566,7200,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",23.25,0.8126,0.02055,39.18,1.2781,0.01846,"EGMX10025348","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","B4","Federal Tier 2 Bin 4","4","HC-NM+NOX",0.025,0.02,"0.31",0,null,"N",{"$nulls":3},1,"Chevrolet: C15 SILVERADO 2WD, C15 SILVERADO 2WD CAB CHASSIS, K15 SILVERADO 4WD, K15 SILVERADO 4WD CAB CHASSIS  GMC: C15 SIERRA 2WD, C15 SIERRA 2WD CAB CHASSIS, K15 SIERRA 4WD, K15 SIERRA 4WD CAB CHASSIS"]
[2015,"GM","FGMXV01.4099","FGMXR0095805","BUICK","ENCORE AWD","14X3SV330A",0,1.4000000000000001,3348,null,3625,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",22.150000000000002,0.1623,0.02239,40.47,0.2629,0.02427,"DGMX10021388","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","B4","Federal Tier 2 Bin 4","4","HC-NM+NOX",0.024,0.02,"0.14",null,null,"N",{"$nulls":3},1,"Buick: ENCORE, ENCORE AWD  Chevrolet: TRAX, TRAX AWD"]
[2015,"GM","FGMXV06.0082","FGMXR0133880","CHEVROLET","CAPRICE PPV","608EEN4447",0,6,4131,null,4500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",11.75,0.3403,0.01863,35.86,0.8526,0.01521,"EGMX10027200","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B4","Federal Tier 2 Bin 4","4","HC-NM+NOX",0.038,0.04,"0.14",null,null,"N",{"$nulls":3},1,"Chevrolet: CAPRICE PPV"]
[2015,"Honda","FHNXV01.5RF2","FHNXR0106VFA","ACURA","ILX HYBRID","ED9C1C",0,1.5,3020,null,3375,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,1,"Y","N",null,null,"Y",9.620000000000001,0.1537,0.01647,30.28,0.0247,0.01969,"DHNX91001285","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","B3","Federal Tier 2 Bin 3","120","NMOG",0.006500000000000001,0.011000000000000001,"0.055",4.3E-3,null,"Y",1.04,{"$nulls":3},"Acura: ILX"]
[2015,"Hyundai","FHYXT02.01TE","FHYXR0132ATE","Hyundai","Tucson","LM4N0AU13B2",0,2,3373,4608,3750,"4","4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N",5.425,0.32611999999999997,0.02401,31.022000000000002,0.42217,0.024183,"EHYX91001816","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","CREE",341,342,"999",0.588129,{"$nulls":6},"HYUNDAI MOTOR COMPANY: Tucson AWD, Tucson FWD"]
[2015,"Hyundai","FHYXV05.01RE","FHYXR0140ARE","HYUNDAI","Genesis","DH5T0GU11A2",0,5,4724,5710,5000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",29.6,-0.35900000000000004,0.024109,64.428,-0.22768,0.024308,"FHYX10028445","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","120","CO",0.34700000000000003,0.76,"2.10",0.41000000000000003,{"$nulls":6},"HYUNDAI MOTOR COMPANY: Genesis AWD, Genesis RWD"]
[2015,"Jaguar Land Rover L","FJLXT03.0001","FJLXR0175001","Land Rover","LR4","LSETT004",0,3,5818,7143,6000,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-19.14,0.12301,0.030452,63.56,0.5129,0.030622999999999997,"EJLX10028146","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","NOX",0.02,0.03,"0.07",0.014,{"$nulls":6},"Land Rover: Land Rover LR4"]
[2015,"Jaguar Land Rover L","FJLXT05.0003","FJLXR0175001","Land Rover","Range Rover Sport","LXEVP084",3,5,5404,6724,6000,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-1.35,-0.45948,0.03412,51.71,-0.06283,0.032964,"EJLX10026624","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","CREE",530,530,"999.9999",0,{"$nulls":6},"Land Rover: Range Rover FFV, Range Rover L FFV, Range Rover Sport FFV"]
[2015,"Kia","FKMXV01.84EE","FKMXR01284EE","Kia","Forte","YD5N8GF05A1",0,1.8,2852,3880,3125,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",9.153,0.06486,0.016309999999999998,25.586000000000002,0.24725,0.015536999999999999,"FKMX10029271","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","4","HC-NM+NOX",0.016,0.02,"0.20",{"$nulls":7},"KIA MOTORS CORPORATION: Forte"]
[2015,"Kia","FKMXV02.44HE","FKMXR0140DHE","KIA","Optima","TF4F4AU24A1",0,2.4,3325,4299,3625,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",7.890000000000001,-0.0494,0.02062,30.174000000000003,0.27416,0.018201,"EKMX10026989","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","NOX",0.004,0.01,"0.07",0.005,{"$nulls":6},"KIA MOTORS CORPORATION: OPTIMA"]
[2015,"MAZDA","FTKXV02.05BB","FTKXR0125GAK","MAZDA","MX-5","0EFLFNS1-013",0,2,2632,null,3000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N","SF","Single Fuel","N",16.842000000000002,0.06754,0.020506,39.18,0.4408,0.019865999999999998,"ATKX10003142","MFR","11","Cold CO","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","120","HC-NM",0.45,0.5,"0.5",0.01,{"$nulls":6},"MAZDA: MX-5"]
[2015,"Mercedes-Benz","FMBXJ03.5U2A","FMBXR0170LNF","Mercedes-Benz","ML 350 4MATIC","W166E35DEH-Z2036",4,3.498,4914,6283,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N",22.447000000000003,0.7836000000000001,0.019965,47.898,1.4684000000000001,0.013781999999999999,"EMBX10024540","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","NOX",0.012,0.02,"0.05",0.013000000000000001,{"$nulls":6},"Mercedes-Benz: ML 350 4MATIC"]
[2015,"Mercedes-Benz","FMBXT03.5U2A","FMBXR0170LNF","Mercedes-Benz","ML 350 4MATIC","W166E35DEH-Z2036",4,3.498,4914,6283,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N",22.447000000000003,0.7836000000000001,0.019965,47.898,1.4684000000000001,0.013781999999999999,"EMBX10024541","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2","California LEV-II LEV","120","CREE",311,311,"999",0,{"$nulls":6},"Mercedes-Benz: ML 350, ML 350 4MATIC"]
[2015,"Mercedes-Benz","FMBXV03.0U2A","FMBXR0160LNF","Mercedes-Benz","S 400 4MATIC","V222E30DETC-Z5016-1",0,2.996,4806,null,5000,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N",19.918,-0.09390000000000001,0.019372,40.414,0.71021,0.011313,"FMBX10031943","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","CREE",238,238,"999",0,{"$nulls":6},"Mercedes-Benz: CLS 400, CLS 400 4MATIC, E 400, E 400 (convertible), E 400 (coupe), E 400 4MATIC, E 400 4MATIC (Wagon), E 400 4MATIC (coupe)"]
[2015,"Mercedes-Benz","FMBXV06.0U2A","FMBXR0170LNS","Mercedes-Benz","S 600","V222E60TC-Z5014",0,5.98,5124,6041,5500,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N",19.044,-0.08950999999999999,0.018911999999999998,36.869,0.72359,0.011948,"FMBX10030957","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV125","California LEV-III ULEV125","120","CREE",545,545,"999",0.3,{"$nulls":6},"Mercedes-Benz: S 600, S 65 AMG, S 65 AMG (coupe)"]
[2015,"Mitsubishi Motors Co","FMTXV02.0GEP","FMTXR0135A1D","MITSUBISHI","LANCER","EB15-CA6A",0,1.998,2996,3969,3250,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)","AV-S6(w / Paddles ; 6-speed)",6,"Y","N",null,null,"N",6.45,0.0731,0.01755,33.897,-0.07177,0.020155,"FMTX10029678","MFR","25","California fuel 2-day exhaust (w/can load)","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","NOX",6.6E-3,0.01,"0.050",0.003,null,"N",{"$nulls":4},"Mitsubishi Motors Corporation: LANCER"]
[2015,"Nissan","FNSXT05.6G9C","FNSXR0174PBC","INFINITI","INFINITI QX80 4WD","TWE232",6,5.6000000000000005,5942,7500,6000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N",8.02,0.25120000000000003,0.03251,32.32,0.9667,0.027389999999999998,"FNSX10030744","MFR","35","California fuel 3-day exhaust","23","CARB Phase II Gasoline","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","NOX",0.008,0.02,"0.07",0.016,1,{"$nulls":5},"INFINITI: QX80 2WD, QX80 4WD"]
[2015,"Nissan","FNSXT05.6G9D","FNSXR0174PBC","INFINITI","INFINITI QX80 4WD LIMITED","ABQ298",0,5.6000000000000005,6075,null,6500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N",17.31,0.3069,0.03035,38.65,0.9573,0.02614,"FNSX10033582","MFR","35","California fuel 3-day exhaust","23","CARB Phase II Gasoline","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","L2","California LEV-II LEV","120","NOX",0.018000000000000002,0.03,"0.07",0.016,1,{"$nulls":5},"INFINITI: QX80 4WD"]
[2015,"Porsche","FPRXT04.8CTD","FPRXR0230RED","Porsche","Cayenne Turbo","EC-92AIIT-15",0,4.8,5243,6382,5500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",31.608,-0.28944,0.03191,48.334,0.12301,0.029109999999999997,"FPRX10033041","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","NOX",0.021,0.02,".07",1E-3,{"$nulls":6},"Porsche: Cayenne Turbo"]
[2015,"Porsche","FPRXV04.6918","FPRXR0200RNI","Porsche","918 Spyder","ECFE-918-15",0,4.6000000000000005,3768,4189,4000,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"Y",17.625,-0.14834,0.02038,40.466,0.27135,0.01805,"FPRX10029652","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","NOX",0.028,0.03,".05",0.005,{"$nulls":6},"Porsche: 918 Spyder"]
[2015,"Subaru","FFJXJ02.5NKR","FFJXR01254CP","SUBARU","OUTBACK WAGON AWD","DBE-DL16",2,2.5,3573,null,3875,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)",null,6,"Y","N",null,null,"N",8.63,0.261,0.022269999999999998,41.63,1.9E-3,0.02617,"DFJX10018922","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","S2","California LEV-II SULEV","4","HC-NM+NOX",0.02,0,"0.2",{"$nulls":7},"Subaru: FORESTER, IMPREZA, IMPREZA SPORT, IMPREZA WAGON, XV CROSSTREK"]
[2015,"Toyota","FTYXT02.7BEN","FTYXR0165P22","TOYOTA","HIGHLANDER","14-AU1A",0,2.672,4150,5665,4500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",9.021,-0.03317,0.029047,34.096000000000004,-0.07400999999999999,0.031014,"ETYX10027081","MFR","90","US06","23","CARB Phase II Gasoline","B","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","4","CO",0.65,0.6,"10.5",null,null,"N",{"$nulls":4},"TOYOTA: HIGHLANDER"]
[2015,"Toyota","FTYXV01.3BEA","FTYXR0085P12","SCION","iQ","11-NJ1C",1,1.329,2135,null,2375,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N","SF","Single Fuel","N",6.135000000000001,-0.04713,0.020946,23.712,-0.07578,0.022272999999999998,"CTYX10014740","MFR","95","SC03","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","4","CO",0.07,0.1,"2.7",null,null,"N",{"$nulls":4},"SCION: iQ"]
[2015,"Toyota","FTYXV04.6BEA","FTYXR0190A12","LEXUS","LS 460 L AWD","09-UF1A",5,4.6080000000000005,4760,null,5000,"A","All Wheel Drive","A","Automatic",null,8,"Y","N","SF","Single Fuel","N",25.299,0.28226999999999997,0.017249999999999998,51.292,0.53166,0.016988,"ATYX10004926","MFR","90","US06","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","4","CO",0.38,0.4,"8.0",null,null,"N",{"$nulls":4},"LEXUS: LS 460, LS 460 AWD, LS 460 L, LS 460 L AWD"]
[2015,"Volkswagen Group of","FVGAJ03.0AUD","FVGAR0140NAF","AUDI","SQ5","E3UF-SQ5",0,2.995,4432,5645,4750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",20.345000000000002,0.19171,0.022872999999999998,52.156000000000006,0.13384,0.025026,"FVGA10031474","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","120","CO",0.56,1.74,"2.10",1.18,{"$nulls":6},"Audi: A6 quattro, A7 quattro"]
[2015,"Volkswagen Group of","FVGAV02.0AUB","FVGAR0140AAC","AUDI","A6 quattro","D3UB-CAQ",0,1.984,3914,null,4250,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-9.307,0.019200000000000002,0.018118,37.835,0.47348999999999997,0.019206,"DADX10020974","MFR","11","Cold CO","27","Cold CO Premium (Tier 2)","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","CO",1.1500000000000001,1.28,"10.00",0.13,{"$nulls":6},"Audi: A4, A4 quattro, A5 Cabriolet, A5 quattro"]
[2015,"Volkswagen Group of","FVGAV04.0NUA","FVGAR0155NAG","BENTLEY","Continental GT","E3UJ-BY62",0,3.9930000000000003,5543,null,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-6.16,-0.0661,0.019438999999999998,54.853,0.04883,0.022116,"EADX10028465","MFR","95","SC03","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",0.29,0.67,"3.70",0.38,{"$nulls":6},"Audi: S8"]
[2015,"Volkswagen Group of","FVGAV04.2NLB","FVGAR0140AAC","AUDI","RS5","D3UL-BSQ",0,4.163,4409,null,4750,"A","All Wheel Drive","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"Y","N",null,null,"N",-15.489,0.27686,0.018566,47.21,0.34725,0.020487,"DADX10020206","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","NOX",0.007,0.008,"0.070",1E-3,{"$nulls":6},"Audi: RS5, RS5 Cabriolet"]
[2015,"Volvo","FVVXJ02.5U3T","FVVXR0130EB2","Volvo","S60 T5 AWD","201415",0,2.4970000000000003,4095,5180,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",11.6,0.53,0.018000000000000002,43.544000000000004,0.5966199999999999,0.018567,"FVVX10028332","MFR","95","SC03","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",0.32,0.51,"3.70",0.19,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: XC60 AWD"]
[2014,"aston martin","EASXV04.7VH2","EASXR0160P1Y","Aston Martin","V8 VANTAGE S","270TT244",0,4.7,3822,4420,4000,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,7,"Y","N",null,null,"N",22.05,0.4056,0.0239,45.78,0.0008,0.0217,"BASX10021220","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2","California LEV-II LEV","120","CO",1.56,2.6,"3.7",1.0130000000000001,{"$nulls":6},"Aston Martin Lagonda Ltd: V8 Vantage, V8 Vantage S"]
[2014,"Audi","EADXV04.03UJ","EADXR0155D4A","BENTLEY","Continental GT","D3UJ-BY62",0,3.9930000000000003,5543,null,6000,"A","All Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-6.205,-0.08030000000000001,0.019323,54.853,0.04883,0.022116,"DADX10019666","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","NOX",0.038,0.041,"0.050",0.003,{"$nulls":6},"Audi: A8, A8L"]
[2014,"Auto Gas America","EAGTT06.2374","EAGTR0223840","CHEVROLET","SILVERADO","3GCUKSEJ5EG307790",0,6.2,5452,7200,6500,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N",17.88,0.0614,0.0339,41.9,0.7108,0.029849999999999998,"FAGT10031706","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.02,0.03,"0.04",0.014,null,"N",{"$nulls":4},"Auto Gas America: Cadillac ESCALADE ESV 2WD, Cadillac ESCALADE ESV 4WD, GMC C1500 YUKON XL 2WD, GMC K1500 YUKON XL AWD"]
[2014,"BMW","EBMXT04.4F15","EBMXR0170N63","BMW","X5 xDrive50i","LL67500",0,4.4,5379,6327,5500,"A","All Wheel Drive","A","Automatic",null,8,"Y","N",null,null,"N",20.6,0.161,0.02634,67.2,-0.24,0.031709999999999995,"BBMX10007859","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDT4","LDT4 (ALVW > 5750, LVW 0-3750, GVW > 6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",0.46,0.7000000000000001,"6.4",null,1.4280000000000002,{"$nulls":5},"BMW: X5 xDrive50i, X6 xDrive50i"]
[2014,"BMW","EBMXV06.0N74","EBMXR0170N63","BMW","760Li","CY40013",3,6,5015,6065,5250,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",18.1,0.14600000000000002,0.01806,55.5,1E-3,0.020409999999999998,"DBMX10021744","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","4","CO",0.3,0.3,"8.0",{"$nulls":7},"BMW: 760Li"]
[2014,"FCA US LLC","ECRXJ02.45P1","ECRXR0130PK0","Dodge","Journey","L1JCD8789",2,2.4,3821,5005,4250,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N","SF","Single Fuel","N",-0.23,0.43610000000000004,0.02412,34.910000000000004,0.49400000000000005,0.02485,"BCRX10014341","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B4","Federal Tier 2 Bin 4","150","NMOG",0.0273,0.027,"0.070",null,1,"Y",1.04,{"$nulls":3},"Chrysler: 200, 200 Convertible  Dodge: Avenger"]
[2014,"FCA US LLC","ECRXT02.45P2","ECRXR0112PK0","Jeep","Patriot 4WD","V0MKJ6992",2,2.4,3378,4575,3750,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",14.120000000000001,0.1327,0.024579999999999998,67.11,-0.5052,0.03338,"ECRX10023780","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT1","LDT1 (LVW-3750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","150","NMOG",0.0337,0.034,"0.070",null,1,"Y",1.04,null,null,0,"Jeep: Compass 4X4, Patriot 4X4"]
[2014,"FCA US LLC","ECRXV01.45P0","ECRXR0116PK0","Dodge","Dart","N2PFD9054",2,1.4000000000000001,3254,4285,3625,"F","2-Wheel Drive, Front","AM","Automated Manual",null,6,"N","N",null,null,"N",3.121,0.2378,0.01672,30.400000000000002,0.2464,0.01822,"ECRX10024774","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",1.09,1.1,"11.1",null,1,"N",0,{"$nulls":3},"Dodge: Dart, Dart Aero  FIAT: 500L, 500L Trekking"]
[2014,"FCA US LLC","ECRXV02.05PA","ECRXR0116PKA","Dodge","Dart","L4PFD6870",0,2,3252,4285,3500,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",19.802,-0.016,0.01772,38.32,0.1579,0.01797,"ECRX10026701","MFR","21","Federal fuel 2-day exhaust (w/can load)","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","B4","Federal Tier 2 Bin 4","120","METHANE",0.029900000000000003,0.03,".030",0,1,"N",{"$nulls":4},"Dodge: Dart"]
[2014,"Ferrari","EFEXV04.3GDI","EFEXR0175149","Ferrari","458 Italia Spyder","171765",0,4.5,3495,4046,3875,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"N","N",null,null,"N",14.599,0.128,0.02,44.063,0.199,0.02,"DFEX10020160","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2","California LEV-II LEV","50","NMOG",0.035,0.037000000000000005,"0.075",1.8000000000000002E-3,{"$nulls":6},"Ferrari North America, Inc.: 458 Italia, 458 Speciale, 458 Spider, Ferrari California"]
[2014,"FOMOCO","EFMXT03.73DP","EFMXR0265NBV","Ford","F-150 FFV 4X4 Supercab","BF61-3.7-J-055",0,3.7,5398,6900,5500,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N",12.632000000000001,0.53782,0.03091,46.83,0.7658,0.03132,"BFMX10010635","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","OPT-CREE",324,325,"999.99",1.2,{"$nulls":6},"Ford: F150 PICKUP 2WD FFV, F150 PICKUP 4WD FFV"]
[2014,"FOMOCO","EFMXV01.5VZ1","EFMXR0130NBX","Ford","Fusion FWD","EC73-1.5-C-488",0,1.5,3468,3750,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",5.481,0.29453,0.015569999999999999,26.46,0.5437000000000001,0.01539,"EFMX10024662","MFR","90","US06","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B3","Federal Tier 2 Bin 3","120","CO",0.75,0.8,"11.1",0,{"$nulls":6},"Ford: FUSION FWD"]
[2014,"FOMOCO","EFMXV02.0VZN","EFMXR0105GDA","Ford","MKZ (HEV)","DR805844",0,2,3876,4250,4250,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y",13.121,0.04162,0.0171,35.76,0.34090000000000004,0.015269999999999999,"EFMX10026695","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B3","Federal Tier 2 Bin 3","120","CO",1.98,2.6,"003.7",0.65,{"$nulls":6},"Ford: FUSION HYBRID FWD  Lincoln: MKZ HYBRID FWD"]
[2014,"GM","EGMXJ02.4199","EGMXR0120818","GMC","1LJ26","241ALN1528",0,2.4,4076,5070,4500,"A","All Wheel Drive","A","Automatic",null,6,"Y","N","SF","Single Fuel","N",10.700000000000001,0.663,0.0193,37.19,0.5967,0.02234,"AGMX91000114","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.027,0.03,"0.04",null,null,"N",{"$nulls":3},1,"Buick: VERANO"]
[2014,"GM","EGMXT04.3187","EGMXR0176820","CHEVROLET","K15 SILVERADO 4WD","43XECPE061",0,4.3,5566,7200,6000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",23.25,0.8126,0.02055,39.18,1.2781,0.01846,"EGMX10025651","MFR","31","Federal fuel 3-day exhaust","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","CA","California + CAA Section 177 states","B4","Federal Tier 2 Bin 4","120","NMOG",0.024900000000000002,0.033,"0.070",0.0079,null,"Y",1.04,null,null,1,"Chevrolet: C15 SILVERADO 2WD, K15 SILVERADO 4WD  GMC: C15 SIERRA 2WD, K15 SIERRA 4WD"]
[2014,"GM","EGMXT05.3382","EGMXR0223840","GMC","K1500 YUKON XL 4WD","53XECUE034",0,5.3,5970,7500,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",29.12,0.2995,0.031779999999999996,56.59,0.7011000000000001,0.03044,"EGMX10024001","MFR","31","Federal fuel 3-day exhaust","38","E85 (85% Ethanol 15% EPA Unleaded Gasoline)","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","HCHO",0.0005,1E-3,"0.011",3.0000000000000003E-4,null,"N",{"$nulls":3},1,"Chevrolet: C15 SILVERADO 2WD, C1500 SUBURBAN 2WD, K15 SILVERADO 4WD, K1500 SUBURBAN 4WD  GMC: C15 SIERRA 2WD, C1500 YUKON XL 2WD, K15 SIERRA 4WD, K1500 YUKON XL 4WD"]
[2014,"GM","EGMXV02.0350",null,"CHEVROLET","CRUZE","201EPV4201",0,2,3481,null,3750,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",7.8100000000000005,0.17880000000000001,0.01457,30.19,0.5273,0.01164,"EGMX10023943","MFR","95","SC03","19","Federal Cert Diesel 7-15 PPM Sulfur","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3LEV160","California LEV-III LEV160","150","NMOG+NOX",0.017,0.02,"99.999",null,null,"N",null,0,0,null,"Chevrolet: CRUZE"]
[2014,"GM","EGMXV06.2089","EGMXR0133880","CHEVROLET","CAMARO","628DEN2313",0,6.2,4215,null,4500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",15.81,0.3239,0.01771,39.61,0.8408,0.0143,"DGMX10019346","MFR","95","SC03","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B4","Federal Tier 2 Bin 4","4","HC-NM+NOX",0.052000000000000005,0.05,"0.20",null,null,"N",{"$nulls":3},1,"Chevrolet: CAMARO"]
[2014,"Honda","EHNXT03.5N44","EHNXR01632FA","HONDA","RIDGELINE","ECJE1A",0,3.5,4610,null,5000,"F","2-Wheel Drive, Front","A","Automatic",null,5,"Y","N",null,null,"N",7.05,0.3215,0.032029999999999996,33.68,0.7413000000000001,0.02989,"CHNX10016520","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","CREE",460,460,"999.9999",0.2388,null,"N",{"$nulls":4},"Honda: RIDGELINE 4WD"]
[2014,"Honda","EHNXV02.0ZG2","EHNXR0129VGA","HONDA","ACCORD HYBRID","EEK12C",1,2,3620,null,3875,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"Y",5.65,-0.0458,0.01803,22.240000000000002,0.0046,0.01846,"EHNX10026044","MFR","3","HWFE","46","CARB LEV3 E10 Regular Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3SULEV30","California LEV-III SULEV30","150","NMOG+NOX",1E-3,0.005,"0.030",3.6000000000000003E-3,null,"Y",1.1,{"$nulls":3},"Honda: ACCORD"]
[2014,"Hyundai","EHYXV02.01VE","EHYXR0130AVE","Hyundai","Santa Fe Sport","AN4F0HU41A5",0,2,3878,5181,4250,"4","4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N",17.133,0.25949,0.025738,38.865,0.49102999999999997,0.023330999999999998,"EHYX10026788","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","CO",0.153,0.24,"3.40",0.09,{"$nulls":6},"HYUNDAI MOTOR COMPANY: Santa Fe Sport 2WD, Santa Fe Sport 4WD"]
[2014,"IMPCO","EZ9XT05.3BC1","EZ9XR0223BC3","Chevrolet","Silverado 1500 2WD Crew Cab LT","113361",2,5.3,6300,null,6500,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",38.619,0.18230000000000002,0.033187999999999995,56.09,0.6234000000000001,0.03091,"AZ9X10023120","MFR","3","HWFE","41","CNG","B","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0,0.01,".05",0.014,null,"N",{"$nulls":4},"IMPCO Automotive - Chevrolet: Chev C10 Avalanche 2WD, Chev C10 Suburban 2WD, Chev K10 Avalanche 4WD, Chev K10 Suburban 4WD  IMPCO Automotive - General Motors: GMC C10 Yukon XL 2WD, GMC K10 Yukon XL 4WD"]
[2014,"Jaguar Land Rover L","EJLXV03.0FSF","EJLXR0160P1Y","Jaguar","XJL 3.0 FFV","KBS6TT34",2,3,4155,5148,4500,"4","4-Wheel Drive","SA","Semi-Automatic",null,8,"Y","N",null,null,"N",-11.24,0.3582,0.013391,43.13,0.3779,0.016326,"EJLX10027249","MFR","90","US06","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","4","HC-NM+NOX",0.027,0.03,"0.14",0,null,"N",{"$nulls":4},"Jaguar: XF FFV, XJ FFV, XJL FFV"]
[2014,"Kia","EKMXV01.8DEE","EKMXR01051DE","KIA","Forte ECO","YD3N8GF23A1",0,1.8,2820,3880,3125,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",10.005,-0.47900000000000004,0.023,29.499000000000002,0.20770999999999998,0.016331,"EKMX91001676","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","NMOG",0.018869999999999998,0.022500000000000003,"0.0400",3.6000000000000003E-3,null,"Y",1.04,{"$nulls":3},"HYUNDAI MOTOR COMPANY: Elantra, Elantra Limited"]
[2014,"Maserati","EMAXV03.8DFI","EMAXR0136DFI","MASERATI","QUATTROPORTE GTS","066158",0,3.8000000000000003,4495,null,4750,"R","2-Wheel Drive, Rear","A","Automatic",null,8,"Y","N",null,null,"N",4.7,0.48400000000000004,0.033,44.287,0.12240000000000001,0.02,"EMAX10025837","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",0.59,0.9,"4.2",0.29,{"$nulls":6},"MASERATI: QUATTROPORTE GTS"]
[2014,"MAZDA","ETKXV02.5NC1","ETKXR0125GAX","MAZDA","MAZDA6","4ECPYS1-010",2,2.5,3232,4288,3500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",9.481,-0.04035,0.017762,27.144000000000002,0.1385,0.017218999999999998,"ETKX10025225","MFR","25","California fuel 2-day exhaust (w/can load)","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","S2","California LEV-II SULEV","120","OPT-CREE",292,292,"999.9999",0,{"$nulls":6},"MAZDA: MAZDA 6"]
[2014,"Mercedes-Benz","EMBXV01.0U2A","EMBXR0085LNC","Mercedes-Benz","smart ForTwo (convertible)","A451E10-Z8010",1,0.999,1850,2125,2125,"R","2-Wheel Drive, Rear","AM","Automated Manual",null,5,"N","N","SF","Single Fuel","N",7.102,0.2228,0.018993,21.196,0.32881,0.018504,"9MBX10004041","MFR","95","SC03","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",0.8200000000000001,1.1,"3.7",0.27,{"$nulls":6},"Mercedes-Benz: Smart fortwo (COUPE), Smart fortwo (Convertible)"]
[2014,"Mercedes-Benz","EMBXV03.5U2B","EMBXR0160LNF","Mercedes-Benz","E 350 4MATIC (coupe)","C207E35DEH-Z4025-4",0,3.498,4055,4883,4250,"R","2-Wheel Drive, Rear","A","Automatic",null,7,"Y","N",null,null,"N",33.766,-0.2746,0.019441,48.564,0.32733999999999996,0.014258999999999999,"EMBX10025169","MFR","90","US06","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",1.68,1.9000000000000001,"11.1",0.18,{"$nulls":6},"Mercedes-Benz: C 300 4MATIC, E 350 4MATIC (coupe)"]
[2014,"Mitsubishi Motors Co","EMTXV02.0GRB","EMTXR0135A1C","MITSUBISHI","LANCER EVOLUTION","EB12-CA83",0,1.998,3664,4542,4000,"A","All Wheel Drive","AM","Automated Manual",null,6,"Y","N","SF","Single Fuel","N",7.65,0.184,0.021928,43.512,0.50916,0.019934999999999998,"CMTX10014378","MFR","25","California fuel 2-day exhaust (w/can load)","23","CARB Phase II Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","CO",0.5630000000000001,0.65,"3.40",0.09,null,"N",{"$nulls":4},"Mitsubishi Motors Corporation: LANCER, LANCER EVOLUTION, LANCER SPORTBACK"]
[2014,"Mitsubishi Motors Co","EMTXV02.4GRB","EMTXR0135A1D","MITSUBISHI","LANCER SPORTBACK","EB11-CB5C",1,2.359,3175,4190,3500,"F","2-Wheel Drive, Front","SCV","Selectable Continuously Variable (e.g. CVT with paddles)","AV-S6(w / Paddles ; 6-speed)",6,"N","N",null,null,"N",36.281,0.42364999999999997,0.019320999999999998,48.174,-0.19505999999999998,0.025549,"BMTX10007337","MFR","11","Cold CO","27","Cold CO Premium (Tier 2)","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L2","California LEV-II LEV","120","HC-NM",0.18,0.2,"0.3",0.011300000000000001,null,"N",{"$nulls":4},"Mitsubishi Motors Corporation: LANCER, LANCER AWD, LANCER SPORTBACK"]
[2014,"Nissan","ENSXV01.6G4A","ENSXR0070PBA","NISSAN","NISSAN VERSA S","HKA402",0,1.6,2426,null,2750,"F","2-Wheel Drive, Front","A","Automatic",null,4,"Y","N",null,null,"N",3.36,0.248,0.01522,21.54,0.2651,0.01602,"DNSX10020976","MFR","35","California fuel 3-day exhaust","23","CARB Phase II Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","CO",0.41000000000000003,0.4,"3.4",0.01,1,{"$nulls":5},"NISSAN: VERSA"]
[2014,"Nissan","ENSXV03.7GAA","ENSXR0120MBA","INFINITI","INFINITI G37x Coupe AWD","MLE432",0,3.7,3906,null,4250,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,7,"Y","N",null,null,"N",12.92,0.2766,0.0171,34.52,0.5726,0.015629999999999998,"ENSX91001703","EPA","25","California fuel 2-day exhaust (w/can load)","23","CARB Phase II Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","120","NOX",0.016,0.03,"0.07",0.012,1,{"$nulls":5},"INFINITI: Q50, Q50 AWD, Q50a, Q50a AWD, Q60 AWD Coupe, Q60 Coupe, Q70  NISSAN: 370Z, 370Z Roadster"]
[2014,"Porsche","EPRXV04.8PSD","EPRXR0200RPD","Porsche","Panamera GTS","ECFE-970IIGTS-14",0,4.8,4385,5512,4750,"R","2-Wheel Drive, Rear","AMS","Automated Manual- Selectable (e.g. Automated Manual with paddles)",null,7,"N","N",null,null,"N",-7.284000000000001,-0.0796,0.02224,28.776,0.36179,0.01627,"EPRX10026547","MFR","11","Cold CO","25","Cold CO Premium (CERT)","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","CO",0.88,0.9,"10.0",0,{"$nulls":6},"Porsche: Panamera GTS"]
[2014,"RUF","ERAXV03.8T12","ERAXR0110T12","RUF","TURBO 12/CTR 3","TURBO 12/CTR 3",0,3.8000000000000003,3315,null,3750,"F","2-Wheel Drive, Front","A","Automatic",null,7,"N","N",null,null,"N",16.299,-0.11721999999999999,0.020669999999999997,37.094,0.32561999999999997,0.0177,"9RAX10031326","MFR","3","HWFE","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","NOX",0.008,0.02,"0.09",0.014,null,"N",{"$nulls":4},"RUF Automobile GmbH: RUFTURBO12/CTR3"]
[2014,"Subaru","EFJXJ03.6WFJ","EFJXR01443DS","SUBARU","OUTBACK AWD","KBE-JA96",0,3.6,3662,4695,4000,"F","2-Wheel Drive, Front","A","Automatic",null,5,"Y","N","SF","Single Fuel","N",2.89,0.4229,0.021502999999999998,27.16,0.8079000000000001,0.017582999999999998,"AFJX91000148","EPA","3","HWFE","23","CARB Phase II Gasoline","C","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","150","OPT-CREE",264,264,"999.999",0,{"$nulls":6},"Subaru: LEGACY AWD, OUTBACK AWD"]
[2014,"Toyota","ETYXT03.5CC4","ETYXR0160E52","LEXUS","RX 450h AWD","10-GL3H",0,3.456,4810,5980,5000,"A","All Wheel Drive","CVT","Continuously Variable",null,1,"N","N","HV","Hybrid","Y",16.761,0.19646999999999998,0.023348999999999998,38.269,0.20331,0.026380999999999998,"ATYX91000026","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B3","Federal Tier 2 Bin 3","120","NMOG",4.8000000000000004E-3,0.007,"0.055",2E-3,null,"Y",1.04,null,null,1,"LEXUS: RX 450h, RX 450h AWD"]
[2014,"Toyota","ETYXV01.8MEA","ETYXR0115P12","TOYOTA","COROLLA LE ECO","14-ZE1C",0,1.798,2855,null,3125,"F","2-Wheel Drive, Front","CVT","Continuously Variable",null,1,"Y","N",null,null,"N",7.165,-0.00477,0.019136,29.814,-0.0833,0.021412,"ETYX10025044","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","L3ULEV70","California LEV-III ULEV70","150","NOX",0.01,0.014,"999.999",0.004200000000000001,null,"N",{"$nulls":4},"TOYOTA: COROLLA LE ECO"]
[2014,"Volkswagen","EVWXJ02.03UA","EVWXR0125241","VOLKSWAGEN","Tiguan","VW316 20145",0,1.984,3710,null,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",24.055,0.34363,0.023628999999999997,42.039,0.47023,0.023746,"DVWX10020405","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","METHANE",2.9000000000000002E-3,0.014,"0.030",0.0106,{"$nulls":6},"Volkswagen: TIGUAN, TIGUAN 4MOTION"]
[2014,"Volkswagen","EVWXV02.5A59","EVWXR0110237","VW","Jetta","VW36100220",0,2.48,3319,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N",-2,0.203,0.0176,33,0.29300000000000004,0.0171,"BVWX91000666","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B3","Federal Tier 2 Bin 3","120","CREE",331,331,"999.9999",0.2,{"$nulls":6},"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volkswagen","EVWXV02.5M59","EVWXR0110237","VW","Jetta","VW36100220",0,2.48,3319,null,3625,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N","SF","Single Fuel","N",-2,0.203,0.0176,33,0.29300000000000004,0.0171,"BVWX91000666","EPA","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B3","Federal Tier 2 Bin 3","120","METHANE",2.6000000000000003E-3,0.003,"0.030",3.0000000000000003E-4,{"$nulls":6},"Volkswagen: BEETLE, BEETLE CONVERTIBLE, GOLF, JETTA SPORTWAGEN, Jetta"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020353","MFR","35","California fuel 3-day exhaust","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","HC-TOTAL",0.012,0.02,"0.410",0.008,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020353","MFR","35","California fuel 3-day exhaust","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","NMOG",0.008400000000000001,0.0134,"0.0750",0.005,null,"N",1.04,null,null,1,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020353","MFR","35","California fuel 3-day exhaust","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","NOX",0.018000000000000002,0.022000000000000002,"0.050",0.004,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020354","MFR","3","HWFE","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","120","NOX",0.006,0.018000000000000002,"0.090",0.012,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020354","MFR","3","HWFE","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","NOX",0.006,0.01,"0.070",0.004,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020354","MFR","3","HWFE","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","CREE",251,251,"999.999",null,1,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020354","MFR","3","HWFE","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","NOX",0.006,0.018000000000000002,"0.090",0.012,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020354","MFR","3","HWFE","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","NOX",0.006,0.01,"0.070",0.004,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020355","MFR","90","US06","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","4","CO",0.3,0.3,"8.00",0,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020355","MFR","90","US06","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","4","HC-NM+NOX",0.0291,0.029,"0.140",0,null,"N",{"$nulls":3},1,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020355","MFR","90","US06","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",0.3,0.49,"11.10",0.19,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020355","MFR","90","US06","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","4","CO",0.3,0.3,"8.00",0,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020355","MFR","90","US06","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","4","HC-NM+NOX",0.0291,0.029,"0.140",0,null,"N",{"$nulls":3},1,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020355","MFR","90","US06","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","CO",0.3,0.36,"9.00",0.06,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020356","MFR","95","SC03","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","4","CO",0.31,0.31,"2.70",0,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020356","MFR","95","SC03","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","4","HC-NM+NOX",0.013000000000000001,0.013000000000000001,"0.200",0,null,"N",{"$nulls":3},1,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020356","MFR","95","SC03","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",0.31,0.5,"3.70",0.19,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020356","MFR","95","SC03","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","4","CO",0.31,0.31,"2.70",0,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020356","MFR","95","SC03","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","4","HC-NM+NOX",0.013000000000000001,0.013000000000000001,"0.200",0,null,"N",{"$nulls":3},1,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020356","MFR","95","SC03","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","CO",0.31,0.37,"3.00",0.06,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",23.8,0.385,0.0181,59.04,0.38980000000000004,0.01941,"DVVX10020357","MFR","11","Cold CO","24","Cold CO Regular (CERT)","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","120","HC-NM",0.11,0.1,"0.3",0.0152,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",23.8,0.385,0.0181,59.04,0.38980000000000004,0.01941,"DVVX10020357","MFR","11","Cold CO","24","Cold CO Regular (CERT)","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","CO",0.72,0.78,"10.00",0.06,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",23.8,0.385,0.0181,59.04,0.38980000000000004,0.01941,"DVVX10020357","MFR","11","Cold CO","24","Cold CO Regular (CERT)","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","HC-NM",0.11,0.1,"0.3",0.0152,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",23.8,0.385,0.0181,59.04,0.38980000000000004,0.01941,"DVVX10020357","MFR","11","Cold CO","24","Cold CO Regular (CERT)","B","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","CO",0.72,0.78,"10.00",0.06,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020358","MFR","51","CA fuel 50 Deg(F) exhaust test","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","CO",0.35000000000000003,0.35000000000000003,"1.70",0,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020358","MFR","51","CA fuel 50 Deg(F) exhaust test","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","NMOG",0.026500000000000003,0.026500000000000003,"0.0800",0,null,"N",1.04,null,null,1,"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Volvo","EVVXV02.5U3T","EVVXR0130ET3","Volvo","S60 T5 AWD","201306",0,2.4970000000000003,3651,4770,4000,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",20.6,0.384,0.016300000000000002,53.14,0.3508,0.01747,"DVVX10020358","MFR","51","CA fuel 50 Deg(F) exhaust test","23","CARB Phase II Gasoline","B","LDV","LDV/Passenger Car","CA","California + CAA Section 177 states","U2","California LEV-II ULEV","50","NOX",0.014,0.014,"0.050",0,null,"N",{"$nulls":4},"Volvo Cars of North America, LLC: S60 AWD, S60 FWD"]
[2014,"Westport ","EBAFD05.4AFD","EBAFR0000001","Ford","E350","E3715",0,5.4,8500,null,10000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N",96.87,1.32266,0.06673,65.86,0.44938,0.07289,"CBAF10027704","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","CO",1.3,1.9000000000000001,"4.2",0.6,{"$nulls":6},"BAF Technologies: E350 Cutaway"]
[2014,"Westport ","EBAFD05.4AFD","EBAFR0000001","Ford","E350","E3715",0,5.4,8500,null,10000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N",96.87,1.32266,0.06673,65.86,0.44938,0.07289,"CBAF10027704","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","HC-NM",0.007,0.037000000000000005,"0.125",0.03,null,"Y",1.5,{"$nulls":3},"BAF Technologies: E350 Cutaway"]
[2014,"Westport ","EBAFD05.4AFD","EBAFR0000001","Ford","E350","E3715",0,5.4,8500,null,10000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N",96.87,1.32266,0.06673,65.86,0.44938,0.07289,"CBAF10027704","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","NOX",0.11,0.2,"0.2",0.04,{"$nulls":6},"BAF Technologies: E350 Cutaway"]
[2014,"Westport ","EBAFD05.4AFD","EBAFR0000001","Ford","E350","E3715",0,5.4,8500,null,10000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N",96.87,1.32266,0.06673,65.86,0.44938,0.07289,"CBAF10027704","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","CO",1.3,1.5,"3.4",0.2,{"$nulls":6},"BAF Technologies: E350 Cutaway"]
[2014,"Westport ","EBAFD05.4AFD","EBAFR0000001","Ford","E350","E3715",0,5.4,8500,null,10000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N",96.87,1.32266,0.06673,65.86,0.44938,0.07289,"CBAF10027704","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","HC-NM",0.007,0.019,"0.100",0.012,null,"Y",1.5,{"$nulls":3},"BAF Technologies: E350 Cutaway"]
[2014,"Westport ","EBAFD05.4AFD","EBAFR0000001","Ford","E350","E3715",0,5.4,8500,null,10000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N",96.87,1.32266,0.06673,65.86,0.44938,0.07289,"CBAF10027704","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","NOX",0.108,0.13,"0.14",0.02,{"$nulls":6},"BAF Technologies: E350 Cutaway"]
[2014,"Westport ","EBAFD05.4AFD","EBAFR0000001","Ford","E350","E3715",0,5.4,8500,null,10000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N",96.87,1.32266,0.06673,65.86,0.44938,0.07289,"CBAF10027705","MFR","3","HWFE","41","CNG","C","HDV2","HDV2 (Federal HD chassis Class 3 GVW 10001-14000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","NOX",0.005,0.005,"0.266",{"$nulls":7},"BAF Technologies: E350 Cutaway"]
[2014,"Westport ","EBAFT03.73DP","EBAFR0000001","Ford","F150","D13533",0,3.7,6000,null,7000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",12.632000000000001,0.53782,0.03091,46.83,0.7658,0.03132,"DBAF10027688","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","CO",0.45,0.4,"2.1",{"$nulls":7},"BAF Technologies: F150"]
[2014,"Westport ","EBAFT03.73DP","EBAFR0000001","Ford","F150","D13533",0,3.7,6000,null,7000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",12.632000000000001,0.53782,0.03091,46.83,0.7658,0.03132,"DBAF10027688","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","HC-NM",0.005,0,"0.07",null,null,"Y",1.5,{"$nulls":3},"BAF Technologies: F150"]
[2014,"Westport ","EBAFT03.73DP","EBAFR0000001","Ford","F150","D13533",0,3.7,6000,null,7000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",12.632000000000001,0.53782,0.03091,46.83,0.7658,0.03132,"DBAF10027688","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.022000000000000002,0.02,"0.04",{"$nulls":7},"BAF Technologies: F150"]
[2014,"Westport ","EBAFT03.73DP","EBAFR0000001","Ford","F150","D13533",0,3.7,6000,null,7000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",12.632000000000001,0.53782,0.03091,46.83,0.7658,0.03132,"DBAF10027689","MFR","3","HWFE","41","CNG","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.005,0.005,"0.053",{"$nulls":7},"BAF Technologies: F150"]
[2014,"Westport ","EBAFT03.7NGD","EBAFR0265NBV","Ford","F150 Super Cab 4x4 (2014 MY)","1FTEX1EM4EFB27373",0,3.7,5398,6900,5500,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N",13.33,0.7362000000000001,0.02871,46.83,0.7658,0.03132,"ENAT10033326","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","CO",0.61,0.9,"2.1",0.29,{"$nulls":6},"BAF_Bifuel: F150 2WD and 4WD"]
[2014,"Westport ","EBAFT03.7NGD","EBAFR0265NBV","Ford","F150 Super Cab 4x4 (2014 MY)","1FTEX1EM4EFB27373",0,3.7,5398,6900,5500,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N",13.33,0.7362000000000001,0.02871,46.83,0.7658,0.03132,"ENAT10033326","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NMOG",6.8000000000000005E-3,0.019,"0.070",0.0123,null,"Y",1.5,{"$nulls":3},"BAF_Bifuel: F150 2WD and 4WD"]
[2014,"Westport ","EBAFT03.7NGD","EBAFR0265NBV","Ford","F150 Super Cab 4x4 (2014 MY)","1FTEX1EM4EFB27373",0,3.7,5398,6900,5500,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N",13.33,0.7362000000000001,0.02871,46.83,0.7658,0.03132,"ENAT10033326","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.011000000000000001,0.02,"0.04",0.014,{"$nulls":6},"BAF_Bifuel: F150 2WD and 4WD"]
[2014,"Westport ","EBAFT03.7NGD","EBAFR0265NBV","Ford","F150 Super Cab 4x4 (2014 MY)","1FTEX1EM4EFB27373",0,3.7,5398,6900,5500,"P","Part-time 4-Wheel Drive","A","Automatic",null,6,"Y","N",null,null,"N",13.33,0.7362000000000001,0.02871,46.83,0.7658,0.03132,"ENAT10033327","MFR","3","HWFE","41","CNG","C","LDT3","LDT3 (ALVW 3751-5750, LVW 0-3750, GVW > 6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",2E-3,0.02,"0.05",0.014,{"$nulls":6},"BAF_Bifuel: F150 2WD and 4WD"]
[2014,"Westport ","EBAFT05.45HK","EBAFR0000001","Ford","E250","E6345",0,5.4,6500,null,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N",35.19,0.12050000000000001,0.0454,75.07000000000001,0.6802,0.09441999999999999,"CBAF10027684","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B6","Federal Tier 2 Bin 6","120","CO",0.37,0.4,"4.2",{"$nulls":7},"BAF Technologies: Ford E-Series Van"]
[2014,"Westport ","EBAFT05.45HK","EBAFR0000001","Ford","E250","E6345",0,5.4,6500,null,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N",35.19,0.12050000000000001,0.0454,75.07000000000001,0.6802,0.09441999999999999,"CBAF10027684","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B6","Federal Tier 2 Bin 6","120","HC-NM",0.003,0,"0.09",null,null,"Y",1.5,{"$nulls":3},"BAF Technologies: Ford E-Series Van"]
[2014,"Westport ","EBAFT05.45HK","EBAFR0000001","Ford","E250","E6345",0,5.4,6500,null,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N",35.19,0.12050000000000001,0.0454,75.07000000000001,0.6802,0.09441999999999999,"CBAF10027684","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B6","Federal Tier 2 Bin 6","120","NOX",0.07,0.1,"0.1",{"$nulls":7},"BAF Technologies: Ford E-Series Van"]
[2014,"Westport ","EBAFT05.45HK","EBAFR0000001","Ford","E250","E6345",0,5.4,6500,null,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N",35.19,0.12050000000000001,0.0454,75.07000000000001,0.6802,0.09441999999999999,"CBAF10027684","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B6","Federal Tier 2 Bin 6","50","CO",0.37,0.4,"3.4",{"$nulls":7},"BAF Technologies: Ford E-Series Van"]
[2014,"Westport ","EBAFT05.45HK","EBAFR0000001","Ford","E250","E6345",0,5.4,6500,null,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N",35.19,0.12050000000000001,0.0454,75.07000000000001,0.6802,0.09441999999999999,"CBAF10027684","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B6","Federal Tier 2 Bin 6","50","HC-NM",0.003,0.003,"0.075",null,null,"Y",1.5,{"$nulls":3},"BAF Technologies: Ford E-Series Van"]
[2014,"Westport ","EBAFT05.45HK","EBAFR0000001","Ford","E250","E6345",0,5.4,6500,null,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N",35.19,0.12050000000000001,0.0454,75.07000000000001,0.6802,0.09441999999999999,"CBAF10027684","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B6","Federal Tier 2 Bin 6","50","NOX",0.07300000000000001,0.07,"0.08",{"$nulls":7},"BAF Technologies: Ford E-Series Van"]
[2014,"Westport ","EBAFT05.45HK","EBAFR0000001","Ford","E250","E6345",0,5.4,6500,null,8000,"R","2-Wheel Drive, Rear","A","Automatic",null,4,"Y","N",null,null,"N",35.19,0.12050000000000001,0.0454,75.07000000000001,0.6802,0.09441999999999999,"CBAF10027685","MFR","3","HWFE","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B6","Federal Tier 2 Bin 6","120","NOX",0.012,0.012,"0.133",{"$nulls":7},"BAF Technologies: Ford E-Series Van"]
[2014,"Westport ","EBAFT06.254B","EBAFF0250NBS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","CO",1.26,1.9000000000000001,"4.2",0.61,{"$nulls":6},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFF0250NBS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","HC-NM",0.026000000000000002,0.056,"0.125",0.029900000000000003,null,"Y",1.5,{"$nulls":3},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFF0250NBS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","NOX",0.03,0.1,"0.2",0.04,{"$nulls":6},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFF0250NBS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","CO",1.26,1.5,"3.4",0.24,{"$nulls":6},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFF0250NBS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","HC-NM",0.026000000000000002,0.038,"0.100",0.0118,null,"Y",1.5,{"$nulls":3},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFF0250NBS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","NOX",0.028,0.04,"0.14",0.016,{"$nulls":6},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFF0265NAS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","CO",1.26,1.9000000000000001,"4.2",0.61,{"$nulls":6},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFF0265NAS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","HC-NM",0.026000000000000002,0.056,"0.125",0.029900000000000003,null,"Y",1.5,{"$nulls":3},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFF0265NAS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","NOX",0.03,0.1,"0.2",0.04,{"$nulls":6},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFF0265NAS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","CO",1.26,1.5,"3.4",0.24,{"$nulls":6},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFF0265NAS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","HC-NM",0.026000000000000002,0.038,"0.100",0.0118,null,"Y",1.5,{"$nulls":3},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFF0265NAS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","NOX",0.028,0.04,"0.14",0.016,{"$nulls":6},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFR0250NBS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","CO",1.26,1.9000000000000001,"4.2",0.61,{"$nulls":6},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFR0250NBS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","HC-NM",0.026000000000000002,0.056,"0.125",0.029900000000000003,null,"Y",1.5,{"$nulls":3},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFR0250NBS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","NOX",0.03,0.1,"0.2",0.04,{"$nulls":6},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFR0250NBS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","CO",1.26,1.5,"3.4",0.24,{"$nulls":6},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFR0250NBS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","HC-NM",0.026000000000000002,0.038,"0.100",0.0118,null,"Y",1.5,{"$nulls":3},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.254B","EBAFR0250NBS","Ford","F250","BPRINS_55337",0,6.2,10000,null,11500,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N","DF","Dual Fuel (2 separate fuel tanks, separate combustion)","N",23.118000000000002,0.4602,0.10656,71.71000000000001,1.6767,0.11037999999999999,"BBAF10022157","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","NOX",0.028,0.04,"0.14",0.016,{"$nulls":6},"BAF_Bifuel: F250/350"]
[2014,"Westport ","EBAFT06.27HL","EBAFR0000001","Ford","F250","F0989",0,6.2,10000,null,11000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",33.52,0.9612,0.03843,71.71000000000001,1.6767,0.11037999999999999,"CBAF10027686","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B6","Federal Tier 2 Bin 6","120","CO",1.95,2,"4.2",{"$nulls":7},"BAF Technologies: Ford F250/350"]
[2014,"Westport ","EBAFT06.27HL","EBAFR0000001","Ford","F250","F0989",0,6.2,10000,null,11000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",33.52,0.9612,0.03843,71.71000000000001,1.6767,0.11037999999999999,"CBAF10027686","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B6","Federal Tier 2 Bin 6","120","NMOG",0.006,0.01,"0.09",null,null,"N",{"$nulls":4},"BAF Technologies: Ford F250/350"]
[2014,"Westport ","EBAFT06.27HL","EBAFR0000001","Ford","F250","F0989",0,6.2,10000,null,11000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",33.52,0.9612,0.03843,71.71000000000001,1.6767,0.11037999999999999,"CBAF10027686","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B6","Federal Tier 2 Bin 6","120","NOX",0.06,0.1,"0.1",{"$nulls":7},"BAF Technologies: Ford F250/350"]
[2014,"Westport ","EBAFT06.27HL","EBAFR0000001","Ford","F250","F0989",0,6.2,10000,null,11000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",33.52,0.9612,0.03843,71.71000000000001,1.6767,0.11037999999999999,"CBAF10027686","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B6","Federal Tier 2 Bin 6","50","CO",1.95,2,"3.4",{"$nulls":7},"BAF Technologies: Ford F250/350"]
[2014,"Westport ","EBAFT06.27HL","EBAFR0000001","Ford","F250","F0989",0,6.2,10000,null,11000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",33.52,0.9612,0.03843,71.71000000000001,1.6767,0.11037999999999999,"CBAF10027686","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B6","Federal Tier 2 Bin 6","50","NMOG",0.006,0.006,"0.075",null,null,"N",{"$nulls":4},"BAF Technologies: Ford F250/350"]
[2014,"Westport ","EBAFT06.27HL","EBAFR0000001","Ford","F250","F0989",0,6.2,10000,null,11000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",33.52,0.9612,0.03843,71.71000000000001,1.6767,0.11037999999999999,"CBAF10027686","MFR","2","CVS 75 and later (w/o can. load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B6","Federal Tier 2 Bin 6","50","NOX",0.061000000000000006,0.06,"0.08",{"$nulls":7},"BAF Technologies: Ford F250/350"]
[2014,"Westport ","EBAFT06.27HL","EBAFR0000001","Ford","F250","F0989",0,6.2,10000,null,11000,"R","2-Wheel Drive, Rear","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",33.52,0.9612,0.03843,71.71000000000001,1.6767,0.11037999999999999,"CBAF10027687","MFR","3","HWFE","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B6","Federal Tier 2 Bin 6","120","NOX",0.01,0.01,"0.133",{"$nulls":7},"BAF Technologies: Ford F250/350"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPF0250NBS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","CO",2.3000000000000003,2.9,"4.2",0.6,{"$nulls":6},"Ford Motor Company: F250 2WD Bed Delete, F250 4WD Bed Delete, F350 2WD, F350 2WD Bed Delete, F350 4WD, F350 4WD Bed Delete"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPF0250NBS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","NMOG",0.032,0.062,".125",0.03,{"$nulls":6},"Ford Motor Company: F250 2WD Bed Delete, F250 4WD Bed Delete, F350 2WD, F350 2WD Bed Delete, F350 4WD, F350 4WD Bed Delete"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPF0250NBS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","NOX",0.085,0.12,".20",0.04,{"$nulls":6},"Ford Motor Company: F250 2WD Bed Delete, F250 4WD Bed Delete, F350 2WD, F350 2WD Bed Delete, F350 4WD, F350 4WD Bed Delete"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPF0250NBS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","CO",2.3000000000000003,2.5,"3.4",0.2,{"$nulls":6},"Ford Motor Company: F250 2WD Bed Delete, F250 4WD Bed Delete, F350 2WD, F350 2WD Bed Delete, F350 4WD, F350 4WD Bed Delete"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPF0250NBS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","NMOG",0.032,0.044000000000000004,".100",0.012,{"$nulls":6},"Ford Motor Company: F250 2WD Bed Delete, F250 4WD Bed Delete, F350 2WD, F350 2WD Bed Delete, F350 4WD, F350 4WD Bed Delete"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPF0250NBS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","NOX",0.085,0.1,".14",0.02,{"$nulls":6},"Ford Motor Company: F250 2WD Bed Delete, F250 4WD Bed Delete, F350 2WD, F350 2WD Bed Delete, F350 4WD, F350 4WD Bed Delete"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPF0265NAS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","CO",2.3000000000000003,2.9,"4.2",0.6,{"$nulls":6},"Ford Motor Company: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPF0265NAS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","NMOG",0.032,0.062,".125",0.03,{"$nulls":6},"Ford Motor Company: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPF0265NAS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","NOX",0.085,0.12,".20",0.04,{"$nulls":6},"Ford Motor Company: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPF0265NAS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","CO",2.3000000000000003,2.5,"3.4",0.2,{"$nulls":6},"Ford Motor Company: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPF0265NAS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","NMOG",0.032,0.044000000000000004,".100",0.012,{"$nulls":6},"Ford Motor Company: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPF0265NAS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","NOX",0.085,0.1,".14",0.02,{"$nulls":6},"Ford Motor Company: F350 Incomplete 2WD, F350 Incomplete 4WD"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPR0250NBS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","CO",2.3000000000000003,2.9,"4.2",0.6,{"$nulls":6},"Ford Motor Company: F250 Pickup 2WD, F250 Pickup 4WD, F350 2WD, F350 4WD"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPR0250NBS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","NMOG",0.032,0.062,".125",0.03,{"$nulls":6},"Ford Motor Company: F250 Pickup 2WD, F250 Pickup 4WD, F350 2WD, F350 4WD"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPR0250NBS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","120","NOX",0.085,0.12,".20",0.04,{"$nulls":6},"Ford Motor Company: F250 Pickup 2WD, F250 Pickup 4WD, F350 2WD, F350 4WD"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPR0250NBS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","CO",2.3000000000000003,2.5,"3.4",0.2,{"$nulls":6},"Ford Motor Company: F250 Pickup 2WD, F250 Pickup 4WD, F350 2WD, F350 4WD"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPR0250NBS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","NMOG",0.032,0.044000000000000004,".100",0.012,{"$nulls":6},"Ford Motor Company: F250 Pickup 2WD, F250 Pickup 4WD, F350 2WD, F350 4WD"]
[2014,"Westport Power Inc.","EWSPT06.2CNG","EWSPR0250NBS","Ford","F250","1FT7X2B63CEA59932",0,6.2,10500,13300,11000,"R","2-Wheel Drive, Rear","A","Automatic",null,6,"Y","N",null,null,"N",47.35,0.9478000000000001,0.10450000000000001,71.71000000000001,1.6767,0.11037999999999999,"DWSP10026339","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","MDPV","MDPV (Federal Tier 2, GVWR 8501-10000)","FA","Federal","B8","Federal Tier 2 Bin 8","50","NOX",0.085,0.1,".14",0.02,{"$nulls":6},"Ford Motor Company: F250 Pickup 2WD, F250 Pickup 4WD, F350 2WD, F350 4WD"]
[2014,"WETL","EWAXV05.9VH1","EWAXR0160P1Y","Aston Martin","Zagato","S31338",0,5.9,3704,4034,4000,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N",17.03,0.3786,0.016,39.5,0.8444,0.0119,"EWAX10028649","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","CO",0.46,0.8,"4.2",0.29,null,"N",{"$nulls":4},"Wallace Environmental Testing Laboratories, Inc.: 2013 Aston Martin Zagato"]
[2014,"WETL","EWAXV05.9VH1","EWAXR0160P1Y","Aston Martin","Zagato","S31338",0,5.9,3704,4034,4000,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N",17.03,0.3786,0.016,39.5,0.8444,0.0119,"EWAX10028649","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","NMOG",0.031,0.04,".09",0.0123,null,"N",{"$nulls":4},"Wallace Environmental Testing Laboratories, Inc.: 2013 Aston Martin Zagato"]
[2014,"WETL","EWAXV05.9VH1","EWAXR0160P1Y","Aston Martin","Zagato","S31338",0,5.9,3704,4034,4000,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N",17.03,0.3786,0.016,39.5,0.8444,0.0119,"EWAX10028649","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","NOX",0.01,0.02,"0.07",0.014,null,"N",{"$nulls":4},"Wallace Environmental Testing Laboratories, Inc.: 2013 Aston Martin Zagato"]
[2014,"WETL","EWAXV05.9VH1","EWAXR0160P1Y","Aston Martin","Zagato","S31338",0,5.9,3704,4034,4000,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N",17.03,0.3786,0.016,39.5,0.8444,0.0119,"EWAX10028649","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","CO",0.46,0.6,"3.4",0.11,null,"N",{"$nulls":4},"Wallace Environmental Testing Laboratories, Inc.: 2013 Aston Martin Zagato"]
[2014,"WETL","EWAXV05.9VH1","EWAXR0160P1Y","Aston Martin","Zagato","S31338",0,5.9,3704,4034,4000,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N",17.03,0.3786,0.016,39.5,0.8444,0.0119,"EWAX10028649","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","NMOG",0.031,0.036000000000000004,".075",0.0049,null,"N",{"$nulls":4},"Wallace Environmental Testing Laboratories, Inc.: 2013 Aston Martin Zagato"]
[2014,"WETL","EWAXV05.9VH1","EWAXR0160P1Y","Aston Martin","Zagato","S31338",0,5.9,3704,4034,4000,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N",17.03,0.3786,0.016,39.5,0.8444,0.0119,"EWAX10028649","MFR","21","Federal fuel 2-day exhaust (w/can load)","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","NOX",0.01,0.02,"0.05",0.005,null,"N",{"$nulls":4},"Wallace Environmental Testing Laboratories, Inc.: 2013 Aston Martin Zagato"]
[2014,"WETL","EWAXV05.9VH1","EWAXR0160P1Y","Aston Martin","Zagato","S31338",0,5.9,3704,4034,4000,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N",17.03,0.3786,0.016,39.5,0.8444,0.0119,"EWAX10028650","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","120","NOX",0.033,0.05,"0.07",0.014,null,"N",{"$nulls":4},"Wallace Environmental Testing Laboratories, Inc.: 2013 Aston Martin Zagato"]
[2014,"WETL","EWAXV05.9VH1","EWAXR0160P1Y","Aston Martin","Zagato","S31338",0,5.9,3704,4034,4000,"R","2-Wheel Drive, Rear","M","Manual",null,6,"N","N",null,null,"N",17.03,0.3786,0.016,39.5,0.8444,0.0119,"EWAX10028650","MFR","3","HWFE","61","Tier 2 Cert Gasoline","C","LDV","LDV/Passenger Car","FA","Federal","B5","Federal Tier 2 Bin 5","50","NOX",0.033,0.04,"0.05",0.005,null,"N",{"$nulls":4},"Wallace Environmental Testing Laboratories, Inc.: 2013 Aston Martin Zagato"]
[2014,"World CNG","EWRDJ03.6VPA","EWRDR0150RKA","Dodge","Grand Caravan","CCAR2013D",1,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"DWRD10029166","MFR","3","HWFE","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.003,0.017,"0.070",0.014,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDJ03.6VPA","EWRDR0150RKA","Dodge","Grand Caravan","CCAR2013D",1,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"DWRD10029167","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","CO",1.17,1.5,"2.1",0.29,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDJ03.6VPA","EWRDR0150RKA","Dodge","Grand Caravan","CCAR2013D",1,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"DWRD10029167","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","HC-NM",0.007,0.02,"0.04",0.0123,null,"Y",1.5,{"$nulls":3},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDJ03.6VPA","EWRDR0150RKA","Dodge","Grand Caravan","CCAR2013D",1,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"DWRD10029167","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.008,0.022000000000000002,"0.070",0.014,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT02.5EDA","EWRDR0125NBV","Ford","Transit Connect","FTCE2014D",0,2.5,3939,null,4500,"F","2-Wheel Drive, Front","SA","Semi-Automatic",null,6,"Y","N",null,null,"N",-0.169,0.4485,0.021625,27.84,0.3758,0.025249999999999998,"EWRD10029589","MFR","3","HWFE","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B5","Federal Tier 2 Bin 5","120","NOX",0.009000000000000001,0.023,"0.070",0.014,{"$nulls":6},"Ford Vehicle Division: Transit Connect Van 2wd, Transit Connect Wagon Fwd"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0116PK1","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","CO",1.17,1.5,"2.1",0.29,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0116PK1","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","HC-NM",0.007,0.019,"0.070",0.0123,null,"Y",1.5,{"$nulls":3},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0116PK1","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.008,0.02,"0.04",0.014,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0116PK1","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030123","MFR","3","HWFE","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.003,0.02,"0.04",0.014,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0150PK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","CO",1.17,1.5,"2.1",0.29,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0150PK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","HC-NM",0.007,0.019,"0.070",0.0123,null,"Y",1.5,{"$nulls":3},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0150PK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.008,0.02,"0.04",0.014,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0150PK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030123","MFR","3","HWFE","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.003,0.02,"0.04",0.014,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0150RK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","CO",1.17,1.5,"2.1",0.29,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0150RK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","HC-NM",0.007,0.019,"0.070",0.0123,null,"Y",1.5,{"$nulls":3},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0150RK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.008,0.02,"0.04",0.014,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0150RK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030123","MFR","3","HWFE","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.003,0.02,"0.04",0.014,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0153PK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","CO",1.17,1.5,"2.1",0.29,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0153PK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","HC-NM",0.007,0.019,"0.070",0.0123,null,"Y",1.5,{"$nulls":3},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0153PK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.008,0.02,"0.04",0.014,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0153PK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030123","MFR","3","HWFE","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.003,0.02,"0.04",0.014,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0170PK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","CO",1.17,1.5,"2.1",0.29,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0170PK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","HC-NM",0.007,0.019,"0.070",0.0123,null,"Y",1.5,{"$nulls":3},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0170PK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030122","MFR","21","Federal fuel 2-day exhaust (w/can load)","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.008,0.02,"0.04",0.014,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]
[2014,"World CNG","EWRDT03.6EDB","EWRDR0170PK0","Dodge","Grand Caravan","CCAR2014D",0,3.6,5000,8500,5250,"F","2-Wheel Drive, Front","A","Automatic",null,6,"Y","N",null,null,"N",-22.908,0.8397,0.020378999999999998,43.87,0.5077,0.02328,"EWRD10030123","MFR","3","HWFE","41","CNG","C","LDT2","LDT2 (LVW 3751-5750, GVW 0-6000)","FA","Federal","B4","Federal Tier 2 Bin 4","120","NOX",0.003,0.02,"0.04",0.014,{"$nulls":6},"Chrysler Vehicle Division: Chrysler, Town & Country FWD, Dodge Grand Caravan FWD"]

{"sheet":"ESRI_MAPINFO_SHEET","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true}