 New Engine EU-3                                                               

                              BPIP (Dated: 04274)
 DATE :  7/20/2022
 TIME : 14:40:49
 New Engine EU-3                                                               

 ============================
 BPIP PROCESSING INFORMATION:
 ============================

   The P  flag has been set for preparing downwash related data
          for a model run utilizing the PRIME algorithm.

   Inputs entered in METERS     will be converted to meters using 
    a conversion factor of    1.0000.  Output will be in meters.

   The UTMP variable is set to UTMY.  The input is assumed to be in
     UTM coordinates.  BPIP will move the UTM origin to the first pair of
     UTM coordinates read.  The UTM coordinates of the new origin will 
     be subtracted from all the other UTM coordinates entered to form 
     this new local coordinate system.

   The new local coordinates will be displayed in parentheses just below
     the UTM coordinates they represent.

   Plant north is set to   0.00 degrees with respect to True North.  




 ==============
 INPUT SUMMARY:
 ==============


 Number of buildings to be processed :   2


 CASINO   has 1 tier(s) with a base elevation of  -11.58 METERS    
 BUILDING  TIER  BLDG-TIER  TIER   NO. OF      CORNER   COORDINATES
   NAME   NUMBER   NUMBER  HEIGHT  CORNERS        X           Y

 CASINO      1        1      9.75    11
                                             575598.31  3730521.14 meters
                                         (        0.00        0.00) meters
                                             575544.61  3730576.25 meters
                                         (      -53.70       55.11) meters
                                             575576.99  3730605.98 meters
                                         (      -21.32       84.84) meters
                                             575567.15  3730615.39 meters
                                         (      -31.16       94.25) meters
                                             575584.86  3730633.63 meters
                                         (      -13.45      112.49) meters
                                             575633.18  3730628.64 meters
                                         (       34.87      107.50) meters
                                             575686.63  3730670.19 meters
                                         (       88.32      149.05) meters
                                             575805.28  3730557.42 meters
                                         (      206.97       36.28) meters
                                             575763.29  3730514.98 meters
                                         (      164.98       -6.16) meters
                                             575697.96  3730575.96 meters
                                         (       99.65       54.82) meters
                                             575658.63  3730577.75 meters
                                         (       60.32       56.61) meters


 PARKING  has 1 tier(s) with a base elevation of  -11.28 METERS    
 BUILDING  TIER  BLDG-TIER  TIER   NO. OF      CORNER   COORDINATES
   NAME   NUMBER   NUMBER  HEIGHT  CORNERS        X           Y

 PARKING     1        2     10.36     6
                                             575538.06  3730504.43 meters
                                         (      -60.25      -16.71) meters
                                             575455.02  3730595.48 meters
                                         (     -143.29       74.34) meters
                                             575518.66  3730668.58 meters
                                         (      -79.65      147.44) meters
                                             575573.97  3730608.17 meters
                                         (      -24.34       87.03) meters
                                             575544.03  3730575.33 meters
                                         (      -54.28       54.19) meters
                                             575577.74  3730541.49 meters
                                         (      -20.57       20.35) meters

 Number of stacks to be processed :   1

                    STACK            STACK   COORDINATES
  STACK NAME     BASE  HEIGHT          X           Y

  NE           -11.28    2.44 METERS    
                                  575638.00  3730651.00 meters
                              (       39.69      129.86) meters
  
    No stacks have been detected as being atop any structures.


                     Overall GEP Summary Table
                          (Units: meters)


 StkNo:  1  Stk Name:NE       Stk Ht:   2.44 Prelim. GEP Stk.Ht:   65.00
            GEP:  BH:   9.75  PBW:  164.39             *Eqn1 Ht:   24.38
          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2  Direction occurred:  269.25
   Bldg-Tier nos. contributing to GEP:   2   1




                     Summary By Direction Table
                          (Units:  meters)

 Dominate stand alone tiers:


 Drtcn:  10.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 259.98  PBL: 162.12  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -134.78  YADJ:  -51.00

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn:  20.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 251.39  PBL: 170.27  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -135.60  YADJ:  -63.50

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn:  30.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 235.21  PBL: 173.24  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -132.31  YADJ:  -74.05

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn:  40.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 219.68  PBL: 170.95  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -124.99  YADJ:  -78.46

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn:  50.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 205.58  PBL: 187.58  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -119.59  YADJ:  -81.94

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn:  60.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 191.97  PBL: 216.33  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -118.25  YADJ:  -84.46

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn:  70.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 172.52  PBL: 238.51  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -113.32  YADJ:  -84.41

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn:  80.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 166.16  PBL: 253.44  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -104.95  YADJ:  -72.63

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn:  90.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 155.21  PBL: 260.67  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -93.39  YADJ:  -58.41

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 100.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 162.12  PBL: 259.98  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -78.99  YADJ:  -53.72

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 110.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 170.27  PBL: 251.39  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -62.19  YADJ:  -50.47

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 120.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 173.24  PBL: 235.21  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -43.55  YADJ:  -45.69

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 130.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 170.95  PBL: 219.68  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -31.38  YADJ:  -39.52

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 140.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 187.58  PBL: 205.58  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -20.85  YADJ:  -25.80

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 150.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 216.33  PBL: 191.97  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -11.53  YADJ:  -10.09

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 160.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 238.51  PBL: 172.52  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:   -1.85  YADJ:    5.93

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 170.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 253.44  PBL: 166.16  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -10.45  YADJ:   21.77

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 180.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 260.67  PBL: 155.21  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -19.19  YADJ:   36.95

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 190.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 259.98  PBL: 162.12  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -27.34  YADJ:   51.00

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 200.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 251.39  PBL: 170.27  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -34.67  YADJ:   63.50

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 210.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 235.21  PBL: 173.24  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -40.93  YADJ:   74.05

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 220.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 219.68  PBL: 170.95  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -45.96  YADJ:   78.46

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 230.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 205.58  PBL: 187.58  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -67.99  YADJ:   81.94

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 240.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 191.97  PBL: 216.33  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ:  -98.08  YADJ:   84.46

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 250.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 172.52  PBL: 238.51  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -125.19  YADJ:   84.41

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 260.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 166.16  PBL: 253.44  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -148.49  YADJ:   72.63

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 270.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 155.21  PBL: 260.67  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -167.28  YADJ:   58.41

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 280.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 162.12  PBL: 259.98  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -180.99  YADJ:   53.72

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 290.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 170.27  PBL: 251.39  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -189.20  YADJ:   50.47

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 300.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 173.24  PBL: 235.21  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -191.66  YADJ:   45.69

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 310.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 170.95  PBL: 219.68  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -188.30  YADJ:   39.52

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 320.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 187.58  PBL: 205.58  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -184.73  YADJ:   25.80

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 330.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 216.33  PBL: 191.97  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -180.44  YADJ:   10.09

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 340.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 238.51  PBL: 172.52  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -170.67  YADJ:   -5.93

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 350.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 253.44  PBL: 166.16  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -155.71  YADJ:  -21.77

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1

 Drtcn: 360.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
     Single tier MAX:  BH:   9.75  PBW: 260.67  PBL: 155.21  *Wake Effect Ht:   24.08
     Relative Coordinates of Projected Width Mid-point: XADJ: -136.02  YADJ:  -36.95

          *adjusted for a Stack-Building elevation difference of    0.30
                BldNo:  1  Bld Name:CASINO    TierNo:  1


 Dominant combined buildings:

 Drtcn:  10.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 351.55  PBL: 189.04  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -161.70  YADJ:   -5.21

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn:  20.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 342.15  PBL: 206.58  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -171.91  YADJ:  -18.12

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn:  30.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 322.36  PBL: 217.84  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -176.90  YADJ:  -30.48

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn:  40.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 292.78  PBL: 222.48  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -176.52  YADJ:  -41.91

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn:  50.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 274.91  PBL: 243.85  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -175.86  YADJ:  -47.28

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn:  60.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 255.34  PBL: 284.30  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -186.23  YADJ:  -52.77

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn:  70.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 228.01  PBL: 316.12  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -190.93  YADJ:  -56.67

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn:  80.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 193.75  PBL: 338.33  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -189.84  YADJ:  -58.84

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn:  90.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 165.76  PBL: 350.26  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -182.98  YADJ:  -63.69

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 100.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 189.04  PBL: 351.55  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -170.56  YADJ:  -67.18

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 110.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 206.58  PBL: 342.15  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -152.96  YADJ:  -68.62

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 120.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 217.84  PBL: 322.36  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -130.71  YADJ:  -67.98

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 130.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 222.48  PBL: 292.78  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -104.48  YADJ:  -65.28

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 140.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 243.85  PBL: 274.91  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ:  -90.18  YADJ:  -53.93

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 150.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 284.30  PBL: 255.34  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ:  -74.89  YADJ:  -44.07

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 160.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 316.12  PBL: 228.01  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ:  -57.34  YADJ:  -32.87

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 170.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 338.33  PBL: 193.75  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ:  -38.04  YADJ:  -20.68

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 180.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 350.26  PBL: 165.76  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ:  -19.19  YADJ:   -7.85

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 190.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 351.55  PBL: 189.04  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ:  -27.34  YADJ:    5.21

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 200.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 342.15  PBL: 206.58  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ:  -34.67  YADJ:   18.12

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 210.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 322.36  PBL: 217.84  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ:  -40.93  YADJ:   30.48

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 220.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 292.78  PBL: 222.48  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ:  -45.96  YADJ:   41.91

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 230.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 274.91  PBL: 243.85  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ:  -67.99  YADJ:   47.28

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 240.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 255.34  PBL: 284.30  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ:  -98.08  YADJ:   52.77

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 250.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 228.01  PBL: 316.12  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -125.19  YADJ:   56.67

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 260.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 193.75  PBL: 338.33  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -148.49  YADJ:   58.84

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 270.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 165.76  PBL: 350.26  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -167.28  YADJ:   63.69

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 280.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 189.04  PBL: 351.55  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -180.99  YADJ:   67.18

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 290.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 206.58  PBL: 342.15  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -189.20  YADJ:   68.62

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 300.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 217.84  PBL: 322.36  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -191.66  YADJ:   67.98

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 310.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 222.48  PBL: 292.78  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -188.30  YADJ:   65.28

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 320.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 243.85  PBL: 274.91  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -184.73  YADJ:   53.93

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 330.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 284.30  PBL: 255.34  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -180.44  YADJ:   44.07

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 340.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 316.12  PBL: 228.01  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -170.67  YADJ:   32.87

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 350.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 338.33  PBL: 193.75  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -155.71  YADJ:   20.68

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1

 Drtcn: 360.00

 StkNo:  1  Stk Name:NE                                Stack Ht:    2.44
                 GEP:  BH:   9.75  PBW: 164.39   *Equation 1 Ht:   24.38
   Combined tier MAX:  BH:   9.75  PBW: 350.26  PBL: 165.76  *WE Ht:   24.38
     Relative Coordinates of Projected Width Mid-point: XADJ: -146.57  YADJ:    7.85

          *adjusted for a Stack-Building elevation difference of    0.00
  No. of Tiers affecting Stk:  2
   Bldg-Tier nos. contributing to MAX:   2   1
